       Printer definition file for WSSINDEX custom print utility

All lines of this file are comments until a line beginning ----.  After that,
alternate lines are comments and parameters.  See the CUSTPRNT documentation
for a description of the format allowed here.  Commands in file are for an
HP Laser Jet or Laser Jet Plus.  This printer lacks the box forming characters
found in the LJ II, so disk cover boxes are made by overprinting | and - with
offset positions.  Other than this, the commands are the same as for an LJ II.
Commands used in this file:

  27 69 = \e E = reset
  27 38 108 1 69 = \e & l 1 E = 1 line top margin
  27 38 108 84 70 = \e & l 84 F = 84 lines per page
  27 38 107 50 83 = \e & k \2 S = 16.66 pitch
  27 38 108 56 68 = \e & l \8 D = 8 lines per inch
  27 12 = \e 12 = form feed (?)
------------------------------------------------------------
Printer name
HP Laser Jet (or LJ+)
Optional string printed on all labels
Property of <your name here>
Printer initialization command for 1,2,... column printing, 50 max
27 69 27 38 108 1 69 27 38 108 84 70
Printer initialization command for labels, 50 max (pitch, line spacing, etc.)
27 38 107 50 83 27 38 108 56 68
Printer initialization command for disk covers, 50 max
27 38 107 50 83 27 38 108 56 68
Printer deinitialization command, 10 max (form feed for laser printer, etc.)
27 12
Number of spaces in left margin for labels
5
Number of columns for labels
2
Width of labels (characters)
50
Number of characters between labels (if multiple columns)
3
Length of label in lines (including unusable lines)
12
Number of usable lines for label
9
Number of spaces in left margin for disk covers
9
Width of paper for disk covers (characters)
90
Length of page in lines for disk covers
40
Printer command to position for the next disk cover

Character to use for sides of disk cover box (32 = blank prints faster)
\e & a - \5 \0 V | \b \e & a + \8 \4 V | \e & a - \3 \4 V
Character to use for top and bottom lines
\e & a - \2 \8 H - \b \e & a + \5 \2 H - \e & a - \2 \4 H
Character to use for top left corner
\e & a + \2 \4 H - \b \e & a - \2 \4 H \e & a + \3 \4 V | \e & a - \3 \4 V
Character to use for top right corner
\e & a - \2 \8 H - \b \e & a + \2 \8 H \e & a + \3 \4 V | \e & a - \3 \4 V
Character to use for bottom left corner
\e & a - \5 \0 V | \b \e & a + \5 \0 V \e & a + \2 \4 H - \e & a - \2 \4 H
Character to use for bottom right corner
\e & a - \2 \8 H - \b \e & a + \2 \8 H \e & a - \5 \0 V | \e & a + \5 \0 V
End of printer configuration file
