
(* SAC Basic I/O System definition module. *)

DEFINITION MODULE SACBIOS;


FROM MASELEM IMPORT GAMMAINT;


PROCEDURE CWRIT2(C1,C2: GAMMAINT);
(*Character write, 2 characters.  C1 and C2 are sequentially
transmitted to the output stream using CWRITE.*)


PROCEDURE CWRIT3(C1,C2,C3: GAMMAINT);
(*Character write, 3 characters.  C1, C2 and C3 are sequentially
transmitted to the output stream using CWRITE.*)


PROCEDURE CWRIT4(C1,C2,C3,C4: GAMMAINT);
(*Character write, 4 characters.  C1, C2, C3, and C4 are sequentially
transmitted to the output stream using CWRITE.*)


PROCEDURE CWRIT5(C1,C2,C3,C4,C5: GAMMAINT);
(*Character write, 5 characters.  C1, C2, C3, C4 and C5 are
sequentially transmitted to the output stream using CWRITE.*)


PROCEDURE CWRIT6(C1,C2,C3,C4,C5,C6: GAMMAINT);
(*Character write, 6 characters.  C1, C2, C3, C4, C5 and C6 are
sequentially transmitted to the output stream using CWRITE.*)


END SACBIOS.


