SBD32.EXE is a 32 Bit demo of 'Speaker Box Design v2.1'.
This EXE file contains the installation program, an uninstall
program, and all the files needed to run the program. The default
directory for the installation is 'C:\SPEAKER' but you
may change this to any directory you wish. To install the program,
select 'START', 'RUN', and type d:\sub\SBD32.EXE'. Where 'd:'
is the drive letter the program is on and 'sub' is the sub-directory
the program is in. The program helps in the design of Closed,
Vented, Passive, and Bandpass enclosures. It also designs
passive and active crossover systems, impedance matching and
notch filter networks, and helps in the design of the coils if
you wish to make your own.
The program has graphics, printing, and load/save capabilities.
With this version you need a VGA monitor, 8 Megs of RAM (16 recomended),
and Win95 or Windows NT. If you wish a 16 Bit version please use
'SBD16.EXE'.
If you have any trouble installing the software or have any questions,
I can be reached at:
E-mail - bodtrons@nauticom.net
Mail -  Al Bodnar
        650 N. Pike Rd.
        Cabot, Pa. 16023

