                 GraphicsENGINE ULTRA Windows 3.1 driver

Installation:
1) Insert the GraphicsENGINE ULTRA Driver diskette into drive A.

2) Run the installation file INSTALL.EXE on drive A.
       Example:  C:\>a:\install

   Then select INSTALL's Microsoft Windows 3.1 menu,
   press ENTER key and complete the installation.
   INSTALL will copy the appropriate files to your default directory.

3) Run Setup program when prompted, selecting  option to change the
   DISPLAY device and following the  instructions to complete the
   driver installation.

Hardware Requirements:
 * IBM-PC compatible or better CPU.
 * GraphicsENGINE ULTRA board.

Resolution:
 Currently the following modes are supported:
 *  640 x 480, 256 colors
 *  640 x 480, 64K colors
 *  640 x 480, 16.7M colors
 *  800 x 600, 16 or 256 colors
 *  800 x 600, 64K colors
 *  800 x 600, 16.7M colors
 * 1024 x 768, 16 or 256 colors
 * 1024 x 768, 64K colors
 * 1280 x 1024, 16 or 256 colors

NOTE:
If you have already installed a previous version of the driver, copy
the file ERASEOLD.BAT into the \windows directory and execute it.
Follow this by typing SETUP and reinstall the driver.

Not all modes are supported by all monitors. Attempting to use modes
which yourmonitor does not support will produce unsatisfactory results.

The GraphicsENGINE ULTRA board is capable of generating more 
frequencies and supporting more modes than most VGA cards.
To switch to a different mode, you can either use SW1.EXE (Software
Switch utility on utility floppy) or SW1. (Hardware Switch on board)

Driver Limitations:
1. No pen support at this time.
2. No SWC resolutions at this time.
3. 1280x1024 Non-Interlaced mode may display color and fading problems.
4. VDD limitation of DOSShell colors will change after Alt-Tab to
   Windows and back. This only occures in 4-planes.

