Readme.txt
1/98
***********************************************************************
Correct Bearing Capacity Trial Version 
Copyright  1998 TAP Software. All rights reserved
***********************************************************************
PURPOSE

This program facilitates calculating the bearing capacity of spread footings on sand or clay.

SET UP

Shut down all programs that may be running in the background.
Failure to do so may result in an unsuccessful installation.
During the initialization, certain Windows system files are updated.

From the “Run” option under File, Type X:\setup where X is the location of the file.  The program will initialize the files required and set up the application in a default directory.  Be sure to make a backup copy of the installation program.

Program requires Windows 95.

Disk space required 4.0 Mb for installation. 

VGA color monitor (min) 


PROGRAM STATUS AND DISTRIBUTION

This is a fully operational trial version of Correct Bearing Capacity V4.0.2

For Registeration information visit our website at www.tapsoftware.com

You can make one backup copy of this program for safe keeping
and install the program on one computer.  You may not make copies of the
program for distribution or alter any of these files in any way.


QUESTIONS

Send questions, comments to info@tapsoftware.com

There is email capability directly from the program.









