Layout  cdio   Date: Sep 03, 1998    14:00:00

Gerber files

Filename    Polarity    Layer name
------------------------------------------------
gerber.1        P       Silkscreen top (Componentside)
gerber.2        P       Paste-mask top (Componentside)
gerber.3        P       Solder mask top (Componentside)
gerber.4        P       Top layer (Componentside)
gerber.5        P       Bottom layer (solderside)
gerber.6        P       Solder mask bottom (solderside)

gerber.txt              Aperture file (Wheel table)


Drill files
------------------------------------------------
cdio.drl                Drill file
drill.txt               Drill tool file

Gerber output specification :
-----------------------------

Number format : 2 4
Suppression   : Leading zero
Coordinates   : Absolute

PCB information :
-----------------

cdio.neu           Neutral_file (PCB testing)

PCB SPECIFICATIONS :
--------------------

PCB size (Width,height)   :   6200.0000 ,  3200.0000  mils
PCB size (Width,height)   :      6.20000,     3.20000 inch
PCB size (Width,height)   :    157.480  ,    81.280   mm

PCB origin (x,y)          :   1000.0000 ,  1000.0000  mils
PCB origin (x,y)          :      1.00000,     1.00000 inch
PCB origin (x,y)          :     25.400  ,    25.400   mm


Board thickness           : 1.6 mm
Material                  : FR4
Basic copper thickness    : 17.5 u
Number of layers          : 2
Minimal Trace width       : 8 mil (0.20 mm)
Minimal Clearance         : 8 mil (0.20 mm)
