ComPhone

Thanks for choosing ComPhone. 
Using ComPhone is very easy. 
Simply enter the telephone number and hit send!
Now it does have some more advanced features such as...
* ComPhone now supports US Robotics Sportster 56k Voice modems!
* Caller ID
* Last Number Re-Dial
* Repeat Dial
* Auto Answer
* Hold
* 60 Entry Phone Book
* Mute and more!

ComPhone will work with most voice modems that have the Rockwell Chipset. 
The default initialization string for most these modems is 'AT#CLS8#VLS=6', 
to enable Caller ID the string is '#CID=1'. 
If these strings produce errors then consult your modem guide or dealer.
Be sure to go to the setup screen and select the correct Comm Port.
If the correct port is not selected the power light will not come on.

To use the built in phone book, press the button marked 'PB'. 
To add an entry select the position you want and press the edit button. 
Fill in the information and press done. To add a person from the Caller ID 
display select the position and press 'Add Caller'.

If you hold the mouse over the buttons you can see a brief description of what they do. 
If you need to contact us email rcrews@netwalk.com.

For ordering information, find us on the Internet @
HTTP://www.crews-net.com

Be shure that you have all necessary files!
They are:

ASYCFILT.DLL
COMCAT.DLL
CTL3D32.DLL
MSVBVM50.DLL
OLEAUT32.DLL
OLEPRO32.DLL
STDOLE2.TLB
These files you can download from the WEB e.g. as:
ftp://www.simtel.net/simtelnet/win95/dll/vb500a.zip

Note:
Some of the funtions described above are not avialable in the shareware version.