These drivers will install only from floppy. Please have 2 formatted, high-
density, 3.5" floppy disks ready before the isntall.

Here are the instructions to unpack the drivers to floppies:

INSTALL <drive letter of your 3.5" drive>

For example, if your 3.5" floppy drive is drive B, the command would read:

INSTALL B:

