-------------------------------------------------------------------------
ZETAFAX for Windows NT
-------------------------------------------------------------------------

Zetafax can be used with a mixture of Windows and Windows NT machines
as required.  The standard version can be used under Windows NT for
both the fax server and client software.  The fax server programs run
in the background, and may therefore be run on a Windows NT fileserver
if you wish.

A single user version of Zetafax is available for Windows NT users.

To install on Windows NT:

1.  Ensure that you have full Administrator rights, then run the
    Zetafax Installation program (INSTALL.EXE) from the disks supplied
    and follow the instructions.

    The workstation installation program will make some changes to 
    the WIN.INI file [devices], [ports], [PrinterPorts] and [extensions] 
    sections.  Under Windows NT these are mapped into sections of the 
    Registry database.

    By default Administrators are allowed to make these changes.
    However if this has been changed on your computer you will get
    an error message when installing.  If you do not wish to use the
    Windows NT machine as a workstation you can ignore this message;
    otherwise you should log in as a user with additional rights
    (or correct the permissions using REGEDIT32), and rerun the 
    installation.

    Restart Windows NT (just logging off is not sufficient), then
    create a printer as described below.

2.  To configure a Zetafax workstation under Windows NT, log in as a
    user with full Administrator rights and then run the Workstation
    Setup program (zfax\SYSTEM\WKSETUP.EXE).  This is done on the fax
    server PC automatically during installation.  See above if an
    error is displayed when trying to update the device settings.

    Restart Windows NT (just logging off is not sufficient).

    Now use print manager to add a new printer with name set to
    "Zetafax printer", driver "Epson LQ-1000", and printing to 
    "C:\WINNT\ZETAFAX.SPL" (in your Windows NT directory).  This will
    be in the list of available ports - ignore the entry for
    "ZETAFAX.SPL" without a path.

3.  Finally, to send a fax you just run the Zetafax workstation,
    then print to the Zetafax printer.	Provided the workstation is
    running and its title bar does not say "offline", the addressing 
    dialog box will be displayed after a few moments.  (If the 
    workstation is offline you should check the Zetafax server is 
    running.)


Currently Zetafax comprises a set of 16 bit programs, and the best
performance on the fax server is therefore obtained by running it under
Windows or OS/2 (the latter is available as an optional upgrade).

A 32 bit Windows NT version is due for release shortly - please contact
Equisys for details.

EQUISYS Limited
Phone: 0171-403 2227 (Intl +44 71 403 2227)
Fax: 0171-378 6886 (Intl +44 71 378 6886)