                        CorelDRAW 4.0 Maintenance Upgrade

Your CorelDRAW 4.0 maintenance upgrade consists of one of the following formats:
     - seven 3.5" diskettes OR eight 5.25" diskettes OR one CD-ROM disk.

Please note that the maintenance upgrade floppy diskettes do NOT contain a full
version of the software. They are only intended to make corrections to your
existing CorelDRAW 4.0 Installation. You must keep your EXISTING installation
and the ORIGINAL program floppy diskettes.

Upgrade Installation Procedure
==============================

(1)  You must install the upgrade from Windows.
(2)  Insert upgrade disk 1 (marked "Rev B Patch Disk 1/7") into drive A
(3)  Choose the Run command from the File Menu.
(4)  Type "A:\Update" in the Command Line field and press ENTER.  The upgrade
     procedure will start.
(5)  NOTE FOR USERS INSTALLING FROM FLOPPY DISKETTE: If you wish to add modules
     not previously installed (eg. CorelCHART, CorelMOVE, etc.), you must use
     the ORIGINAL diskettes to install the module(s), then run the update again.
(6)  IF YOU INSTALL FROM THE CD-ROM TO YOUR HARD DISK: Complete the upgrade
     installation procedure detailed above.  Note that the CD-ROM disk supplied
     contains updated versions of the same files as CD #1 of your original
     purchase, in addition to the update setup routine (UPDATE.EXE).  You MUST
     use this updated CD-ROM for all future re-installs.
(7)  IF YOU'RE RUNNING CorelDRAW 4.0 DIRECTLY FROM THE CD-ROM: You must run
     SETUP2.EXE from the upgrade CD.  BEFORE DOING SO, you should make backup
     copies of any of the files listed below in Notes (b) that you've
     customized.  These are in the CUSTOM directory and are NOT automatically
     backed up when installing to run directly from the CD-ROM.  Once SETUP2
     procedure has been completed, the previously-customized files can be copied
     back into the CUSTOM directory, overwriting the newer ones that were just
     installed.  Finally, you MUST also use the upgrade CD to run the programs,
     instead of the original CD.
(8)  NOTES FOR NETWORK ADMINISTRATORS AND USERS INSTALLING FROM NETWORKS:
     Network administrators must first run UPDATE /A from the upgrade disk. 
     Once this is complete, network users can then run SETUP from the network's
     SETUP directory to update their local configuration.  BEFORE DOING SO,
     network users should make backup copies of any of the files listed below
     in Notes (b) that they've customized.  These are found in the user's CUSTOM
     subdirectory and are NOT automatically backed up when installing from the
     network.  Once the local setup procedure has been completed, the
     previously-customized files can be copied back into the CUSTOM directory,
     overwriting the newer ones that were just installed.

Notes
=====

The upgrade installation procedure will create a log file called UPDATE.LOG in
your windows directory.  This file is useful if you run into problems with the
installation and need to contact us for technical assistance.

The installation procedure will also create backups of certain files:
     (a)  Any .INI files the upgrade procedure changes. The old ones will be
          stored in the configuration directory (eg. C:\COREL40\CONFIG) and will
          have a .BAK extension.
     (b)  Any user-customizable files found in the "\COREL40\CUSTOM" directory
          that you have altered. The backups will be renamed as follows:
               COREL1.CMY     is renamed to: COR1_CMY.BAK
               COREL1.RGB     is renamed to: COR1_RGB.BAK
               COREL1.SMT     is renamed to: COR1_SMT.BAK
               COREL2.CMY     is renamed to: COR2_CMY.BAK
               COREL2.RGB     is renamed to: COR2_RGB.BAK
               COREL2.SMT     is renamed to: COR2_SMT.BAK
               DEFAULT.CMY    is renamed to: DEF_CMY.BAK
               DEFAULT.RGB    is renamed to: DEF_RGB.BAK
               DEFAULT.SMT    is renamed to: DEF_SMT.BAK



                                                                 SW\PATCH-B-LETTER