Sauber-Ford C 14 Technical Specification
-----------------------------------------------------------

Chassis:               Carbonfibre monocoque
Engine:                Ford Zetec-R V8

Front suspension:      Upper and lower wishbones, combined
                       spring/damper units mounted inboard
                       with pushrod actuation.

Rear suspension:       Upper and lower wishbones, combined
                       spring/damper units mounted inboard
                       with pushrod actuation.

Brakes:                Four-piston calipers from and rear
                       (Brembo); carbon discs (Carbon
                       Industrie/Hitco)

Transmission:          Semi-automatic, longitudinally
                       mounted, six-speed transmission
                       (Sauber)

Dimensions:
===========
   
   Length:             434 cm (170.8 in)
   Front track:        171 cm (67.3 in)
   Rear track:         161 cm (63.4 in)
   Fuel tank:          140 Hues (30.8 gals)

-----------------------------------------------------------
Source: PP Sauber AG
Scan & ocr by Tero Virta
-----------------------------------------------------------