Technical Specification of Tyrrell Yamaha 023
-----------------------------------------------------------

Chassis
----------------------------------------------------------- 
Construction:          Moulded carbon fibre and honeycomb
                       composite structure to fully meet
                       the FIA 1995 strength and impact
                       regulations. 

Front Suspension:      Tyrrell Hydrolink Suspension System,
                       developed with the assistance of
                       Fondmetal Technologies. 

Rear Suspension:       Separate spring and damper units
                       operated by push rods and rockers,
                       mechanical anti-roll bar. 

Dampers:               Koni 

Wheels:                Fondmetal cast magnesium
                       Front 4-spoke, 11.0 in wide
                       Rear 5-spoke, 13.7 in wide

Tyres:                 Goodyear 
Brakes:                AP Racing
                       Front 2 x 6 piston calipers
                       Rear 2 x 4 piston calipers

Brake Discs & Pads:    Hitco carbon
Pipe Systems:          Titeflex 
Steering:              Tyrrell rack and pinion 
Steering Wheel:        Personal 
Driverīs Seat:         Anatomically formed carbon composite 

Seat Belts:            Willans 6-point harness
                       (75 mm wide shoulder straps) 

Extinguisher:          Tyrrell carbon fibre moulded tank to
                       FIA 1995 specification, pressure
                       filled with Spraylance AFFF
                       extinguishant. 

Fuel Tank:             ATL Kevlar bladder to FIA FT5
                       specification 
Battery:               Tyrrell 12v 5Ah lead acid 
Instrumentation:       PI Research System V, integrated
                       digital data display and telemetry. 


Engine
----------------------------------------------------------- 
Type:                  Yamaha OX10C V-10 3-litre 
Injection/Ignition:    Zytek 
Spark Plugs:           NGK 


Transmission
----------------------------------------------------------- 
Gearbox:               Tyrrell transverse three-shaft
                       6-speed unit 
Gear selection:        Pneumatic, sequential 
Drive Shafts:          Tyrrell 
Clutch:                AP Racing carbon plate 
Differential:          Tyrrell / X-Trax viscous coupling 


Dimensions
----------------------------------------------------------- 
Overall length:        4380 mm 
Wheelbase:             2890 mm 
Front track:           1700 mm 
Rear track:            1610 mm 
Overall width:         2000 mm 
Height:                950 mm 


-----------------------------------------------------------
Source: http://www.nokia.com/
