Technical characteristics of the Jordan Peugeot 195
===========================================================


Chassis:              Single shell entirely made of
                      composite carbon fibres.

Front suspension:     Power connecting rods in composite
                      fibres, working two Jordan GP shock
                      absorbers, drawn in unequal-length
                      triangles with the upper triangle in
                      composite material and the lower
                      triangle in steel; the arms are built
                      in steel, as is the front roll-bar. 

Rear suspension:      Power connecting rods in composite
                      material working two double Jordan GP
                      shock absorbers mounted on the
                      transmission-box with unequal-length
                      triangles, with arms and rear
                      anti-roll bar in steel. 

Transmission column:  In-house design Seven speed (plus
                      reverse) longitudinal gearbox
                      Electronically-piloted sequential
                      control for gear changes. 

Clutch:               Double-disc Tilton Racing system.
Brakes:               Brembo braking systems, front and rear
                      metallic matrix four-piston toe-links,
                      discs and brake pads in SEP carbon. 

Wheel rims:           OZ Racing forged according to
                      Jordan's specifications

Motor:                Peugeot V10 A10E 3 liter engine.
Tires:                Goodyear
Fuel tank capacity:   124 liters

Wheelbase:            2950 mm
Front width:          1700 mm
Rear width:           1618 mm

Overall height:       950 mm
Overall length:       4450 mm
Total weight:         595 kg including the driver
                   



===========================================================
Source: http://www.peugeot.com
-----------------------------------------------------------