      PROBLEM. Easy Base fails to start with the message "Insufficient
               memory to load overlays"

      If EMS is present EB will attempt to load its overlays in it. EB
      requires just under 2Meg of EMS. If there is no EMS then EB will
      swap its overlays from disk. If EMS is present but there is not
      enough then EB may fail with the above error message. 

      If you get the above message you can either:-

      1.   Free up more EMS if you physically have it but it has been
           assigned to another device.

      2.   Rem out your EMS driver in your Config.SYS if you do not
           have enough physical EMS.


      PROBLEM. Easy Base starts but will not change Data Directories.

      To change data directories Easy Base requires an MS DOS or 
      compatible Command processor as Shell.  Changing directories
      may not be possible if you are running a DOS extender such as
      4DOS and have customized the DIR Command.