
An OS/2* graphics accelerator driver supporting the 86C801, 86C805,
and 86C928 chip set(s) from S3** Incorporated. The file is a 1.44 mb
disk image.  Use LOADDSKF to recreate the disk.

    For example:  LOADDSKF C:\S3_16MD1.DSK A:

     S3_16MIN.DSK          Driver disk (Install)
     S3_16MD1.DSK          Driver disk (Disk 1)
     README.16M            Readme text file

This graphics accelerator driver is compatible with OS/2 2.11, and 3.0.

