<  Installation instructions for Warp FixPak XR_W016
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
  
 
  
  
 
 
 
  Build level 8.240
  
  
  Supported CSD levels
  
  XR_3000 Warp for Windows
  XR_3001 Warp with WIN-OS2
  XR_3002 Warp for Windows Manufacturing Refresh
  XR_3003 Warp with WIN-OS2 Connect
  XR_3004 Warp for Windows Manufacturing Refresh Connect
  XR_3005 Warp With WIN-OS2 Server
  
  
  OS/2 Fix Distribution
  Personal System Products
  Boca Raton, Fl
  
  
  (c) Copyright International Business Machines Corporation, 1995.
  All rights Reserved.
 
  December 15, 1995 Warp FixPak XR_W016
 

 
                  December 15, 1995 Warp FixPak XR_W016
 
  CONTENTS
 
    Terms and Conditions ............................................. 1
 
    Installation Notes ............................................... 2
    Corrective Service Facility boot diskettes ....................... 2
    Read Only files .................................................. 3
 
    Relocated OS/2 file support ...................................... 4
 
    Installation Process ............................................. 5
    Method 1: Install from booted OS/2 partition.  ................... 5
    Method 2: Boot from Corrective Service Disk 1.  .................. 7
    Additional Corrective Service Facility information ............... 7
 
    Recovering from Installation problems ............................ 8
      No files to service ............................................ 8
      Previous installation interrupted .............................. 9
      Unable to open Archive directory ............................... 9
 
    System problems after Fixpak installation ....................... 10
      Updating systems with the CMD chipset ......................... 10
      RZ1000 and CMD640 Data Problems (APAR=PJ19409) ................ 10
      SYS3175 when opening LS 4.0 Lan Server Administration ......... 12
      Traps when cancelling print jobs after FixPak is installed .... 13
      Novell Requester .............................................. 13
      System date changing erratically (APAR= PJ21043) .............. 13
 
    CSD level of SYSLEVEL.OS2 ....................................... 14
 
    Where Fixes can be found ........................................ 15
 
    FixPak Corrective Service levels and disk layouts ............... 16
 
    Space Utilization ............................................... 25
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
  
                                                            Contents  ii

 
                  December 15, 1995 Warp FixPak XR_W016
 
  TERMS AND CONDITIONS
 
                          IMPORTANT
                          ---------
  IMPORTANT - PLEASE READ THE FOLLOWING TERMS AND CONDITIONS.
  DOWNLOADING THE FIXPAK XR_W016 SERVICE FIXES THAT FOLLOW
  INDICATES YOUR ACCEPTANCE OF THE FOLLOWING TERMS AND CONDITIONS:
 
 
   A)  YOU MUST BE, AND AGREE THAT YOU ARE, A CURRENT LICENSEE OF
        OS/2;
 
   B)  YOU MAY MAKE COPIES OF THE OS/2 SERVICE FIXES EQUAL TO THE
        NUMBER OF LICENSED COPIES OF OS/2 YOU POSSESS;
 
   C)  YOU MAY ONLY USE THE SERVICE FIXES INCLUDED WITH FIXPAK XR_W016
        FOR MAINTENANCE PURPOSES;
 
   D)  YOU MAY ONLY USE THE WIN-OS/2 SERVICE FIXES INCLUDED WITH FIXPAK
        XR_W016 TO MAINTAIN COPIES OF OS/2 WITH WIN-OS/2;
 
   E)  ALL OTHER TERMS AND CONDITIONS OF YOUR OS/2 LICENSE
       AGREEMENTS APPLY TO THE SERVICE FIXES; HOWEVER, THIS DOES NOT
       EXTEND ANY WARRANTY AND/OR SERVICES, INCLUDING BUT NOT LIMITED
       TO THE "GETTING STARTED" PERIOD, OUTLINED IN SUCH AGREEMENTS.
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
  
                                                                 Page  1

 
                  December 15, 1995 Warp FixPak XR_W016
 
  INSTALLATION NOTES
 
  Warning: OS/2 FixPak will not install on Aptiva M series models
  preloaded with OS/2 Warp. FixPaks will install on these machines if
  OS/2 has been reinstalled from any shrink wrap version of OS/2 Warp.
  Contact OS/2 Technical Support if you need assistance in this process.
 
  Note: When editing fonts, users of Dell machines may discover a slight
  regression.  When editing a font size, the font palette is updated
  correctly; however, should the user browse (select around) the
  palette, he may, at times, notice an inconsistancy between the font
  size displayed on the palette and the one which is displayed on the
  font editor.  In all cases, the font size displayed on the font
  palette is the correct size for the font when dragged to the target
  (desktop, folder, application, etc.)
 
  The following instructions describe how to install this FixPak on your
  system.
 
 
  CORRECTIVE SERVICE FACILITY BOOT DISKETTES
 
  You will need the OS/2 Warp 3.0 Corrective Service Facility boot disks
  to install this FixPak. These files should be available from the same
  place you got this FixPak.
 
     CSFBOOT.1DK - Corrective Service Facility disk 1
     CSFBOOT.2DK - Corrective Service Facility disk 2
 
        - or -
 
     WKICKR.ZIP   - File compressed with PKZIP. Contains both of the
                    above disk images. Requires PKUNZIP or UNZIP to
                    extract original files from compressed file.
 
 
  To create diskettes from the disk image files you need LOADDSKF.EXE.
  This is also available from the same place you got this FixPak.
 
     LDF.COM      - Self extracting file that will create LOADDSKF.EXE.
                    Place in a separate directory on your harddisk then
                    enter LDF.
 
        - or -
 
     LOADDF.ZIP   - File compressed with PKZIP, contains LOADDSKF.EXE.
                    Requires PKUNZIP or UNZIP to extract original files
                    from compressed file.
 
  Note: LOADDSKF.EXE is also on any CD-ROM version of OS/2.
 
 
  
                                                   Installation Notes  2

 
                  December 15, 1995 Warp FixPak XR_W016
 
  Use LOADDSKF.EXE to create the diskettes. For each disk image place a
  2MB HD (1.44MB formatted) diskette in A:. Please DO NOT use a 1MB
  (720KB formatted) diskette as you may have problems trying to install
  this FixPak.
 
  1.  Enter LOADDSKF CSFBOOT.1DK A: /F. Label as CSF DISK Diskette 1 (SP
      DISK 1)
 
  2.  Enter LOADDSKF CSFBOOT.2DK A: /F. Label as CSF DISK Diskette 2 (SP
      DISK 2)
 
  3.  Enter LOADDSKF XR_W016.1DK A: /F. Label as FixPak XR_W016
      Corrective Service Diskette 1 (CSF DISK 1)
 
  4.  Enter LOADDSKF XR_W016.2DK A: /F. Label as FixPak XR_W016
      Corrective Service Diskette 2 (CSF DISK 2)
 
  5.  Enter LOADDSKF XR_W016.3DK A: /F. Label as FixPak XR_W016
      Corrective Service Diskette 3 (CSF DISK 3)
 
  6.  Enter LOADDSKF XR_W016.4DK A: /F. Label as FixPak XR_W016
      Corrective Service Diskette 4 (CSF DISK 4)
 
  7.  Enter LOADDSKF XR_W016.5DK A: /F. Label as FixPak XR_W016
      Corrective Service Diskette 5 (CSF DISK 5)
 
  8.  Enter LOADDSKF XR_W016.6DK A: /F. Label as FixPak XR_W016
      Corrective Service Diskette 6 (CSF DISK 6)
 
  9.  Enter LOADDSKF XR_W016.7DK A: /F. Label as FixPak XR_W016
      Corrective Service Diskette 7 (CSF DISK 7)
 
 
 
  READ ONLY FILES
 
  If you installed OS/2 Warp 3.0 from a CD-ROM some files being updated
  may have the Read Only attribute set. This will cause the update
  program to ask you if you want them replaced. Answer OK.
 
 
 
 
 
 
 
 
 
 
 
 
 
  
                                                   Installation Notes  3

 
                  December 15, 1995 Warp FixPak XR_W016
 
  RELOCATED OS/2 FILE SUPPORT
 
  This FixPak will service directories based on the location of
  supported SYSLEVEL.OS2 and SYSLEVEL.MPM files.  Please check your
  system to make sure extra copies of these files are not located in
  directories other than
 
    \OS2\INSTALL\SYSLEVEL.OS2 on the boot drive of your OS/2 partition(s)
    \MMOS2\INSTALL\SYSLEVEL.MPM on any partition
 
 
  If additional copies of these files are found in other locations on
  your harddrive then CSF will try to service files as follows:
 
  For SYSLEVEL.OS2
 
    ..\..\   all files in a directory two levels above (toward the root).
             This should be the root directory of your boot drive.
    ..\*     all files in a directory one level above (toward the root) and
             all subdirectories below. This should be the OS2 directory and
             subdirectories.
 
 
  For SYSLEVEL.MPM
 
    ..\*     all files in a directory one level above (toward the root) and
             all subdirectories below. This should be the MMOS2 directory and
             subdirectories.
 
 
  If you have moved OS/2 files or directories then you need to do the
  following in order to have them serviced:
 
  1.  Create a file USERDIRS.OS2 in the \OS2\INSTALL directory of the
      OS\2 Warp partition to be serviced.
 
      In this file you place the full path to the directory you want to
      be serviced. Examples would be
 
       C:\JSI\*
       D:\JSI\SH\*
 
 
      Be sure to include the trailing * (asterisk) after the last
      backslash.
 
  Note: Leave this file for any future OS/2 Warp FixPaks you may apply.
 
 
 
 
 
  
                                          Relocated OS/2 file support  4

 
                  December 15, 1995 Warp FixPak XR_W016
 
  INSTALLATION PROCESS
 
  Before installing any FixPak it is recommended that you run CHKDSK /F
  against all drives on your system to correct any file system errors
  that may be present. You cannot do this while OS/2 is active. You must
  shutdown and run CHKDSK by one of the following methods:
 
  þ   Boot from your Install and DISK 1 disks you used to install OS/2
      with.  If your file system is HPFS then you need to put diskette
      with CHKDSK and UHPFS.DLL on it in your A: drive before issuing
      the CHKDSK command.
 
  þ   Boot from the Utilities disk you created via the "Create Utility
      Diskettes" icon in the System Setup folder.
 
  þ   Boot from a different OS/2 partition
 
  To INSTALL this FixPak use one of the following methods:
 
 
  METHOD 1: INSTALL FROM BOOTED OS/2 PARTITION.
 
  This method allows you to select the partition or partitions to be
  serviced of those supported by this FixPak (based on the SYSLEVEL.OS2
  or SYSLEVEL.MPM files found).
 
  This is the method you should use if you have more than one OS/2
  partition and want to control which one will be serviced.
 
  Note: You can use a diskette drive other than A: with this method so
  if your 3.5" diskette drive is B: use B: where A: is mentioned (this
  method only).
 
  1.  Insert CSF DISK Diskette 1 in A:.
 
  2.  Open an OS/2 window or Full Screen.
 
  3.  Enter A:\SERVICE and press the ENTER key.
 
  4.  Follow displayed instructions. When prompted to insert Corrective
      Service Diskette 1 (not CSF DISK Diskette 1) place FixPak XR_W016
      Corrective Service Diskette 1 in A:. Repeat for the rest of the
      FixPak disks when requested to do so.
 
  5.  If this is the first OS/2 Warp FixPak you have applied to this
      system then enter the path where a copy of replaced file(s) will
      be stored in the ARCHIVE directory, Ex. D:\ARCHIVE.
 
      Note: This ARCHIVE directory is not related to the ARCHIVES
      directory built into OS/2 Warp 3.0. Please specify a different
      path.
 
  
                                                 Installation Process  5

 
                  December 15, 1995 Warp FixPak XR_W016
 
 
      Note: You must specify a different ARCHIVE directory for each
      product to be serviced
 
      If this is not the first OS/2 Warp v3.0 FixPak then enter the path
      where a copy of replaced file(s) will be stored in the BACKUP
      directory, EX. D:\BACKUP.
 
      Note: You must specify a different BACKUP directory for each
      product to be serviced
 
      For either case make sure there is sufficient space available on
      the drive you specify. Even though these files are kept in
      compressed (PACK2) format they will require approximately 7.0MB of
      disk space.
 
  6.  Click on "OK".
 
  7.  You will see an "Application in use" dialog box showing a list of
      locked files that cannot be serviced while the system is running.
      You are given two choices, to Continue or Reboot. Please select
      Continue.
 
  8.  During the install process you may see messages about Archiving,
      Updating and Deferring service.
 
      þ   Archiving saves a compressed copy of the original file in the
          ARCHIVE or BACKUP path you specified. These occur only if you
          apply service to the OS/2 partition you are booted from.
 
      þ   Updating means the original files is replaced with the new one
          from this FixPak.
 
      þ   Deferring service means the file to be updated is currently in
          use by the system and cannot be updated. The new files from
          the FixPak are placed in the \OS2\INSTALL\IBMCSFLK\FIX
          directory on your Warp boot drive in unpacked format for use
          by the locked file device driver during reboot after you
          shutdown.
 
  9.  Select NO for redisplay of "Product List" after the first part of
      the FixPak apply process has completed if this message is
      displayed.
 
  10. Click Cancel and Exit to close the Corrective Service Facility
      window if necessary.
 
  11. Shut down and reboot your system.
 
  12. You will see the following during reboot if you applied service to
      the OS/2 partition you were booted from.
 
  
                                                 Installation Process  6

 
                  December 15, 1995 Warp FixPak XR_W016
 
     The locked file driver is loaded.
 
            Processing locked files
 
            Processing complete
 
 
      After a bit the system may do an automatic reboot. In some cases
      it may do an additional reboot.
 
 
 
  METHOD 2: BOOT FROM CORRECTIVE SERVICE DISK 1.
 
  This method is fully automatic. No interaction with the user takes
  place. All serviceable partitions on your system will be serviced
  automatically. Be especially careful of extra SYSLEVEL.OS2 or
  SYSLEVEL.MPM files when using this method as they can direct CSF to
  apply service to directories you did not want serviced.
 
  1.  Shutdown your OS/2 system.
 
  2.  Insert CSF DISK Diskette 1 in A:.
 
  3.  Press Ctrl-Alt-Del to boot the disk in A:.
 
  Service will be applied to ALL partitions that have a version of OS/2
  on it that is supported by this FixPak. See the section "FixPak
  Corrective Service Notes" for the CSD levels this FixPak applies to.
 
 
  ADDITIONAL CORRECTIVE SERVICE FACILITY INFORMATION
 
  For additional information on the Corrective Service Facility, use the
  VIEW command with the README.INF file on the first Corrective Service
  Facility disk.
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
  
                                                 Installation Process  7

 
                  December 15, 1995 Warp FixPak XR_W016
 
  RECOVERING FROM INSTALLATION PROBLEMS
 
 
 
  NO FILES TO SERVICE
 
  If you see a "No files to service" message while applying this FixPak
  then the Current CSD level or Component ID of the "IBM OS/2 Base
  Operating System" may not be supported by this FixPak.
 
  Correct values must be:
 
  OS/2 Version        OS/2 Base Operating System  Mutimedia Presentation Manager
  ------------------  --------------------------  --------------------------
  Warp for Windows    Current CSD level: XR_3000  Current CSD level: XR_3000
                      Component ID: 562260100     Component ID: 562137400
 
  Warp with WIN-OS2   Current CSD level: XR_3001  Current CSD level: XR_3001
                      Component ID: 562274700     Component ID: 562274700
 
  Warp for Windows    Current CSD level: XR_3002  Current CSD level: XR_3002
  Mfg Refresh         Component ID: 562260100     Component ID: 562260100
 
  Warp with WIN-OS2   Current CSD level: XR_3003  Current CSD level: XR_3003
  Connect             Component ID: 562274700     Component ID: 562274700
 
  Warp for Windows    Current CSD level: XR_3004  Current CSD level: XR_3004
  Mfg Refresh Cnt     Component ID: 562260100     Component ID: 562260100
 
  Warp with WIN-OS2   Current CSD level: XR_3005  Current CSD level: XR_3005
  Server              Component ID: 562274700     Component ID: 562274700
 
 
  If these values are correct then check for the following files on your
  OS/2 boot drive in the \OS2\INSTALL directory and in your
  MMOS2\INSTALL directory wherever it is installed.
 
     LOGF0000.OS2
     LOGSTART.OS2
     LOGARCH.OS2
 
 
  Also check for the following file:
 
     C:\CSF_SEL.000
 
 
  If any of them exist then rename them and try the FixPak install
  again.  If it works then delete the renamed files.
 
 
 
  
                                Recovering from Installation problems  8

 
                  December 15, 1995 Warp FixPak XR_W016
 
  PREVIOUS INSTALLATION INTERRUPTED
 
  If you get a message that the previous installation of a FixPak was
  interrupted even though it completed successfully then check for the
  following file:
 
     C:\FIXSTART
 
 
  If it exists then rename it and try the FixPak install again.  If it
  works then delete the renamed file. If this does not resolve the
  problem then follow the procedure "Recovering from Installation
  problems".
 
 
  UNABLE TO OPEN ARCHIVE DIRECTORY
 
  If you get a message about problems with the Archive directory (cannot
  find, unable to open, etc) then the most probable cause is that you
  have applied a previous FixPak and have deleted the FixPak ARCHIVE or
  BACKUP directory to recover the space.
 
  To recover from this follow the "No files to service" and "Previous
  installation interrupted" steps.
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
  
                                Recovering from Installation problems  9

 
                  December 15, 1995 Warp FixPak XR_W016
 
  SYSTEM PROBLEMS AFTER FIXPAK INSTALLATION
 
 
 
  UPDATING SYSTEMS WITH THE CMD CHIPSET
 
  If you are installing this FixPak on a machine that has the CMD PCI
  IDE chipset a CONFIG.SYS modification will be required after this
  FixPak is installed.
 
  Add the following statements to your CONFIG.SYS
 
     BASEDEV=CMD640X.ADD     (add this line below BASEDEV=IBM1S506.ADD)
     BASEDEV=CMDATAPI.FLT    (add this line below BASEDEV=IBMIDECD.FLT)
 
 
 
 
  RZ1000 AND CMD640 DATA PROBLEMS (APAR=PJ19409)
 
  Problem Description:
 
  IDE disks can incur possible data read conflicts that can cause data
  problems.
 
  OS/2 Versions:
 
  All versions of OS/2 Warp
 
  To Verify System Susceptibility to this Problem:
 
  To verify existence of the problem on your system, you may turn on the
  verbose option on the new IBM1S506.ADD.  After installing the update
  per the instructions above, edit config.sys and add the /V (verbose)
  switch option to the IBM1S506.ADD line:
 
          BASEDEV=IBM1S506.ADD /V
 
 
  If your config.sys does not have this line you may add it any place
  before the line:
 
          BASEDEV=CMD640X.ADD
 
 
  After adding the /V and rebooting your system, if your system displays
  on the 3rd line of disk information during start-up:
 
 
 
 
 
  
                           System problems after Fixpak installation  10

 
                  December 15, 1995 Warp FixPak XR_W016
 
     PCI Rev: 02.00  RZ1000 PCI to IDE IC, Rev: 0x01  VID:0x1000 DID:0x1042
                             or
     PCI Rev: 02.00  CMD640 PCI to IDE IC, Rev: 0x01  VID:0x1095 DID:0x0640
 
 
  then your system does contain an RZ1000 or CMD640 chip and is
  susceptible to the above problem.
 
  Warning: on some systems this message may be displayed for only a
  brief time during system boot.
 
  If no such line appears, then you may revert to the originally shipped
  device drivers or leave the new drivers installed.
 
  Note: This fix has no affect on other IDE systems.
 
  Remove the /V option from config.sys if you no longer want the verbose
  information displayed.
 
  Fix Description:
 
  Disable Read-ahead mode for the RZ1000 and CMD640x PCI IDE chips in
  the OS/2 IBM1S506.ADD and CMD640X.ADD device drivers.  These are
  generic device drivers which fix all the above releases and are
  compatible with systems that DO NOT use the RZ1000 or CMD640x chips.
 
  The new IBM1S506 device driver detects the RZ1000 and disables
  read-ahead for both RZ1000 IDE channels.  The IBM1S506 device driver
  also detects the CMD640x chip and disables read-ahead for the primary
  IDE channel.
 
  The new CMD640X device driver detects the CMD640 chip and disables
  read-ahead mode for both CANT IDE channels.
 
  Also included with this fix distribution are the corresponding ATAPI
  CD-ROM device drivers so as to remain synchronized with IDE drivers.
 
          IBM1S506.ADD   -> Generic IDE/ATA Device Driver
          IBMIDECD.FLT   -> Generic IDE/ATAPI Device Driver
 
          CMD640X.ADD    -> CMD Optimized IDE/ATA Device Driver
          CMDATAPI.FLT   -> CMD Optimized IDE/ATAPI Device Driver
 
 
  Performance Impact:
 
  IBM's benchmarks show no system performance degradation by disabling
  the read-ahead mode in either the RZ1000 or CMD640 IDE PCI interface
  chips.
 
 
 
  
                           System problems after Fixpak installation  11

 
                  December 15, 1995 Warp FixPak XR_W016
 
  SYS3175 WHEN OPENING LS 4.0 LAN SERVER ADMINISTRATION
 
  Contact IBM LAN support and request the fix for APAR IC11718 which is
  IP08169.
 
  If you need relief while waiting to obtain the fix, a temporary
  workaround for this problem is to backout SOM.DLL to the pre-Fixpak
  level as follows
 
  1.  Shutdown your system.
 
  2.  Reboot and press Alt-F1 when you see OS/2 and a white block in the
      top left corner of the screen.
 
  3.  Press C to goto a command prompt.
 
  4.  Rename x:\OS2\DLL\SOM.DLL to SOMFP.DLL (x: is your OS/2 boot
      drive)
 
  5.  Change to the Fixpak archive directory
 
  6.  Enter  UNPACK SOM.DL_ x:\OS2\DLL       (x: is your OS/2 boot
      drive)
 
  7.  Enter  EXIT
 
  Your system will reboot with the pre-FixPak version of SOM.DLL in
  place. The SYS3175 problem should be resolved.
 
  Once you receive and apply the fix for APAR IC11718 you should do the
  following to reinstall SOM.DLL from this FixPak.
 
  1.  Shutdown your system.
 
  2.  Reboot and press Alt-F1 when you see OS/2 and a white block in the
      top left corner of the screen.
 
  3.  Press C to goto a command prompt.
 
  4.  Delete x:\OS2\DLL\SOM.DLL              (x: is your OS/2 boot
      drive)
 
  5.  Rename x:\OS2\DLL\SOMFP.DLL to SOM.DLL (x: is your OS/2 boot
      drive)
 
  6.  Enter  EXIT
 
 
 
 
 
 
  
                           System problems after Fixpak installation  12

 
                  December 15, 1995 Warp FixPak XR_W016
 
  TRAPS WHEN CANCELLING PRINT JOBS AFTER FIXPAK IS INSTALLED
 
  If you experience a Trap when cancelling print jobs using a Laserjet
  driver, down load the Laserjet driver FixPak XR0P012, revision level
  30.453 or later from any of the sites listed in "Where fixes can be
  found" section of this document.
 
  If you are using the IBMNULL printer driver call service for APAR
  PJ19995.
 
 
  NOVELL REQUESTER
 
  If you are using Novell Requester for OS/2 you need to obtain the
  latest version of OS2C1.EXE. The number for the Novell BBS is
  801-221-5197.
 
 
  SYSTEM DATE CHANGING ERRATICALLY (APAR= PJ21043)
 
  IF you experience a problem where your system date jumps ahead
  whenever you open a DOS session then you need to backout VCMOS.SYS to
  the version prior to applying this FixPak.
 
  Do the following:
 
  1.  Shutdown your system.
 
  2.  Reboot and press Alt-F1 when you see OS/2 and a white block in the
      top left corner of the screen.
 
  3.  Press C to goto a command prompt.
 
  4.  Rename x:\OS2\MDOS\VCMOS.SYS VCMOSFP.SYS (x: is your OS/2 boot
      drive)
 
  5.  Change to the FixPak archive directory
 
  6.  Enter  UNPACK VCMOS.SY_ x:\OS2\MDOS      (x: is your OS/2 boot
      drive)
 
  7.  Enter  EXIT
 
  System will reboot. Reset the system date.
 
 
 
 
 
 
 
 
  
                           System problems after Fixpak installation  13

 
                  December 15, 1995 Warp FixPak XR_W016
 
  CSD LEVEL OF SYSLEVEL.OS2
 
  The Current CSD level for the "IBM OS/2 Base Operating System" will
  not be changed by installation of this FixPak even though the
  SERVICE.LOG file states it will. This FixPak is not a Service Level
  change, it upgrades the existing service level (XR_300n), therefore
  the SYSLEVEL is not changed. All fix information is recorded in the
  SERVICE.LOG.
 
  Look at the file
 
     \OS2\INSTALL\SERVICE.LOG
 
 
  for information relating to the installation of this (or any) FixPak
  on your system. To see the current level and other related information
  use the SYSLEVEL command.
 
  Use the VER /R command to see the current revision of OS/2 installed.
  The response will look like the following for this FixPak:
 
  The Operating System/2 Version is 3.00
  Revision 8.240
 
             -- or --
 
  The Operating System/2 Version is 3.01
  Revision 8.240
 
 
  Look at README.1ST on the first FixPak disk of any FixPak for the
  Build Level: n.nnn line.  That is the number you should see for that
  FixPak when you issue the VER /R command.
 
 
  See the README2 file on the first FixPak disk for a list of APARs
  fixed.
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
  
                                           CSD level of SYSLEVEL.OS2  14

 
                  December 15, 1995 Warp FixPak XR_W016
 
  WHERE FIXES CAN BE FOUND
 
  You can find other files, such as new drivers or fixes for specific
  video cards, from the following locations:
 
  þ   CompuServe - Subscribers can download fixes from the OS/2 Support
      Forum (GO OS2SUPPO).
 
  þ   IBM OS/2 BBS - Subscribers can download fixes from the Software
      Download Library. U.S. customers who are not subscribers can call
      1-800-547-1283 for information on how to subscribe.
 
  þ   Internet - Customers with access to Internet services can download
      fixes using the following methods:
 
        Anonymous FTP to "ftp.software.ibm.com" (IP Address 198.17.57.66)
        fixes are located in the "/ps/products/os2/fixes" directory.
 
        World Wide Web (WWW) access via:
          IBM Home Page                         http://www.ibm.com
          IBM Software Manufacturing Solutions  http://service.boulder.ibm.com
 
 
  þ   Prodigy - Subscribers can download fixes from the OS2CLUB in the
      Download Library, IBM Files, Fixes area. Files are updated weekly
      and are available on Friday.
 
  þ   PCC BBS - Customers can call the IBM Personal Computer Company BBS
      In Raleigh NC, and download fixes from the public area. You can
      access this BBS at 1-919-517-0001.
 
  þ   America On line - Subscribers can download fixes from the OS/2
      Area.
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
  
                                            Where Fixes can be found  15

 
                  December 15, 1995 Warp FixPak XR_W016
 
  FIXPAK CORRECTIVE SERVICE LEVELS AND DISK LAYOUTS
 
  Build Level: 8.240
 
  Product location on CSD:  A:\FIX\OS2.1
  Product name:  "IBM OS/2 Base Operating System"
  Standard Edition  3.00
  Fixpak name:   XR_W016_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3000_
  System Id:  1000
  Component Id:  562260100
  Archive is ON for this product.
  _____________________________________________________________
  Product name:  "IBM OS/2 Base Operating System"
  Standard Edition  3.00
  Fixpak name:   XR_W016_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3001_
  System Id:  1000
  Component Id:  562274700
  Archive is ON for this product.
  _____________________________________________________________
  Product name:  "IBM OS/2 Base Operating System"
  Standard Edition  3.01
  Fixpak name:   XR_W016_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3002_
  System Id:  1000
  Component Id:  562260100
  Archive is ON for this product.
  _____________________________________________________________
  Product name:  "IBM OS/2 Base Operating System"
  Standard Edition  3.00
  Fixpak name:   XR_W016_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3003_
  System Id:  1000
  Component Id:  562274700
  Archive is ON for this product.
  _____________________________________________________________
  Product name:  "IBM OS/2 Base Operating System"
  Standard Edition  3.01
  Fixpak name:   XR_W016_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3004_
  System Id:  1000
  Component Id:  562260100
  Archive is ON for this product.
  _____________________________________________________________
  Product name:  "IBM OS/2 Base Operating System"
  Standard Edition  3.01
  Fixpak name:   XR_W016_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3005_
  System Id:  1000
  Component Id:  562274700
 
  
                   FixPak Corrective Service levels and disk layouts  16

 
                  December 15, 1995 Warp FixPak XR_W016
 
  Archive is ON for this product.
  _____________________________________________________________
 
  Default directories:
 
          ..\..\
          ..\*
 
  Files contained in Fixpak for product:
 
  Filename      Name on CSD   Disk#  Date      Time   Size
  ------------  ------------  -----  --------  -----  -------
  AHA152X.ADD   AHA152X.AD_     5    10/30/95  14:54    38060
  AHA164X.ADD   AHA164X.AD_     6    10/30/95  14:52    19716
  AIC7770.ADD   AIC7770.AD_     5    10/30/95  14:54    42428
  AIC7870.ADD   AIC7870.AD_     5    10/30/95  14:55    34124
  APM.SYS       APM.SY_         6    10/30/95  15:16     6704
  ARCINST.EXE   ARCINST.EX_     6    12/05/95  02:15    21358
  ARCRECOV.EXE  ARCRECOV.EX_    6    12/05/95  02:16    24635
  AUTODRV2.SYS  AUTODRV2.SY_    6    11/29/95  22:11    10862
  BTSCSI.ADD    BTSCSI.AD_      6    10/30/95  15:01    22485
  BVHVGA.DLL    BVHVGA.DL_      5    12/04/95  19:44    31054
  BVHWNDW.DLL   BVHWNDW.DL_     6    12/04/95  19:45    12664
  CDFS.IFS      CDFS.IF_        6    12/04/95  21:34    41795
  CDROM.TBL     CDROM.TB_       6    05/19/95  17:16     3949
  CHKDSK.COM    CHKDSK.CO_      5    12/04/95  23:07    68656
  CMD.EXE       CMD.EX_         5    12/04/95  23:16    79360
  CMD640X.ADD   CMD640X.AD_     5    10/30/95  17:35    35924
  CMDATAPI.FLT  CMDATAPI.FL_    6    10/30/95  15:03    21554
  COM.SYS       COM.SY_         6    10/30/95  15:15    16912
  COMMAND.COM   COMMAND.CO_     5    12/04/95  23:16    52972
  DATABASE.DAT  DATABASE.DA_    5    12/05/95  00:19    83419
  DATABASE.TXT  DATABASE.TX_    5    08/17/95  09:30   609497
  DETNE2.SYS    DETNE2.SY_      6    10/30/95  14:41     5640
  DISPLAY.DLL   DISPLAY.DL_     5    12/04/95  22:32    44196
  DOSCALL1.DLL  DOSCALL1.DL_    3    12/04/95  22:44   123186
  DOSKRNL       DOSKRNL.___     6    12/04/95  19:53    30077
  DPT20XX.ADD   DPT20XX.AD_     6    10/30/95  14:59    24254
  DSPINSTL.EXE  DSPINSTL.EX_    5    12/05/95  00:35   170424
  E.EXE         E.EX_           5    12/04/95  22:57    70917
  EAUTIL.EXE    EAUTIL.EX_      5    12/04/95  23:23    37984
  FD16-700.ADD  FD16-700.AD_    6    11/29/95  21:59    31260
  FD7000EX.ADD  FD7000EX.AD_    6    11/29/95  22:01    20848
  FD8XX.ADD     FD8XX.AD_       6    11/29/95  22:02    30030
  FDISK.COM     FDISK.CO_       5    12/04/95  21:50   110245
  FORMAT.COM    FORMAT.CO_      5    12/04/95  23:34    68880
  FSFILTER.SYS  FSFILTER.SY_    6    12/05/95  03:20    12988
  HELPMGR.DLL   HELPMGR.DL_     4    12/04/95  23:30   176108
  HELPMSG.EXE   HELPMSG.EX_     5    12/04/95  23:34    36256
  HPFS.IFS      HPFS.IF_        1    12/09/95  15:17   143938
  IBM16AFS.EXE  IBM16AFS.EX_    6    11/29/95  22:03     3177
 
  
                   FixPak Corrective Service levels and disk layouts  17

 
                  December 15, 1995 Warp FixPak XR_W016
 
  IBM1FLPY.ADD  IBM1FLPY.AD_    6    10/30/95  14:47    31170
  IBM1S506.ADD  IBM1S506.AD_    6    10/30/95  15:13    30636
  IBM2AMB1.SYS  IBM2AMB1.SY_    6    11/29/95  22:18    12437
  IBM2AST1.SYS  IBM2AST1.SY_    6    11/29/95  22:18    10047
  IBM2CAD1.SYS  IBM2CAD1.SY_    6    11/29/95  22:20    12479
  IBM2CMQ1.SYS  IBM2CMQ1.SY_    6    11/29/95  22:18    10085
  IBM2FLPY.ADD  IBM2FLPY.AD_    6    10/30/95  14:47    13754
  IBM2IDE.ADD   IBM2IDE.AD_     6    10/30/95  15:13    31396
  IBM2MAT1.SYS  IBM2MAT1.SY_    6    11/29/95  22:20    10067
  IBM2NCR1.SYS  IBM2NCR1.SY_    6    11/29/95  22:19    10047
  IBM2NEC1.SYS  IBM2NEC1.SY_    6    11/29/95  22:19    10047
  IBM2SCSI.ADD  IBM2SCSI.AD_    6    10/30/95  14:50    32691
  IBM2SS01.SYS  IBM2SS01.SY_    6    11/29/95  22:16    13203
  IBM2SS02.SYS  IBM2SS02.SY_    6    11/29/95  22:17    10477
  IBM2TOS1.SYS  IBM2TOS1.SY_    6    11/29/95  22:17    10054
  IBM2ZEN1.SYS  IBM2ZEN1.SY_    6    11/29/95  22:17    10047
  IBM2ZOS1.SYS  IBM2ZOS1.SY_    6    11/29/95  22:19    10063
  IBMIDECD.FLT  IBMIDECD.FL_    6    10/30/95  15:14    20358
  IBMKBD.SYS    IBMKBD.SY_      6    07/18/95  09:31     5612
  ICMEMCDD.SYS  ICMEMCDD.SY_    6    11/29/95  22:22    13932
  ICMEMFMT.EXE  ICMEMFMT.EX_    5    11/29/95  22:24    51031
  ICMEMMTD.SYS  ICMEMMTD.SY_    6    11/29/95  22:23     8300
  KBDBASE.SYS   KBDBASE.SY_     6    10/30/95  15:17    28501
  KEYBOARD.DCP  KEYBOARD.DC_    6    12/04/95  23:36   157804
  LINK386.EXE   LINK386.EX_     4    10/31/94  19:41   154052
  LMS205.ADD    LMS205.AD_      6    10/30/95  15:14    36380
  LMS206.ADD    LMS206.AD_      6    10/30/95  15:14    38732
  MIGRATE.EXE   MIGRATE.EX_     4    12/05/95  00:12   173644
  MINXOBJ.DLL   MINXOBJ.DL_     5    12/05/95  00:30    37543
  MIRRORS.DLL   MIRRORS.DL_     1    11/07/95  16:36   705196
  MITFX001.ADD  MITFX001.AD_    6    10/30/95  15:08    20488
  MOUSE.SYS     MOUSE.SY_       6    10/30/95  15:15    18169
  NPXEMLTR.DLL  NPXEMLTR.DL_    6    12/04/95  23:58    20692
  NWIAPI.DLL    NWIAPI.DL_      6    12/04/95  18:56    10075
  OS2ASPI.DMD   OS2ASPI.DM_     6    10/30/95  14:45    10970
  OS2CDROM.DMD  OS2CDROM.DM_    6    10/30/95  15:05    26580
  OS2CHAR.DLL   OS2CHAR.DL_     6    12/04/95  22:37      512
  OS2DASD.DMD   OS2DASD.DM_     6    10/30/95  14:44    34228
  OS2DUMP       OS2DUMP.___     6    12/04/95  19:02    16909
  OS2KRNL       OS2KRNL.___     2    12/04/95  21:31   571440
  OS2LDR        OS2LDR.___      6    12/04/95  18:59    30208
  OS2LDR.MSG    OS2LDR.MS_      6    12/04/95  19:02     8430
  OS2MM.DLL     OS2MM.DL_       4    11/27/95  20:21   366710
  OSO001.MSG    OSO001.MS_      5    12/04/95  18:21   174390
  OSO001H.MSG   OSO001H.MS_     5    12/04/95  18:22   240113
  PCM2ATA.ADD   PCM2ATA.AD_     6    10/30/95  15:30    23110
  PCMCIA.SYS    PCMCIA.SY_      5    11/29/95  22:10    47622
  PCMCIA.TBL    PCMCIA.TB_      6    01/24/95  19:28     1681
  PMCTLS.DLL    PMCTLS.DL_      3    12/16/95  13:11   613242
  PMDDE.DLL     PMDDE.DL_       6    12/05/95  00:25    24008
  PMDRAG.DLL    PMDRAG.DL_      6    12/16/95  13:10     1731
 
  
                   FixPak Corrective Service levels and disk layouts  18

 
                  December 15, 1995 Warp FixPak XR_W016
 
  PMGPI.DLL     PMGPI.DL_       4    12/08/95  22:38   335438
  PMGRE.DLL     PMGRE.DL_       6    12/12/95  21:15     2231
  PMMERGE.DLL   PMMERGE.DL_     1    12/13/95  17:53  1185784
  PMMLE.DLL     PMMLE.DL_       6    12/08/95  16:06      673
  PMPRINT.QPR   PMPRINT.QP_     6    12/04/95  19:13    12249
  PMSDMRI.DLL   PMSDMRI.DL_     6    12/08/95  16:06    12800
  PMSHAPI.DLL   PMSHAPI.DL_     6    11/14/95  14:04     4549
  PMSPL.DLL     PMSPL.DL_       4    12/04/95  19:35   211690
  PMVDMP.DLL    PMVDMP.DL_      5    12/04/95  22:53    45851
  PMVIOP.DLL    PMVIOP.DL_      5    12/04/95  22:52    54070
  PMWIN.DLL     PMWIN.DL_       6    12/13/95  17:51    11264
  PMWP.DLL      PMWP.DL_        2    12/04/95  20:56   939461
  PMWPMRI.DLL   PMWPMRI.DL_     5    12/04/95  20:31    45342
  POINTDD.SYS   POINTDD.SY_     1    08/09/95  16:23     1811
  PRINT01.SYS   PRINT01.SY_     6    10/30/95  15:33    11038
  PRINT02.SYS   PRINT02.SY_     6    10/30/95  15:33    10166
  QUECALLS.DLL  QUECALLS.DL_    6    12/04/95  22:36     1024
  RESERVE.SYS   RESERVE.SY_     6    10/30/95  14:41     5702
  RESTORE.EXE   RESTORE.EX_     5    12/05/95  00:03    36080
  REXX.DLL      REXX.DL_        4    09/07/95  10:20   254768
  REXXAPI.DLL   REXXAPI.DL_     6    08/17/95  09:34    33735
  REXXUTIL.DLL  REXXUTIL.DL_    6    06/09/95  16:49    30331
  RSPDSPI.EXE   RSPDSPI.EX_     5    12/05/95  00:46   141752
  RSPINST.EXE   RSPINST.EX_     4    12/04/95  22:00   342752
  RUPINST2.EXE  RUPINST2.EX_    4    12/04/95  21:52   151024
  SBCD2.ADD     SBCD2.AD_       6    10/30/95  15:08    18834
  SEAMLESS.DLL  SEAMLESS.DL_    5    12/04/95  23:37    42624
  SEMAINT.EXE   SEMAINT.EX_     5    12/05/95  00:07    65984
  SESMGR.DLL    SESMGR.DL_      6    12/04/95  19:40     1536
  SETBOOT.EXE   SETBOOT.EX_     6    12/04/95  21:48    19632
  SIPANEL2.DLL  SIPANEL2.DL_    6    12/04/95  21:37    49472
  SOM.DLL       SOM.DL_         5    10/27/95  21:00   130955
  SOM.IR        SOM.IR_         4    10/27/95  21:00   496503
  SOMD.DLL      SOMD.DL_        2    10/27/95  21:00   434110
  SOMD.MSG      SOMD.MS_        6    10/27/95  21:01    15056
  SOMDD.EXE     SOMDD.EX_       6    10/27/95  21:01    37904
  SOMDSVR.EXE   SOMDSVR.EX_     6    10/27/95  21:01    34912
  SOMEM.DLL     SOMEM.DL_       5    10/27/95  21:00    59700
  SOMIR.DLL     SOMIR.DL_       5    10/27/95  21:01   132044
  SOMK.MSG      SOMK.MS_        3    10/27/95  21:01     3718
  SOMS.DLL      SOMS.DL_        6    10/27/95  21:01    31138
  SOMTC.DLL     SOMTC.DL_       5    10/27/95  21:01    42432
  SOMU.DLL      SOMU.DL_        5    10/27/95  21:01   126228
  SONY31A.ADD   SONY31A.AD_     6    10/30/95  15:11    32588
  SS2PCIC1.SYS  SS2PCIC1.SY_    6    11/29/95  22:16    10549
  SS2TCIC1.SYS  SS2TCIC1.SY_    6    11/29/95  22:16    12595
  SSVLSI.SYS    SSVLSI.SY_      6    11/29/95  22:20     6502
  SYSINST1.EXE  SYSINST1.EX_    6    12/04/95  21:45     4224
  SYSINST2.EXE  SYSINST2.EX_    4    12/04/95  21:51   149856
  SYSINSTX.COM  SYSINSTX.CO_    5    12/04/95  19:04    39472
  SYSLEVEL.SDS  SYSLEVEL.SD_    6    12/07/95  21:35      254
 
  
                   FixPak Corrective Service levels and disk layouts  19

 
                  December 15, 1995 Warp FixPak XR_W016
 
  SYSLEVEL.SEM  SYSLEVEL.SE_    6    12/07/95  21:35      191
  SYSLEVEL.SIR  SYSLEVEL.SI_    6    12/07/95  21:35      188
  SYSLEVEL.SRK  SYSLEVEL.SR_    6    12/07/95  21:35      185
  SYSLEVEL.SUT  SYSLEVEL.SU_    2    12/07/95  21:35      177
  SYSTEM.TDF    SYSTEM.TD_      6    12/13/95  18:49    82893
  SYSTEM.TFF    SYSTEM.TF_      5    12/13/95  18:49   109330
  TEDIT.EXE     TEDIT.EX_       6    12/05/95  00:07     9390
  TESTCFG.SYS   TESTCFG.SY_     6    10/30/95  15:33     5434
  TRACEFMT.DLL  TRACEFMT.DL_    6    12/05/95  00:33    18061
  TRACEFMT.EXE  TRACEFMT.EX_    5    12/05/95  00:38    53793
  UCDFS.DLL     UCDFS.DL_       6    12/04/95  21:24    13264
  UHPFS.DLL     UHPFS.DL_       4    12/09/95  15:12   187088
  UNPACK2.EXE   UNPACK2.EX_     5    12/05/95  00:11    79792
  VBIOS.SYS     VBIOS.SY_       6    12/05/95  00:07     8688
  VCMOS.SYS     VCMOS.SY_       5    12/05/95  00:07     5744
  VCOM.SYS      VCOM.SY_        6    12/05/95  00:09    12384
  VDPMI.SYS     VDPMI.SY_       4    12/05/95  00:11    22337
  VDPX.SYS      VDPX.SY_        6    12/04/95  23:56    25857
  VKBD.SYS      VKBD.SY_        6    12/05/95  00:11    23575
  VLPT.SYS      VLPT.SY_        6    12/05/95  00:16    10113
  VPIC.SYS      VPIC.SY_        6    12/05/95  00:12     9894
  VTIMER.SYS    VTIMER.SY_      6    12/05/95  00:12     9936
  VWIN.SYS      VWIN.SY_        6    12/05/95  00:18    24592
  VXGA.SYS      VXGA.SY_        6    12/05/95  00:01    24772
  WPCMPNP.DLL   WPCMPNP.DL_     2    12/05/95  00:33   131769
  WPCONFIG.DLL  WPCONFIG.DL_    3    12/04/95  22:28   253747
  WPHELP.HLP    WPHELP.HL_      3    12/05/95  00:16   704236
  WPPRINT.DLL   WPPRINT.DL_     3    12/04/95  22:04   349829
  WPPRTMRI.DLL  WPPRTMRI.DL_    5    12/04/95  22:04    47482
  XDFH.MSG      XDFH.MS_        2    12/04/95  23:25     1045
 
  *************************************************************
  Product location on CSD:  A:\FIX\OS2.2
  Product name:  "IBM OS/2 Base Operating System"
  Standard Edition  3.00
  Fixpak name:   XR_W016_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3000_
  System Id:  1000
  Component Id:  562260100
  Archive is ON for this product.
  _____________________________________________________________
  Product name:  "IBM OS/2 Base Operating System"
  Standard Edition  3.01
  Fixpak name:   XR_W016_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3002_
  System Id:  1000
  Component Id:  562260100
  Archive is ON for this product.
  _____________________________________________________________
  Product name:  "IBM OS/2 Base Operating System"
  Standard Edition  3.01
 
  
                   FixPak Corrective Service levels and disk layouts  20

 
                  December 15, 1995 Warp FixPak XR_W016
 
  Fixpak name:   XR_W016_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3004_
  System Id:  1000
  Component Id:  562260100
  Archive is ON for this product.
  _____________________________________________________________
 
  Default directories:
 
          ..\..\
          ..\*
 
  Files contained in Fixpak for product:
 
  Filename      Name on CSD   Disk#  Date      Time   Size
  ------------  ------------  -----  --------  -----  -------
  COMMS.SCR     COMMS.SC_       6    12/04/95  18:49     2560
  FIXMGR.DLL    FIXMGR.DL_      6    12/04/95  18:49     2048
  GDIS.SCR      GDIS.SC_        6    12/04/95  18:49     6144
  INSTALL.EXE   INSTALL.EX_     6    05/05/95  19:31   466324
  MCISEQS.SCR   MCISEQS.SC_     6    12/04/95  18:48     2048
  TIMERS.SCR    TIMERS.SC_      6    12/04/95  18:51     2048
  USERS.SCR     USERS.SC_       6    12/04/95  18:49    17408
  WINOS2.COM    WINOS2.CO_      6    12/04/95  18:49    31866
  WINSCLIP.DLL  WINSCLIP.DL_    6    12/04/95  18:50    20480
  WINSDDE.DLL   WINSDDE.DL_     6    12/04/95  18:50    24064
  WINSHELD.EXE  WINSHELD.EX_    6    12/04/95  18:50    23552
  WINSMSG.DLL   WINSMSG.DL_     6    12/04/95  18:50    29184
 
  *************************************************************
  Product location on CSD:  A:\FIX\OS2.3
  Product name:  "IBM OS/2 Base Operating System"
  Standard Edition  3.00
  Fixpak name:   XR_W016_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3001_
  System Id:  1000
  Component Id:  562274700
  Archive is ON for this product.
  _____________________________________________________________
  Product name:  "IBM OS/2 Base Operating System"
  Standard Edition  3.00
  Fixpak name:   XR_W016_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3003_
  System Id:  1000
  Component Id:  562274700
  Archive is ON for this product.
  _____________________________________________________________
  Product name:  "IBM OS/2 Base Operating System"
  Standard Edition  3.01
  Fixpak name:   XR_W016_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3005_
 
  
                   FixPak Corrective Service levels and disk layouts  21

 
                  December 15, 1995 Warp FixPak XR_W016
 
  System Id:  1000
  Component Id:  562274700
  Archive is ON for this product.
  _____________________________________________________________
 
  Default directories:
 
          ..\..\
          ..\*
 
  Files contained in Fixpak for product:
 
  Filename      Name on CSD   Disk#  Date      Time   Size
  ------------  ------------  -----  --------  -----  -------
  COMM.DRV      COMM.DR_        7    06/12/95  16:58     9520
  COMMDLG.DLL   COMMDLG.DL_     7    11/29/95  18:26    89296
  GDI.EXE       GDI.EX_         7    11/29/95  18:29   226000
  INSTALL.EXE   INSTALL.EX_     6    12/04/95  21:45   476318
  OS2K386.EXE   OS2K386.EX_     7    11/29/95  18:29    80066
  S8514.DRV     S8514.DR_       7    06/12/95  16:53    89744
  USER.EXE      USER.EX_        7    11/08/95  14:35   276800
  WINSCLIP.DLL  WINSCLIP.DL_    7    11/29/95  18:30    14848
  WINSDDE.DLL   WINSDDE.DL_     6    11/29/95  18:31    17920
  WINSHELD.EXE  WINSHELD.EX_    6    11/29/95  18:30    20992
  WINSMSG.DLL   WINSMSG.DL_     6    11/29/95  18:30    24857
 
  *************************************************************
  Product location on CSD:  A:\FIX\OS2.4
  Product name:  "IBM OS/2 Base Operating System"
  Standard Edition  3.00
  Fixpak name:   XR_W016_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3003_
  System Id:  1000
  Component Id:  562274700
  Archive is ON for this product.
  _____________________________________________________________
  Product name:  "IBM OS/2 Base Operating System"
  Standard Edition  3.01
  Fixpak name:   XR_W016_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3004_
  System Id:  1000
  Component Id:  562260100
  Archive is ON for this product.
  _____________________________________________________________
  Product name:  "IBM OS/2 Base Operating System"
  Standard Edition  3.01
  Fixpak name:   XR_W016_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3005_
  System Id:  1000
  Component Id:  562274700
  Archive is ON for this product.
 
  
                   FixPak Corrective Service levels and disk layouts  22

 
                  December 15, 1995 Warp FixPak XR_W016
 
  _____________________________________________________________
 
  Default directories:
 
          ..\..\
          ..\*
 
  Files contained in Fixpak for product:
 
  Filename      Name on CSD   Disk#  Date      Time   Size
  ------------  ------------  -----  --------  -----  -------
  REXX.DLL      REXX.DL_        7    12/13/95  19:50   248416
  REXXAPI.DLL   REXXAPI.DL_     7    12/13/95  19:50    33415
  REXXUTIL.DLL  REXXUTIL.DL_    7    12/13/95  19:50    30315
 
  *************************************************************
  Product location on CSD:  A:\FIX\MPM.5
  Product name:  "IBM Multimedia Presentation Manager/2"
  Standard Edition  3.00
  Fixpak name:   XR_W016_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3000_
  System Id:  1000
  Component Id:  562137400
  Archive is ON for this product.
  _____________________________________________________________
  Product name:  "IBM Multimedia Presentation Manager/2"
  Standard Edition  3.00
  Fixpak name:   XR_W016_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3001_
  System Id:  1000
  Component Id:  562274700
  Archive is ON for this product.
  _____________________________________________________________
  Product name:  "IBM Multimedia Presentation Manager/2"
  Standard Edition  3.01
  Fixpak name:   XR_W016_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3002_
  System Id:  1000
  Component Id:  562260100
  Archive is ON for this product.
  _____________________________________________________________
  Product name:  "IBM Multimedia Presentation Manager/2"
  Standard Edition  3.00
  Fixpak name:   XR_W016_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3003_
  System Id:  1000
  Component Id:  562274700
  Archive is ON for this product.
  _____________________________________________________________
  Product name:  "IBM Multimedia Presentation Manager/2"
  Standard Edition  3.01
 
  
                   FixPak Corrective Service levels and disk layouts  23

 
                  December 15, 1995 Warp FixPak XR_W016
 
  Fixpak name:   XR_W016_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3004_
  System Id:  1000
  Component Id:  562260100
  Archive is ON for this product.
  _____________________________________________________________
  Product name:  "IBM Multimedia Presentation Manager/2"
  Standard Edition  3.01
  Fixpak name:   XR_W016_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3005_
  System Id:  1000
  Component Id:  562274700
  Archive is ON for this product.
  _____________________________________________________________
 
  Default directories:
 
          ..\*
 
  Files contained in Fixpak for product:
 
  Filename      Name on CSD   Disk#  Date      Time   Size
  ------------  ------------  -----  --------  -----  -------
  AUDIOSH.DLL   AUDIOSH.DL_     6    11/27/95  19:00      532
  BUSAUDIO.SYS  BUSAUDIO.SY_    7    11/27/95  18:48    27949
  CS4231.SYS    CS4231.SY_      7    06/15/95  15:39    33145
  ES688DD.SYS   ES688DD.SY_     7    11/27/95  18:34    44944
  MEMSH.DLL     MEMSH.DL_       7    11/27/95  18:31    12752
  MMPM.DLL      MMPM.DL_        7    11/27/95  20:36   704504
  MPGIO.DLL     MPGIO.DL_       7    11/27/95  18:53    25219
  MVPRODD.SYS   MVPRODD.SY_     7    11/27/95  19:09    52074
  SB16D2.SYS    SB16D2.SY_      7    11/29/95  10:34    62378
  SBAWED2.SYS   SBAWED2.SY_     7    11/27/95  10:18    88490
  SSM.DLL       SSM.DL_         6    11/27/95  18:13     1044
  SSMDD.SYS     SSMDD.SY_       7    11/27/95  18:15    33272
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
  
                   FixPak Corrective Service levels and disk layouts  24

 
                  December 15, 1995 Warp FixPak XR_W016
 
  SPACE UTILIZATION
 
  The FixPak install process needs to write some files to your C: drive
  even if C: is not where you boot Warp from. These files will be
  deleted when service is complete.
 
                      Min   Max
                      ---   ---
     PACK.EXE         60k   60k
     IBMCSFLK.EXE     11k   11k
     IBMCSFLK.SYS      4k    4k
     IBMCSFLK.DLL     33k   33k
     IBMCSFLK.MSG      1k    1k
     FIXSTART          2k   15k
     CSF_SEL.000       1k    2k
     --------------------------
     Totals          112k  126k
 
 
  Additionally, the following file will be on your boot drive:
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
  
                                                   Space Utilization  25

 
                  December 15, 1995 Warp FixPak XR_W016
 
  In the \OS2\DLL directory:
 
                      Min   Max
                      ---   ---
     IBMCSFLK.DLL     33k   33k
     --------------------------
     Totals           33k   33k
 
  In the \OS2\INSTALL directory:
 
                      Min   Max
                      ---   ---
     SERVICE.LOG      10k   60K
     IBMCSFLK.EXE     11k   11k
     IBMCSFLK.SYS      4k    4k
     IBMCSFLK.DLL     33k   33k
     IBMCSFLK.MSG      1k    1k
     IBMCSFLK.LST      1k   15K
     --------------------------
     Totals           60k  124k
 
  On all drives being serviced in the directory a supported SYSLEVL
  file was found in:
 
                      Min   Max
                      ---   ---
     LOGF0000.OS2     10k   100k
     LOGSTART.OS2     10k   100k
     LOCARCH.OS2       5k    15K
     ---------------------------
     Totals           25k   215k
 
 
  On the drive with the most free space in the \IBMCSFLK\FIX directory
  (and sub-directories) files that had service deferred because they
  were locked (in use) are placed in unpacked format. The amount of
  space this requires varies but can be between 1 and 12MB. These files
  are then moved to the correct directory as part of the Locked File
  process when you reboot, the directory and subdirectories are then
  removed.
 
 
 
 
 
 
 
 
 
 
 
 
  
                                                   Space Utilization  26

