This document contains installation instructions for the Atrex 5 Package:

Installation Instructions:

To install the enclosed copy of Atrex for Windows:
  1. Copy the contents of the distribution file(s) into a single
     directory on your hard drive.  For this example, we will assume
     that you decompressed the files into C:\TEMP.  The complete
     installation package of Atrex consists of INSTALL.EXE, INSTALL.W02,
     INSTALL.W03, & INSTALL.W04.
  2. From the File menu in the Windows Program Manager, select Run.
     (When installing from Windows 95, click on the Start button and
     select the Run command).
  3. In the Command Line field, type C:\TEMP\INSTALL and click OK.
  4. Enter the information as requested to indicate where you wish
     to install Atrex. For most installations, you can simply accept the
     default locations.

*The installation program is capable of modifying your CONFIG.SYS file to
correctly set the maximum number of open files.  If you did not allow the
installation package to automatically make these changes, you must make
the changes manually using an ASCII text editor.  Atrex requires that the
FILES = 75 statement must be present. Refer to your DOS manual for more
information about editing your CONFIG.SYS.

If you are upgrading from a 3.x or 4.x version, please follow the
directions in the manual for converting the data.

To start Atrex, open the Atrex program group in the program manager and
double click on the Atrex icon.  If you are running Windows 95, select
the Atrex icon inside the Atrex group on the start menu.  The on-line
manual for Atrex is a Microsoft Word for Windows document called
ATREX.DOC.  This file can be viewed by most Windows word processors
including the Windows 95 Wordpad.


If you have any questions, or any problems with the installation, please
feel free to contact us at the number below.

Millennium Software, LLC
PO Box 2209
Dublin, CA 94568

Voice: 510-828-5892
Fax: 510-829-1851
BBS: 510-828-4153
Internet: 72560.2466@compuserve.com

