  *************************************************************************
    Copyright (c) Creative Technology Ltd, 1995/1996. All rights reserved.
  *************************************************************************
                                      
                  Video Blaster SE100 for Windows 95
                 -----------------------------------

Overview of the Installation process
====================================
It is recommended that you do not install the hardware into the computer
until you have finished the software installation steps below.

Software Installation Steps:
1.   Insert the installation disk into your floppy drive.
2.   Install the software application package into the system.  See "To
     Install Package" in README.HLP for more instructions.
3.   Next, you will need to install the software drivers.  At the end of the
     installation, a help file (README.HLP) will be launched to guide you
     through this step.
4.   After the drivers have been installed, Windows 95 will assign resources
     for the hardware.  Take note of this resource configuration, and shut
     down the system when prompted.
5.   Set the jumpers on the hardware using the resource settings obtained
     from (4).
6.   Now install the hardware into a free expansion slot in the system.
     (Remember to turn off all power to the computer first!)
7.   Restart the computer.  The installation is complete!
8.   See "To Align Video" in README.HLP to set up video alignment for the
     hardware.  Note that video alignment may differ for different screen
     resolutions.


Troubleshooting Hardware Problems:
==================================
If you encounter hardware problems after installation, please run the Video
Blaster SE100 Diagnose utility which will help pinpoint any hardware fault.

Uninstallating the Software Package:
====================================
Refer to "To Uninstall" in README.HLP which will give you step-by-step
instruction on how to uninstall the software applications and drivers from
the system.

