REM Fighter Duel by Jaeger Software Inc
REM DIGITAL throttle and ANALOG hat switch
REM Set red Base Mode Switch to Digital, black hat switch to Analog

GAME 1 75              REM Type 1 Digital Throttle rate=75
BTN MB /N ENT       	  REM Middle Button
BTN LB /N i            REM Lower Button

THR 33 1 z x b b BSP BSP   REM boost switched on after last stop