The ConnectýFACSys installation routine is designed to operate from
diskette.

This ZIP file contains a disk image of one of the two diskettes that contain
an evaluation version of the FAX server and the DOS-based client utilities.
The Windows client utilities are included in a separate ZIP file.

Insert a blank formatted diskette in one of your available diskette
drives, and type:

MKDISK filename.DSK A:

filename.DSK will be C2FS1.DSK for Diskette #1, and C2FS2.DSK for Diskette #2.

Once you have completed this procedure, insert Diskette #1 into your diskette
drive, make that drive your default drive (e.g., type A:), and then issue
the INSTALL command to execute INSTALL.EXE (INSTALL.EXE is one of the files
that will be in the root directory of Diskette #1).
