IP.TXT
17Nov95

IP.TXT only applies if you have an IP client which uses BOOTP and you have
also installed NWC201.EXE and upgraded your clients after installing
NWC202.EXE.


I. Replace NWCBOOTP.NLM with DHCPD.NLM
======================================
After installing Both NWC201 and NWC202
---------------------------------------
do not load NWCBOOTP.NLM.
Instead, load DHCPD.NLM.

*!IMPORTANT: DHCPD.NLM is ONLY for use with NetWare Connect 2.0.25 or
above.  Do not use the DHCPD.NLM provided in NWC201, with NetWare
MultiProtocol Router, NetWare IP, or LAN Workplace/group!

The upgrade from NWCBOOTP.NLM to DHCPD.NLM should not require any
reconfiguration except for loading DHCPD.NLM instead of NWCBOOTP.NLM.

II. How To Use DHPCD.NLM for BOOTP
----------------------------------
A. During set-up of PPPRNS, complete the following steps to configure an
address range to be used for IP connections through PPPRNS.

A1. Load NWCCON NLM.

A2. From the NetWare Connect Options menu, select "Set Up NetWare Connect".

A3. From the System Setup Options Menu, choose "Select NetWare Connect
Services".

A4. Select PPPRNS from the list of NetWare Connect Services.

A5. Select IP from the List of Protocols for Service window.

A6. In the Local IP Address field, specify a local IP address for the
server.  This is the local IP address for the WAN interface on the NetWare
Connect server.

A7. In the Subnet Mask field, specify a subnet mask address.

A8. To use IP header compression, set the Use Header Compression field to
YES. 
Otherwise, set the field to NO.

A9. Set the "Use Client Address Range" field to YES.

A10. Specify the starting and ending address of the Client Address Range.
The starting and ending address must be in the same network or subnetwork
as the server address specified in the Local Address field.

A11. Press <Esc> and save your changes.

NOTE: The following steps are only required If PPPRNS clients will use
Domain Name Service (DNS) and will obtain DNS information through BOOTP.

A13. From the NWCCON NetWare Connect Options menu, select "Configure
NetWare Connect".

A14. From the Configuration Options menu, select Services.

A15. From the NetWare Connect Services menu, select PPPRNS.

A16. From the PPPRNS Configuration Options menu, select Set IP Parameters.

A17. For each user who will use BOOTP to get Domain Name Server and Domain
Name Server address information, configure IP Parameters.
You can do this for all of the users in a container or for individual
users.  
|    - To select a container or a user, use the "Select User" form to 
|      move up and down the NDS tree.
|    - When the container that you want is displayed, select "." to 
|      choose the container.  To select a specific user, select the 
|      username from the form.
|    - Set the Set Domain Information field  to Yes.
|    - Set the Domain Server Address for the Domain Name Server the 
|      user's will use.
|    - Set the Domain Name for the users.  If you do not know this 
|      name, obtain it from the LAN administrator.

B. After reading the note below, load DHCPD.NLM, by entering the following
at the NetWare console prompt (:) LOAD DHCPD 
 
NOTE: You can use parameters after "LOAD DHCPD" 
<log=yes/no> <file=filename>
If you specify YES for the LOG parameter AND:
- specify a filename, DHCPD activity will be logged to the specified file. 
- do not specify a file name, DHCPD activity will be logged to the console
screen.

<Alt>+<Esc> will toggle between the console screen and the DHCPD log
screen.

NOTE: Also see the DHCPD Client Configuration instructions in NWC202.EXE.
