PDT - Particle displacement tracking software

PDT is an all-electronic Particle Imaging Velocimetry (PIV) data
acquisition and reduction procedure which is simple, fast, and easily
implemented. The procedure uses a low power, continuous wave laser and a
Charged Coupled Device (CCD) camera to electronically record the particle
images. A frame grabber board in a PC is used for data acquisition and
reduction processing. Written in FORTRAN 77 and C-language for IBM PC
compatibles running MS-DOS. 

PROGRAM NUMBER: LEW-14925

DOCUMENTATION: $23.00 PROGRAM: $480.00

NASA's Software Technology Transfer Center
COSMIC, The University of Georgia
382 East Broad St, Athens, GA 30602-4272
(706) 542-3265;  Fax: (706) 542-4807
Internet Email: service@cossack.cosmic.uga.edu
 
 =========================================================
 From the 'New Product News' Electronic News Service on...
 AOL (Keyword = New Products) and Delphi (GO COMP PROD)
 =========================================================
 This information was processed from data provided by the
 company/author mentioned. For additional details, please
 contact them directly at the address/phone# indicated.
 Trademarks are the property of their respective owners!
 =========================================================
 All submissions for this service should be addressed to:
 BAKER ENTERPRISES,  20 Ferro Dr,  Sewell, NJ  08080  USA
 Email:   rbakerpc@aol.com   --or--   rbakerpc@delphi.com
 =========================================================
