*
PRINTER: HP LaserJet Series II
*
*--------------------------------------------------------------------
* The following options are set immediately.  They are not activated
* by parameters.
*--------------------------------------------------------------------
*DOT
LASER                   * LASER PRINTER
TOPMARGIN 0
BOTMARGIN 0
LINELEN 80				* characters per line in normal mode
CLINELEN 132			* characters per line in compressed mode
LINESPAGE 60			* not used for /S processing.  Use /LP:nn MAX 60
*MICSPACE 27 65 9         * SET MICRO SPACING to n 72nds of an inch
*FORMLENL 27 38 108 54 54 80  * set form length in lines  66 = 66 lines
FFEED 12 13                * Form Feed Characters top of page  / Carr return
*--------------------------------------------------------------------
*                         landscape  16.6 pitch   point sz 8.5  Line prnter  lines inch   Help text
CDEF KSL   /lp:71/ll:176   27 .&l1O   27 .(s16.6H  27 .(s8.5V    27 .(s0T     27 .&l5C              * I23  SMALL Landscape  71 lines page 176 line length
CDEF KSP   /lp:95/ll:133   27 .&l0O   27 .(s16.6H  27 .(s8.5V    27 .(s0T     27 .&l5C              * I23  SMALL Portrait   95 lines page 133 line length
CDEF KBP8  /lp:78/ll:80    27 .&l0O   27 .(s10H    27 .(s12V     27 .(s3T     27 .&l8D   27 .(s3B   * I23  Courier BOLD 8lpi (portrait)
CDEF KBL8  /lp:58/ll:100   27 .&l1O   27 .(s10H    27 .(s12V     27 .(s3T     27 .&l8D   27 .(s3B   * I23  Courier BOLD 8lpi (landscape)
CDEF KCP8  /lp:78/ll:80    27 .&l0O   27 .(s10H    27 .(s12V     27 .(s3T     27 .&l8D              * I23  Courier normal 8lpi (portrait)
CDEF KCL8  /lp:58/ll:100   27 .&l1O   27 .(s10H    27 .(s12V     27 .(s3T     27 .&l8D              * I23  Courier normal 8lpi (landscape)
CDEF KBP6  /lp:58/ll:80    27 .&l0O   27 .(s10H    27 .(s12V     27 .(s3T     27 .&l6D   27 .(s3B   * I23  Courier BOLD 6lpi (portrait)
CDEF KBL6  /lp:43/ll:100   27 .&l1O   27 .(s10H    27 .(s12V     27 .(s3T     27 .&l6D   27 .(s3B   * I23  Courier BOLD 6lpi (landscape)
CDEF KCP6  /lp:58/ll:80    27 .&l0O   27 .(s10H    27 .(s12V     27 .(s3T     27 .&l6D              * I23  Courier normal 6lpi (portrait)
CDEF KCL6  /lp:43/ll:100   27 .&l1O   27 .(s10H    27 .(s12V     27 .(s3T     27 .&l6D              * I23  Courier normal 6lpi (landscape)
CDEF -KSL 27 69
CDEF -KSP 27 69
CDEF -KBP8 27 69
CDEF -KBL8 27 69
CDEF -KCP8 27 69
CDEF -KCL8 27 69
CDEF -KBP6 27 69
CDEF -KBL6 27 69
CDEF -KCP6 27 69
CDEF -KCL6 27 69
*--------------------------------------------------------------------
* The following parameters are activated by parameters
*--------------------------------------------------------------------
EMPH 27 40 115 51 66
EMPHOFF 27 40 115 48 66
PERFSKIP  27 38 108 49 76 * set number lines to skip over perfs (4)
PERFSKIPOFF 27 38 108 48 76
8LPI 27 38 108 56 68
6LPI 27 38 108 54 68
COMPON 27 40 115 49 54 46 54 72     * 16.66 CPI
COMPOFF 27 40 115 49 48 72        * 10 CPI
*12CPI 27 40 115 49 50 72         * 12 characters per inch
*12CPIOFF 27 40 115 49 48 72      * 10 CPI
*
* FUTURES ------------------------------------------------------
*
PROPORTIONAL 27 40 115 49 80
PROPORTIONALOFF 27 40 115 48 80   * FIXED SPACING

* ORIENTATION
PORTRAIT 27 38 108 48 79
LANDSCAPE 27 38 108 49 79

* SYMBOL SET
ROMAN8 27 40 56 85
USASCII 27 40 48 85
ROMANX 27 40 48 69
LEGAL 27 40 49 85
LINEDRAW 27 40 48 66
PIFONT 27 40 49 53 85
PIFONTA 27 40 50 81

* POINT SIZE
POINT7  27 40 115 55 86
POINT8  27 40 115 56 86
POINT85 27 40 115 55 46 53 86
POINT10 27 40 115 49 48 86
POINT12 27 40 115 49 50 86
POINT14 27 40 115 49 52 46 52 86

* TYPEFACE
COURIER 27 40 115 51 84
LINEPRINTER 27 40 115 48 84
HELV 27 40 115 52 84
TIMESROMAN 27 40 115 53 84
PRESTIGEELITE 27 40 115 56 84
GOTHIC 27 40 115 54 84

* laser codes for 2 up printing
*       "\033E\033&l1O\033(s17H\033&l5.14C\033&l70F\033&l7E" init laserjet for landscape printing
LASERLANDI 27 69 27 38 108 49 79 27 40 115 49 55 72 27 38 108 53 46 49 52 67 27 38 108 55 48 70 27 38 108 55 69

*       "\033&a0r85m5L\015"
LASERLEFT  27 38 97 48 114 56 53 109 53 76 13         * laserjet to left half

*       "\033&a0r171m91L\015"
LASERRIGHT 27 38 97 48 114 49 55 49 109 57 49 76 13   * laserjet to right half

*       "\015\033E"
LASERCLEAR 13 27 69            * clear laserjet

*       "\033(s3B"
LASERBOLD 27 40 115 51 66      * set laserjet to bold

*       "\033(s-3B"
LASERNORM 27 40 115 45 51 66   * set laser back from bold to normal print

*       "\033&a0r90m88L\015|"
LASERVERT 27 38 97 48 114 57 48 109 56 56 76 13 124  * draw verticle line
