OSIN5BCD - 5.25" CD-ROM Install for WARP
10/28/94

================================================================
          5.25" CD-ROM INSTALLATION FOR WARP
================================================================

Please Read Entire Document for Full Explanation of Procedures
----------------------------------------------------------------

NOTE: You need two 5.25" diskettes for this procedure.
Label one OS/2 WARP 525 CD DISK 0 and the other OS/2 WARP 525 CD
DISK 1.

NOTE: If using Advanced Install, do NOT choose to format HPFS.

1.  Start the system from DOS.

2.  Insert the 525 CD DISK 1 into Drive A:. From the C:\> prompt,
    type:
            FORMAT A: /U and press Enter

3.  When prompted for the volume label, type:
            DISK 1 and press Enter.

4.  From the C:\> prompt, type pressing Enter after each:
        MD CDINST
        CD CDINST
        MD DISK0
        MD DISK1
        CD DISK1

5.  Insert the 3.5" WARP DISK 1 in Drive B.  Type the following,
    pressing Enter after each:
        COPY B:\*.*
        DEL IBM2*.*
        DEL *02.SYS
        DEL TEDIT.*
        DEL PRINT01.SYS
        DEL HPFS.IFS

6.  Insert the 3.5" WARP Install diskette in drive B: and type:
      COPY B:\LMS205.ADD and press Enter.

7.  Using an editor, edit C:\CDINST\DISK1\CONFIG.SYS
    Put REM before the each of following lines:
        IFS=HPFS.IFS /C:64
        BASEDEV=PRINT01.SYS
        BASEDEV=IBM2FLPY.ADD
        BASEDEV=IBM2ADSK.ADD
        BASEDEV=IBM2SCSI.ADD

8.  Below the line BASEDEV=LMS206.ADD, add the line:
        BASEDEV=LMS205.ADD

9.  Save the file and exit the editor.

10. Copy the entire directory to the 525 CD DISK 1 in the A:
    drive.
        COPY *.* A:\ and press Enter.

11. Insert the 525 CD DISK 0 in Drive A: and from the C:\>
    prompt, type:
        FORMAT A: /U and press Enter.

12. When prompted for the volume label, type:
        DISK 0 and press Enter.

13. Type the following, pressing Enter after each.
        CD..
        CD DISK0
        COPY B:\*.*
        DEL BUNDLE

14. Type:
        DEBUG and press Enter.

15. From the - prompt, type the following, pressing Enter after
    each:

        L DS:0 1 0 1
        E 13 60
        E 14 09
        E 15 F9
        E 16 07
        E 18 0F
        W DS:0 0 0 1
        Q

        COPY *.* A:\

16. Remove the WARP Installation diskette from drive B: and
    restart the system to begin the install.

17. Insert OS/2 WARP 525 CD DISK 1 when prompted to insert DISK
    1 and follow the prompts.

Select Easy or Advanced Installation.

