OSIN5BDS - 5.25" DISKETTE INSTALLATION FOR WARP
10/28/94

================================================================
      5.25" DISKETTE INSTALLATION FOR WARP
================================================================

Please Read Entire Document for Full Explanation of Procedures
----------------------------------------------------------------

The following procedures are for a system with 5.25" 1.2MB A:
Drive and 3.5" 1.44MB B: Drive.


NOTE: You need two 5.25" diskettes for this procedure.
Label one OS/2 WARP 525 DISK 0 and the other OS/2 WARP 525
DISK 1.

1.  Start the system from DOS.

2.  Insert the 525 DISK 1 into Drive A:. From the C:\> prompt,
    type:
            FORMAT A: /U and press Enter

3.  When prompted for the volume label, type:
            DISK 1 and press Enter.

4.  From the C:\> prompt, type the following, pressing Enter
    after each.
            MD CDINST
            CD CDINST
            MD DISK0
            MD DISK1
            CD DISK1

5.  Insert the 3.5" WARP Diskette 1 in Drive B.  Type the
    following, pressing Enter after each.
           COPY B:\*.*
           DEL BUNDLE
           COPY *.* A:\

6.  Insert the 3.5" WARP Install diskette in Drive B:

7.  Insert the 525 DISK 0 in Drive A: and type:
           FORMAT A: /U and press Enter.

8.  When prompted for the volume label, type:
           DISK 0 and press Enter.

9.  Type the following, pressing Enter after each:
           CD..
           CD DISK0
           COPY B:\*.*
           DEL BUNDLE

10. Type:
          DEBUG and press Enter.

11. From the - prompt, type the following, pressing Enter after
    each.
           L DS:0 1 0 1
           E 13 60
           E 14 09
           E 15 F9
           E 16 07
           E 18 0F
           W DS:0 0 0 1
           Q

           COPY *.* A:\

12. Remove the WARP Installation diskette from B: and restart the
    system to begin the install.

13. Insert OS/2 WARP 525 DISK 1 when prompted to insert DISK
    1 and follow the prompts.

