APAR= PJ15346
 WORD PERFECT OFFICE 820E ERROR MESSAGE AFTER INSTALLING FIXPACK
 38 OR FIXPACK 39.

APAR= PJ15661
 COUNTRY.SYS ERROR OCCURS WHEN BOOTING WITH PROMISE IDE
 CACHING CONTROLLER USING THE IBM1S506.ADD DRIVER.

APAR= PJ15828
 CHKDSK WARP 3.0
 CHKDSK TRAPS THE SYSTEM ON A PARTITION THAT IS 128 OR 512 MEG

APAR= PJ15841
 BUSLOGIC PCI SCSI DRIVER HANGS WARP INSTALL FROM CDROM, BT-946C

APAR= PJ15906
 CUSTOMER IS UNABLE TO ACCESS PCMCIA MODEM ON AN IBM THINKPAD 720
 (THE MODE COMMAND RETURNS AN ERROR).

APAR= PJ15926
 DUMP TO HARDFILE IN A SYSTEM WITH 64 MB OF RAM OR MORE CORRUPTS
 THE HARDFILE PARTITIONS.

APAR= PJ15963
 WHEN "CLOSE WINDOW ON EXIT" IS UNSELECTED ON A DOS WINDOWED
 SESSION UNDER WARP THE SESSION CLOSES WHEN IT SHOULD NOT

APAR= PJ15995
 SELECTIVE INSTALL IN WARP RESULT IN SYS3175 IN
 OS2MM.DLL 0001:0002930C ** EIP MUST END IN 930C **

APAR= PJ16049
 TRAP E WHEN RUNNING DATAGLANCE V 1.21 ON OS/2 WARP
 PJ16355 DUP OF THIS APAR

APAR= PJ16058
 SONY 55E AND 55D, MITSUMI FX001DE CDROM'S DO NOT WORK IN WARP.

APAR= PJ16074
 AHA164X.ADD DRIVER FOR THE ADAPTEC 1640 SCSI CARD FAILS TO
 LOAD AND THE CDROM DRIVE ATTACHED IS NOT SEEN.

APAR= PJ16085
 UNZIP PROBLEM INSTALLING "INTERNET CONNECTION FOR OS/2"
 PORTION OF THE WARP BONUSPACK FROM CDROM ON MITSUMI DRIVES.

APAR= PJ16077
 SYSTEM HANGS ON WARP DISK1 WITH A BLANK SCREEN, CURSOR BLINKING
 IN TOP LEFT. IBMKBD.SYS BROKEN/REGRESSED.

APAR= PJ16094
 WORD PERFECT OFFICE/NOVELL GROUPWISE 820E FILE I/O ERROR.

APAR= PJ16105
 TRAP 003 IN MACHINES WITH IDE CDROM WITH HEAVY SWAPPING
 UNDER WARP OS/2 VERSION 3.0

APAR= PJ16116
 ICONS OF SEAMLESS WINAPS (LOCALLY) ARE NOT CROSS HATCHING
 WHEN THEY ARE RUN FOR THE 1ST TIME.

APAR= PJ16121
 WARP AHA152X.ADD NOT WORKING WITH SOME CDROM'S.

APAR= PJ16123
 "FLOAT TO TOP" OPTION STILL CAUSING TRAPS IN SYSTEM EDITOR WHEN
 SAVING FILES WITH NO EA'S

APAR= PJ16125
 WARP CDROM DRIVER SBCD2.ADD DOES NOT WORK WITH REVEAL CDROM.

APAR= PJ16129
 IN A SEAMLESS SESSION AFTER INTIAL SOUND HAS BEEN PRODUCED NO
 OTHER WAVE FILE CAN BE PLAYED.
 CLOSED DUP OF PJ16116

APAR= PJ16148
 UNDER WARP, DOSQUERYCURRENTDIR AND OTHER APIS NEEDLESSLY RETURN
 ERROR_INVALID_PARAMETER

APAR= PJ16151
 IBM2SCSI WON'T ALLOW BOOT PARTITIONS > 4 GIGS OR BEYOND 4 GIGS
 IF THE PARTITIONS ARE SMALL UNDER OS2 3.0, 2.11 ABD BELOW

APAR= PJ16152
 AFTER AN APPARENTLY SUCCCESSFUL INSTALL, MACHINE BOOTS UP
 TO "RUN WORKPLACE ERROR MESS. IN PMSHELL.EXE. DEFECT 105124.

APAR= PJ16160
 COMMUNICATION PROGRAMS ARE NOT WORKING IN WIN-OS2 SESSIONS IF
 WARP WAS INSTALLED OVER A WINDOWS 3.11 (OR WORKGROUPS) SYSTEM.

APAR= PJ16162
 TRAP 0160:FFF869A7 REV 8.162

APAR= PJ16163
 THINKPADS 755C WITH THE CRYSTAL SEMI SOUND CHIP, ADJUST SOUND
 WITH  ALT+F5  AND  ALT+F6  THE SETTING IS NOT SAVED.

APAR= PJ16168
 TRAP 000D,EIP=000017EB,CSLIM=2E4B TRAP IS IN COM.SYS AND USUALLY
 OCCURS WHEN TERMINATING APPLICATIONS.  SAME PROBLEM AS PJ14545

APAR= PJ16170
 POCKET RECORDER RECEIVES A GPF INMODULE USER.EXE AT 0001:3ACA.

APAR= PJ16211
 CTRL+ALT+DEL DOES NOT REBOOT SYSTEM AFTER SHUTDOWN. MUST POWER O
 FF SYSTEM

APAR= PJ16217
 STATIC NOISE WITH MEDIA VISION PRO AUDIO SPECTRUM 16 OR
 PRO AUDIO STUDIO UNDER OS/2 WARP MMPM/2.

APAR= PJ16231
 WARP FAILS TO INSTALL ON HARD DRIVES CONNECTED TO ADAPTEC 2940
 SCSI CARD.   AIC7870.ADD

APAR= PJ16234
 TRAPS AT 0160 FFF5DB60 OR FFF5DB6C DURING ARCHIVING REV 8.162
 _PACKGEA + 1

APAR= PJ16246
 1.44MB DISKETTE WILL BE FORMATTED  AS 2.88MB WITH IBM1FLPY.ADD
 DRIVER.  THIS COULD CAUSE DATA LOSS.

APAR= PJ16249
 PENTIUM SYSTEMS RUNNING WITH THE MACH32 VIDEO DEVICE DRIVERS
 HANG WHEN START WINOS/2 FULLSCREENS AND WINDOWS

APAR= PJ16252
 IMAGE INVERTED WHEN PRINTING (TIF) BITMAP  FROM LOTUS AMIPRO 3.0
 WITH OS/2 WARP

APAR= PJ16278
 INTERNET DIALER WHEN DOWNLOADING FROM ADVANTIS WILL NOT WORK.
 CUSTOMERS EXPERIENCE TIME OUTS, SLOW RESPONSE AND OTHER FAILURES

APAR= PJ16282
 DATA CORRUPTION DURING I/O ON HARD DRIVE CONNECTED TO PCI IDE
 PORT.

APAR= PJ16298
 WARP SEAMLESS ICONS STAY CROSSHATCHED AFTER APP CLOSED

APAR= PJ16336
 CHKDSK GENERATES AN ACCESS VIOLATION AT 00004825

APAR= PJ16352
 EXITING PRESTIGE 2.1 PROMPTS AN ERROR MESSAGE, SQLRUN41
 CAUSED A GENERAL PROTECTION FAULT IN MODULE USER AT 0001:7EE0.
 PJ16482 DUP OF THIS APAR

APAR= PJ16358
 IPE AT 0160:FFF65576 - 000D:0001357B 2144, 4023 REVISION 8.162

APAR= PJ16359
 WARP WILL NOT FORMAT A 1.44 MEG DISKETTE WHICH IS UNFORMATTED.

APAR= PJ16402
 CUSTOMER RECEIVING PRINTER OFFLINE MESSAGE AFTER INSTALLING WARP

APAR= PJ16477
 WARP SONY31A.ADD CDROM DRIVER DOES NOT ALLOW IO PORT ADDRESSES
 GREATER THAN 3FF.

APAR= PJ16699
 INTERNEL PROCESSING ERROR  ( IPE )  @ LINE 826 IN VMALLOC.C
 VMASSERT(!VMRELOADREQ(F1))

APAR= PJ16715
 SYS3175 IN PMMERGE USING SYTOS TAPE BACKUP WITH WARP
 AT 1BD30ED2

APAR= PJ16749
 CAN'T USE ALL 3 PCMCIA ADAPTERS ON THINKPAD 755C IN A DOCK II
 DOCKING STATION.
 PJ16200 DUP OF THIS APAR

APAR= PJ16901
 IDE DRIVES >540MB THAT HAVE ONTRACK DISKMANAGER INSTALLED
 CANNOT BE READ.

APAR= PJ16973
 HPFS FILE CORRUPTION UNDER WARP FOR WINDOWS IN OPEN FILE WHEN
 NO SHUTDOWN OF THE SYSTEM IS PREFORMED.
 PJ16993 DUP OF THIS APAR

APAR= PJ17331
 USING TWO IDE CDROM DRIVES ON A SINGLE CHANNEL CAUSE TRAP

APAR= PJ17332
 SLAVE ONLY CONFIGURATIONS FOR ATAPI CDROMS

APAR= PJ17396
 NMIS CAUSE TRAPS AT 0160:C3C9C033 OR IN TRAP$VMPFAULTENTRY OR
 TRAP$V86FAULTENTRY
