XF ree86 $N @_ Dj $K $D $$ $F CJ 3, E* %, %$ %I Copyrigh t c David W exelblat $H XF ree86 %W %m %8 %’ %/ %H <R F| K\ 8l Lu 2, K\ !! 0l 9, Kazuyuki Ok amoto < ikko-@paci�c.rim.or.jp > $3 $N J8 =q $O XFree86 %5 !< %P !< $r $I $& $d $C $F @_ Dj $9 $k $+ $K $D $$ $F $H !" XF86Config %U %! %$ %k $r 5! 4o 9= @. $K 0l CW $5 $; $k ;v $K $D $$ $F =q $$ $F $$ $^ $9 !# $3 $N J8 =q $N <j =g $I $* $j $K :n 6H $9 $l $P !" Ld Bj L5 $/ %5 !< %P !< $, =‘ Hw $G $- !" $9 $0 $K <B 9T $G $- $k $h $& $K $J $j $^ $9 !# $3 $N J8 =q $O HF MQ $K $J $k $h $& $K @_ 7W $5 $l $F $$ $^ $9 !# @_ Dj BP >] OS 8G M- $N README %U %! %$ %k !J Nc $( $P !" README.SVR4 !K $H !" @_ Dj BP >] %S %G %* %+ !< %I / %A %C %W %; %C %H 8G M- $N README %U %! %$ %k !J Nc $( $P !" README.trident !K $r I, $: ;2 >H $7 $F 2< $5 $$ !# $3 $l $i 8G M- $N %U %! %$ %k $H HF MQ $K $J $C $F $$ $k %U %! %$ %k $H $G L7 =b $r @8 $8 $k >l 9g $O !J A4 It $N >l 9g $, $= $& $G $" $k $H $O 8B $j $^ $; $s $, !K !" 8G M- $N %U %! %$ %k $N <j =g $K => $C $F 2< $5 $$ !#

L\ <! 1 L\ <! 1 <j =g 35 MW 2 2 @5 $7 $$ I8 =‘ %5 !< %P !< $N @_ Dj 2 3 XF86Con�g $N 0W $7 $$ It J, 3 4 %S %G %* %\ !< %I $N @_ Dj $K $D $$ $F 4 5 %b %K %? !< $H $= $N %b !< %I $N @_ Dj $K $D $$ $F 5 6 %S %G %* %\ !< %I $H %b %K %? !< %G !< %? $N AH $_ 9g $o $; $K $D $$ $F 6 7 HF MQ %S %G %* %b !< %I $K $D $$ $F 7

1. <j =g 35 MW 2 1 <j =g 35 MW =‘ Hw $H <B 9T $O #2 $D $N CJ 3, $G 9T $J $$ $^ $9 !# $^ $: :G =i $K !" ;H MQ $7 $? $$ E, @Z $J %5 !< %P !< $r A* Br $7 $F !" =i 4| CM $N $^ $^ @_ Dj $7 $^ $9 !# <! $K !" XF86Config %U %! %$ %k $r @_ Dj $7 $^ $9 !# $3 $N %U %! %$ %k $O %5 !< %P !< $K !" 2h LL ;X <( Au CV !J Nc $( $P !" %^ %& %9 $d %H %i %C %/ %\ !< %k !K !" %S %G %* %+ !< %I $d %b %K %? !< Ey !" $= $N B> >/ $7 $N 5! 4o $K $D $$ $F @_ Dj $9 $k $b $N $G $9 !# XF86Config %U %! %$ %k $O $$ $/ $D $+ $N 9‘ L\ $G 9= @. $5 $l $F $$ $^ $9 !# $3 $l $i $N <j B3 $- $O $= $l $> $l $N It J, $r =q $- 9~ $‘ $3 $H $G !" <+ A3 $K F3 $$ $F $/ $l $k $G $7 $g $& !# /usr/X11R6/lib/X11/XF86Con�g.sample $H $$ $& !" =i 4| CM $N %5 %s %W %k $H $7 $F XF86Config %U %! %$ %k $, $" $j $^ $9 !# $3 $N %U %! %$ %k $r /usr/X11R6/lib/X11/XF86Config.sample $K %3 %T !< $7 $F @_ Dj BP >] 5! 4o 9= @. $K 8G M- $J It J, $r =$ @5 $7 $F 2< $5 $$ !# XF86Con�g !J 4 >O / 5 >O !K $N %* %s %i %$ %s %^ %K %e %" %k $K XF86Config %U %! %$ %k $N Cf ?H $H %* %W %7 %g %s $N >\ :Y $, =q $+ $l $F $^ $9 !# $* <j 85 $N XF86Config %U %! %$ %k $r =q $- 9~ $‘ $? $a $K !" %* %s %i %$ %s %^ %K %e %" %k $r DL FI $7 $F 2< $5 $$ !# XF86Config %U %! %$ %k $N 3F @a $O <! $N DL $j $G $9 !# : Files I8 =‘ %U %) %s %H $H RGB %G !< %? %Y !< %9 $N %Q %9 $r @_ Dj $7 $^ $9 !# Server Flags 0l HL E* $J %5 !< %P !< $N >/ NL $N %* %W %7 %g %s $r @_ Dj $7 $^ $9 !# $3 $l $i $K $D $$ $F JY 6/ $7 $? $$ >l 9g $O !" %* %s %i %$ %s %^ %K %e %" %k $r ;2 >H $7 $F 2< $5 $$ !# Keyb oard %- !< %\ !< %I Au CV $r @_ Dj $7 $^ $9 !# >/ NL $N %* %W %7 %g %s %Q %i %a !< %? $r @_ Dj $7 $^ $9 !# Poin ter 2h LL ;X <( Au CV $r @_ Dj $7 $^ $9 !# >/ NL $N %* %W %7 %g %s %Q %i %a !< %? $r @_ Dj $7 $^ $9 !# Monitor %5 !< %P !< $K BP $7 $F %b %K %? !< !J J# ?t !K $r 5- =R $7 $^ $9 !# Graphics Device %5 !< %P !< $K BP $7 $F %S %G %* %+ !< %I $r 5- =R $7 $^ $9 !# Screen. %b %K %? !< $H %S %G %* %+ !< %I $I $N $h $& $K ;H MQ $9 $k $Y $- $+ 5- =R $7 $^ $9 !# 2 @5 $7 $$ I8 =‘ %5 !< %P !< $N @_ Dj I8 =‘ %5 !< %P !< $N L> A0 $O /usr/X11R6/bin/X $G $9 !# $3 $l $O /usr/X11R6/bin/ $K $" $k FC Dj $N %5 !< %P !< $N %P %$ %J %j %U %! %$ %k $G $" $k XF86 xxxx %j %s %/ %U %! %$ %k $G $9 !# X $, ;H $$ $? $$ %5 !< %P !< $N %j %s %/ %U %! %$ %k $K $J $C $F $$ $k $+ 3N G’ $7 $F 2< $5 $$ !# @5 $7 $$ %j %s %/ %U %! %$ %k $K $J $C $F $$ $J $$ $H $- $O !" X $r :o =| $7 $F @5 $7 $$ %5 !< %P !< $N ?7 $7 $$ %j %s %/ %U %! %$ %k $r :n $C $F 2< $5 $$ !# %5 !< %P !< $N %P %$ %J %j %U %! %$ %k $O <! $N DL $j $G $9 !# : XF86 SVGA: Sup er-VGA %5 !< %P !< !# Cirrus 542 f 0,2,4,6,8,9 g !" 543 f 0,4 g $H W estern Digital 90C3 f 1,3 g $H Oak T ec hnologies Inc. OTI087 $N %A %C %W %; %C %H BP 1~ $N %" %/ %; %i %l !< %? $H ;D $j $N %A %C %W %; %C %H BP 1~ $N Hs %" %/ %; %i %l !< %? $r 4^ $s $G $$ $^ $9 !#

3. XF86CONFIG $N 0W $7 $$ It J, 3 XF86 Mono: %* %W %7 %g %s $G Hercules $^ $? $O B> $N Gr 9u %S %G %* %+ !< %I $r %5 %] !< %H $9 $k (S)VGA Gr 9u %5 !< %P !< $, F~ $C $F $$ $^ $9 !# XF86 VGA16: HF MQ VGA 16 ?’ %5 !< %P !< !# XF86 S3: S3 %" %/ %; %i %l !< %? %5 !< %P !< !# XF86 Mach32: A TI Mach32 %" %/ %; %i %l !< %? %5 !< %P !< !# XF86 Mach64: A TI Mach64 %" %/ %; %i %l !< %? %5 !< %P !< !# XF86 Mach8: A TI Mach8 %" %/ %; %i %l !< %? %5 !< %P !< !# XF86 8514: 8514/A %" %/ %; %i %l !< %? %5 !< %P !< !# XF86 P9000: P9000 %" %/ %; %i %l !< %? %5 !< %P !< !# XF86 AGX: AGX %" %/ %; %i %l !< %? %5 !< %P !< !# XF86 W32: ET4000/W32 %" %/ %; %i %l !< %? %5 !< %P !< !# $= $l $> $l $N %5 !< %P !< BP 1~ $N %* %s %i %$ %s %^ %K %e %" %k $, $" $j $^ $9 $N $G !" %5 %] !< %H $7 $F $$ $k %A %C %W %; %C %H 8G M- $N >\ :Y $H %5 !< %P !< 8G M- $N 9= @. $N %* %W %7 %g %s $O %* %s %i %$ %s %^ %K %e %" %k $r ;2 >H $7 $F 2< $5 $$ !# LinkKit $K $F %5 !< %P !< $K %I %i %$ %P !< $r AH $_ 9~ $_ !" JQ 99 $9 $k >l 9g $K Cm 0U ;v 9‘ $, $" $j $^ $9 !# G[ IU J* $, $I $& $f $& Iw $K AH $_ N) $F $i $l $F $$ $k $+ $K $h $j $^ $9 $, !" %5 !< %P !< $N %P %$ %J %j %U %! %$ %k $K $O ;H MQ 2D G= $J A4 $F $N %I %i %$ %P !< $O 4^ $^ $l $F $$ $^ $; $s !# AH $_ 9~ $^ $l $F $$ $k %I %i %$ %P !< $N 0l Mw $r F@ $k $K $O !" /usr/X11R6/bin/X -showconfig $r <B 9T $7 $F 2< $5 $$ !# %5 !< %P !< $r :F %j %s %/ $9 $k I, MW $, $" $k >l 9g $O !" 8G M- $N >p Js $K $D $$ $F LinkKit $N <tt>README.LinkKit</tt> (LinkKit.html) $r ;2 >H $7 $F 2< $5 $$ !# 3 XF86Con�g $N 0W $7 $$ It J, XF86Config %U %! %$ %k $N " Files " $N @a $O !" RGB ( @V NP @D ) $N %G !< %? %Y !< %9 %U %! %$ %k !J 0l HL $K !" $3 $l $r JQ 99 $9 $k $Y $- $G $O $" $j $^ $; $s !K $X $N %Q %9 $H !" I8 =‘ %U %) %s %H $N %Q %9 $r Fb B" $5 $; $k $3 $H $G $9 !# J# ?t $N F on tP ath 9T $r XF86Config $K =q $$ $F $" $k >l 9g $O !" F on tP ath $r 7k 9g $7 $F ;H MQ $G $- $^ $9 !# $= $l $> $l $N F on tP ath $N %G %# %l %/ %H %j $, B8 :_ $9 $k $3 $H $H !" $A $c $s $H %U %) %s %H $, ;H $( $k $3 $H $r 3N G’ $7 $F 2< $5 $$ !# %5 !< %P !< $, " Can’t op en default font ’�xed’ " !J I8 =‘ $N ’ 8G Dj I} ’ %U %) %s %H $, M- $j $^ $; $s !K $H 8@ $C $F $- $? $i !" $= $l $O %U %) %s %H $N EP O? $, @5 $7 $/ $J $$ $+ $i $G $9 !# $= $l $> $l $N %U %) %s %H $N EP O? $r @5 $7 $/ $7 $? $$ $J $i !" $= $l $> $l $N %U %) %s %H

4. %S %G %* %\ !< %I $N @_ Dj $K $D $$ $F 4 $N %G %# %l %/ %H %j $N =j $G ‘mkfontdir’ %3 %^ %s %I $r <B 9T $7 $F $_ $F 2< $5 $$ !# XF86Con�g $N %* %s %i %$ %s %^ %K %e %" %k $N 4 >O / 5 >O $K !" XF86Config %U %! %$ %k $N :G =i $N It J, $N B> $N %Q %i %a %? $K $D $$ $F 5- =R $7 $F $$ $^ $9 !# <! $O " Keyb oard " $N @a $G $9 !# $3 $N @a $K $O !" %- !< %\ !< %I $N DL ?. <j =g !J Xqueue $^ $? $O Normal !K !" %- !< $N 7+ $j JV $7 $N B. EY $d $$ $/ $D $+ $N =$ >~ %- !< $N I8 =‘ E* $J 3d $j IU $1 $K $D $$ $F @_ Dj $G $- $^ $9 !# 0l HL $K $3 $3 $O JQ 99 $9 $k I, MW $O L5 $$ $G $7 $g $& !# 1Q 8l MQ $G $J $$ %- !< %\ !< %I $N %f !< %6 !< $O =$ >~ %- !< $N Dj 5A $r JQ $( $? $$ $3 $H $G $7 $g $& !# >\ :Y $O XF86Con�g $N %* %s %i %$ %s %^ %K %e %" %k $N 4 >O / 5 >O $r 8+ $F 2< $5 $$ !# [ Lu Cm !’ =$ >~ %- !< = B> $N %- !< $H 0l =o $K 2! $9 !" %* %k %? %M %$ %H %- !< (Alt) !" %3 %s %H %m !< %k %- !< (Cntl) $d %7 %U %H %- !< (Shift) Ey 2! $7 $F $b ;z $N =P $J $$ %- !< $N ;v $G $7 $g $& ] <! $O " Poin ter " $N @a $G $9 !# $3 $N @a $G $O 2h LL ;X <( Au CV $N DL ?. <j =g $H Au CV $K $D $$ $F ;X Dj $G $- $^ $9 !# DL ?. <j =g L> >N $O @= B$ <T L> >N $G $O $J $$ $3 $H $K Cm 0U $7 $F 2< $5 $$ !# Nc $( $P !" $$ $/ $D $+ $N Logitech $N %^ %& %9 !J FC $K ?7 $7 $$ $b $N !K $N >l 9g !" Logitech $N DL ?. <j =g L> >N $G $O $J $/ MouseMan $^ $? $O Microsoft $N DL ?. <j =g L> >N $r MQ $$ $^ $9 !# $= $N B> $N %^ %& %9 $N %Q %i %a %? $O $3 $N @a $G !" D4 @0 $G $- $^ $9 !# #2 %\ %? %s %^ %& %9 $r ;H $C $F $$ $k $H $- $O !" Emulate3Buttons $H $$ $& %- !< %o !< %I $r %3 %a %s %H $K $7 $J $$ $G 2< $5 $$ !# Emulate3Buttons %b !< %I $G ;H $& $H $- $O !" F1 ;~ $K #2 $D $N %\ %? %s $r 2! $9 $3 $H $G !" %5 !< %P !< $K ?? $s Cf $N %\ %? %s $r 2! $7 $? $3 $H $r CN $i $; $k $3 $H $K $J $j $^ $9 !# %5 !< %P !< $, %^ %& %9 %G %P %$ %9 $r G’ <1 $7 $J $$ !" $H J8 6g $r 8@ $& $H $- $O $= $l $O %5 !< %P !< $N Ld Bj $G $O $J $$ $3 $H $K Cm 0U $7 $F 2< $5 $$ !# $= $l $O $h $/ 5/ $3 $k @_ Dj %_ %9 $G $" $j !" 99.999% $N 3N N( $G OS $K %G %P %$ %9 $, @5 $7 $/ @_ Dj $5 $l $F $$ $J $$ ;v $, M} M3 $G !" $$ $/ $D $+ $N OS $G $O %( %i !< $H $J $k $G $7 $g $& !# $= $l 8N !" OS %l %Y %k $G $N %5 %] !< %H $, @5 $7 $$ $3 $H $r $h $/ D4 $Y $k $^ $G $O !" 2f !9 $K %P %0 Js 9p $r $7 $J $$ $G 2< $5 $$ !# 4 %S %G %* %\ !< %I $N @_ Dj $K $D $$ $F " Device " $N @a $G $O %S %G %* %\ !< %I $K $D $$ $F 5- =R $7 $^ $9 !# J# ?t $N 5! 4o $N @a $r =q $/ $3 $H $r 5v $7 $F $* $j !" $= $l $> $l $N @a $4 $H $K #1 $D $N %S %G %* %+ !< %I $r 5- =R $7 $^ $9 !# @_ Dj $7 $h $& $H $7 $F $$ $k HF MQ $G $J $$ >p Js $K $D $$ $F !" %5 !< %P !< $N %* %s %i %$ %s %^ %K %e %" %k $H %A %C %W %; %C %H 8G M- $N README %U %! %$ %k $r FI $s $G 3N G’ $7 $F 2< $5 $$ !# Device $N @a $r =q $/ $? $a $K !" @_ Dj BP >] Au CV $N %G !< %? $r =8 $a $k I, MW $, $" $j !" @_ Dj J} ?K $r 7h $a $F 2< $5 $$ !# I, MW $J Au CV $N %G !< %? $O <! $N $H $* $j $G $9 !# : � %A %C %W %; %C %H $N <o JL � I= <( MQ %a %b %j $N NL � ;H MQ 2D G= $J %I %C %H %/ %m %C %/ $N CM !J %W %m %0 %i %‘ 2D G= $J >l 9g !K � Ramdac $N <o JL !J 4v $D $+ $N %5 !< %P !< MQ !K XF86Config %U %! %$ %k $N Cf $G A4 $F ;X Dj $N CM $r Kd $a 9~ $s $G $* $/ $h $j $O !" DL >o !" %5 !< %P !< $K <+ J, <+ ?H $G Au CV $N %G !< %? $r <h $j 9~ $^ $; $? $[ $& $, $$ $$ $G $7 $g $& !# $= $N J} $, 4V 0c $$ $J $/ @_ Dj $G $- $^ $9 !# ’Chipset’ $O @_ Dj $7 $F $$ $k %I %i %$ %P !J ’X -show con�g’ $r <B 9T $9 $l $P I= <( $G $- $^ $9 !K BP 1~ $N %- !< %o !< %I $N #1 $D $G $9 !# %" %/ %; %i %l !< %? %5 !< %P !< $G $O !" 8= :_ !" $$ $/ $D $+ $N %5 !< %P !< $, %A %C %W %; %C %H %I %i %$ %P $r ;} $C $F $$ $^ $9 !# %a %b %j $N NL $O %- %m %P %$ %H C1 0L $G ;X Dj $7 $^ $9 $N $G !" #1 %a %, %P %$ %H $N %a %b %j $N >l 9g $O 1024 $H ;X Dj $7 $^ $9 !# %I %C %H %/ %m %C %/ $O %0 %i %U %# %C %/ %\ !< %I $N @_ Dj $K $* $$ $F 0l HV J# ;( $J It J, $G $9 !# 9, 1? $K $b %I %C %H %/ %m %C %/ $r =8 $a $? Bg $- $J %G !< %? %Y !< %9 $, Mx MQ 2D G= $G $9 !# $$ $/ $D $+ $N %0 %i %U %# %/ %\ !< %I BP 1~ $N Device $N %G !< %? $N 0l Mw $, ‘Devices’ %U %! %$ %k $K $" $j $^ $9 !# $" $J $? $N %0 %i %U %# %C %/ %\ !< %I $, 8+ $D $+ $l $P !" $= $N %G !< %? $+ $i ;O $a $k $3 $H $, =P Mh $^ $9 !# modeDB.txt %U %! %$ %k $N :G =i $N It J, $O L5 ?t $N SVGA %+ !< %I $N >p Js $, 0l Mw $K $J $C $F $$ $^ $9 !# %" %/ %; %i %l !< %? %+ !< %I $G $O !" ‘AccelCards’ %U %! %$ %k $r 8+ $F 2< $5 $$ !# 9, 1? $J $i $P !" <+ J, $N %+ !< %I $, 2? =h $+ $K 8+ $D $+ $k $G $7 $g $& !# $b $7 %+ !< %I $, 8+ $D $+ $C $? $i !" XF86Config %U %! %$ %k $N Clo cks 9T $K %G !< %? %Y !< %9 $+ $i ?t Ns $r !" %G !< %? %Y !< %9 $K I= <( $5 $l $F $$ $k $= $N $^ $^ $r JB $Y BX $( $? $j $7 $J $$ $G ;D $5

5. %b %K %? !< $H $= $N %b !< %I $N @_ Dj $K $D $$ $F 5 $: %3 %T !< $7 $^ $7 $g $& !# ?7 $7 $$ %" %/ %; %i %l !< %? %+ !< %I $O %W %m %0 %i %^ %V %k %/ %m %C %/ %8 %’ %M %l !< %? $r ;H $C $F $$ $k $N $G XF86Config %U %! %$ %k $N Clo ckChip 9T $K 0z MQ Id !J " !K IU $- $G %/ %m %C %/ %8 %’ %M %l !< %? $N 7? <0 $, =q $$ $F $" $k $3 $H $K Cm 0U $7 $F 2< $5 $$ !# !J Nc $( $P !" #9 GXe $r ;H $& $J $i $P !" ‘Clo ckChip " icd2061a " ’ $N MM $K =q $$ $F $" $k $G $7 $g $& !K !# %0 %i %U %# %C %/ %\ !< %I $, 0l Mw $K 8+ $D $+ $i $J $$ $H $- $O !" %5 !< %P !< $K %0 %i %U %# %C %/ %\ !< %I $N 8! =P $r G$ $; $F $7 $^ $$ $^ $7 $g $& !# sh Kt $O ksh $N >l 9g $O !" ‘X -prob eonly > /tmp/out 2 > &1’ !" csh $N >l 9g $O !" ‘X -prob eonly > &/tmp/out’ $H %3 %^ %s %I $r <B 9T $7 $^ $7 $g $& !# $3 $N ;~ !" XF86Config %U %! %$ %k $K Clo c ks 9T $r =q $+ $J $$ $G $* $$ $F 2< $5 $$ !# %3 %^ %s %I $r <B 9T $7 $? $i !" %5 !< %P !< $, AG B. $/ %/ %m %C %/ $r =d 2s $7 $F D4 $Y $k 4V !" ?t IC 4V 2h LL $, 0E $/ $J $j $^ $9 !# D4 $Y $k $3 $H $G %b %K %? !< $r DK $a $k $3 $H $O $" $j $^ $; $s $, !" I= <( ;E MM 0J >e $G 8! :: $r $9 $k >l 9g $, $" $k $? $a !" ?7 $7 $$ %b %K %? !< $N >l 9g $O <+ F0 E* $K $= $l <+ ?H $G %b %K %? !< $N EE 8; $r Mn $H $7 $F $7 $^ $& >l 9g $, $" $j $^ $9 !# $H $K $+ $/ !" D4 :: $, =* $o $C $? $i !" %I %C %H %/ %m %C %/ $N 8! =P 7k 2L $N /tmp/out %U %! %$ %k $r 8+ $^ $7 $g $& !# /tmp/out $N ?t Ns $r $= $N $^ $^ XF86Config %U %! %$ %k $N Clo c ks 9T $K %3 %T !< $7 $^ $7 $g $& !# JB $S JQ $( $? $j !" $$ $+ $J $k JQ 99 $b $7 $F $O $$ $1 $^ $; $s !# %0 %i %U %# %C %/ %\ !< %I $, %W %m %0 %i %^ %V %k %/ %m %C %/ %8 %’ %M %l !< %? $r ;} $C $F $$ $k 2D G= @- $, $" $j $^ $9 !# $3 $N >l 9g $O !" 2 !" 3 8D $N %/ %m %C %/ $@ $1 CM $r ;} $A !" ;D $j $, A4 $F %< %m $K $J $C $F $$ $k $3 $H $G $7 $g $& !# $b $7 !" %\ !< %I $, %G !< %? %Y !< %9 $N Cf $K 8+ Ev $? $i $J $+ $C $? $i !" XF ree86 %A !< %‘ $K O" Mm $r <h $k $+ !" comp.windows.x.i386unix $K %a %C %; !< %8 $r %] %9 %H $7 $F 2< $5 $$ !# KX $I $N >l 9g Diamond <R $N Au CV $, $3 $N <o $N J, N‘ $K $J $j $^ $9 $, !" Diamond <R $O %W %m %0 %i %‘ $N >\ :Y $r 8x 3+ $7 $F $/ $l $^ $; $s $N $G !" 2f !9 $O =u $1 $k $3 $H $, =P Mh $^ $; $s !# %M %C %H %K %e !< %9 $G $O !" NQ M} E* $K Ld Bj $N $" $k 2r 7h :v $, Mx MQ 2D G= $G $9 $, !" 2f !9 $O $3 $N J} K! $r Ds >’ =P Mh $^ $; $s $N $G !" $3 $N J} K! $K $D $$ $F 2f !9 $K O" Mm $7 $J $$ $G 2< $5 $$ !# $$ $/ $D $+ $N %5 !< %P !< (S3 $H AGX) $K $O RAMDA C $N 7? <0 $H B. EY $, !" $= $N B> $N Au CV $N >p Js $r <h $j =P $9 $? $a $K I, MW $K $J $j $^ $9 !# $3 $N ;X Dj $O ’Ramdac’ $H ’DacSp eec’ $H $$ $& 5- :\ $r DI 2C $7 $F 9T $J $$ $^ $9 !# %5 %] !< %H $7 $F $$ $k RAMDA C $N >\ :Y $O !" E, @Z $J %5 !< %P !< $N %* %s %i %$ %s %^ %K %e %" %k $r ;2 >H $7 $F 2< $5 $$ !# 0J A0 $N XF ree86 $N %P !< %8 %g %s $G $O !" RAMD A C $N 7? <0 $O %* %W %7 %g %s %U %i %0 $G @_ Dj $7 $F $$ $? $3 $H $K Cm 0U $7 $F 2< $5 $$ !# <+ J, $N Au CV $K 9g $o $; $F !" $$ $/ $D $+ $N %* %W %7 %g %s %U %i %0 $r ;X Dj $9 $k I, MW $, $" $k $G $7 $g $& !# %5 !< %P !< $N %* %s %i %$ %s %^ %K %e %" %k $K $3 $l $i $N %* %W %7 %g %s $K $D $$ $F 5- =R $, $" $j !" %A %C %W %; %C %H 8G M- $N README %U %! %$ %k $K $* <j 85 $N %\ !< %I $N 0Y $K $J $K $, I, MW $+ =q $$ $F $j $^ $9 !# 5 %b %K %? !< $H $= $N %b !< %I $N @_ Dj $K $D $$ $F %b %K %? !< %b !< %I $N @_ Dj $O !" %b %K %? !< Au CV $N I8 =‘ 2= $, == J, $G $J $$ $N $G !" ;D G0 $J $, $i !" <B 83 $N 7+ $j JV $7 $G 7h Dj $7 $^ $9 !# FC Dj $N %b %K %? !< >p Js $r %G !< %? %Y !< %9 $K <} =8 $9 $k $3 $H $K $h $j !" $3 $N <B 83 :n 6H $r 4J C1 $K $9 $k ;v $H !" KX $I $N %b %K %? !< $K $+ $J $j 0l CW $9 $k 5! G= $r =8 $a !" HF MQ %b !< %I $N AH $_ 9g $o $; $r $^ $H $a $k ;v $r ;n $_ $F $$ $^ $9 !# 7l $N $K $8 $‘ $h $& $J EX NO $G =P Mh $? A4 $F $N %b %K %? !< %b !< %I $N :n @. $H 2~ NI $K $D $$ $F $N >\ :Y $O !" Eric Raymond ;a $, =q $$ $? Vide oMo des.do c (VidModes.html) $r ;2 >H $7 $F 2< $5 $$ !# XF86Config %U %! %$ %k $N " Monitor " @a $K %b %K %? !< $N ;E MM $H %S %G %* $N %b !< %I $r 5- =R $7 $^ $9 !# Monitor $N @a $r =q $/ $? $a $K !" <+ J, $N %b %K %? !< $N ;E MM $r CN $k I, MW $, $" $j $^ $9 !# FC $K !" %b %K %? !< $N %5 %] !< %H $7 $F $$ $k ?e J? F1 4| ?. 9f $H ?b D> %j %U %l %C %7 %e ?. 9f $N B. EY $H %S %G %* ?. 9f $N BS 0h $K $D $$ $F CN $k I, MW $, $" $j $^ $9 !# $3 $N >p Js $O %b %K %? !< $N %f !< %6 !< %^ %K %e %" %k $K =q $$ $F $" $k $G $7 $g $& !# $^ $? !" <+ J, $N %b %K %? !< $N 5- :\ $, $" $k $+ $b $7 $l $J $$ $N $G ’Monitors’ %U %! %$ %k $r 8+ $F !" 3N G’ $7 $F 2< $5 $$ !# Moniter $N @a $K $3 $N >p Js $r $I $& $d $C $F EP O? $9 $k $+ $N >\ :Y $O XF86Con�g $N %* %s %i %$ %s %^ %K %e %" %k $N 4 >O / 5 >O $r 8+ $F 2< $5 $$ !# <! $K !" %b %K %? !< $K 9g $o $; $? %S %G %* $N %b !< %I $N AH $r M? $( $k I, MW $, $" $j $^ $9 !# $^ $: :G =i $K ’Monitors’ $H modeDB.txt %U %! %$ %k $N Cf $K <+ J, $N ;X Dj $9 $k %b %K %? !< $K BP 1~ $9 $k %b !< %I $, 0l Mw $K $" $k $+ 3N G’ $7 $F 2< $5 $$ !# $" $C $? >l 9g $O !" XF86Config %U %! %$ %k $N Mo deDB $N @a $K $= $l $i $N %b !< %I $r %3 %T !< $7 $F 2< $5 $$ !# XF86Config %U %! %$ %k $N Clo cks 9T $K $" $k %/ %m %C %/ $H !" 3F %b !< %I $N 9T $N #2 HV L\ $N %Q %i %a !< %? $N %I %C %H %/

6. %S %G %* %\ !< %I $H %b %K %? !< %G !< %? $N AH $_ 9g $o $; $K $D $$ $F 6 %m %C %/ $, 0l CW $7 $F $$ $k $+ 3N G’ $7 $F !" <+ J, $N %+ !< %I $N %/ %m %C %/ $H 0l CW $7 $J $$ %b !< %I $N 9T $O >C $7 $F 2< $5 $$ !# $= $7 $F %b !< %I $, ;D $C $? ;~ $O !" NI $$ >u BV $K $J $j $^ $9 !# FC Dj $N %b !< %I $, 8+ $D $+ $i $J $$ $+ !" $b $C $H ;H $$ $? $$ 2r A| EY $N %b !< %I $, CN $j $? $$ $H $- $O !" 8e =R $9 $k HF MQ %S %G %* %b !< %I $N 0l Mw $r ;2 >H $7 $F 2< $5 $$ !# %b %K %? !< $N ;E MM $K BP $7 $F @_ Dj $9 $k %b !< %I $N ;E MM $r 9g $o $; $^ $7 $g $& ; ;E MM Fb $G 0l HV 9b $$ %j %U %l %C %7 %e %b !< %I $r <h $j =P $7 $F !" Clo c ks 9T $N %I %C %H %/ %m %C %/ $K 9g $C $F $$ $k $3 $H $r 3N G’ $7 $F 2< $5 $$ !# 2r A| EY $, 0l CW $9 $k 8r Be (Alternate) %b !< %I $K @Z $j BX $( $k A0 $K VESA %b !< %I $r ;n $7 $F $_ $F 2< $5 $$ !# @_ Dj $r 9g $o $; $? %b !< %I $r XF86Config %U %! %$ %k $N Monitor $N @a $K %3 %T !< $7 $F 2< $5 $$ !# $3 $l $i $N %b !< %I $O :G E, $J CM $G $O $J $$ ;v $K Cm 0U $7 $F 2< $5 $$ !# $3 $l $i $O 40 ‘z $J 2h LL %5 %$ %: $G $O $J $$ $G $7 $g $& $7 !" ?? $s Cf $K I= <( $5 $l $F $O $$ $J $$ $G $7 $g $& !# $7 $+ $7 !" D4 @0 2D G= $G $9 !# @_ Dj BP >] $N %b %K %? !< $K 9g $o $; $F %b !< %I $r Hy D4 @0 $7 $? $$ >l 9g $O !" VideoMo des.do c %U %! %$ %k $N ’ I= <( $N Ld Bj =$ @5 ’ $N @a $r FI $s $G 2< $5 $$ !# Hy D4 @0 $r 9T $J $& $K $" $? $j !" Cm 0U ;v 9‘ $, $" $j $^ $9 !# XF86Config %U %! %$ %k $N Monitor $N @a $K F1 $8 %b !< %I $N L> A0 $, #2 $D 0J >e Dj 5A $5 $l $F $$ $k >l 9g $K !" %5 !< %P !< $O %/ %m %C %/ $N 0l CW $9 $k :G =i $N %b !< %I $r ;H MQ $7 $^ $9 !# 0l HL E* $K !" XF86Config %U %! %$ %k $K F1 $8 %b !< %I $N L> A0 $r #2 $D 0J >e Dj 5A $9 $k $3 $H $O 0- $$ 9M $( $@ $H ;W $$ $^ $9 !# 6 %S %G %* %\ !< %I $H %b %K %? !< %G !< %? $N AH $_ 9g $o $; $K $D $$ $F 0l C6 !" %5 !< %P $, @_ Dj BP >] $N %b %K %? !< $H %0 %i %U %# %C %/ %\ !< %I $r $I $N $h $& $K ;H $& $+ 5- =R $7 $F ;X Dj $9 $k I, MW $, $" $j $^ $9 !# $3 $l $r XF86Config %U %! %$ %k $N " Screen " $N @a $G 9T $J $$ $^ $9 !# ;H MQ $7 $? $$ %5 !< %P !< $N %I %i %$ %P !< $N 7? <0 $N $= $l $> $l $r Screen @a $G M? $( $^ $9 !# %I %i %$ %P !< $N 7? <0 $O " SVGA " $N @a $G $O (XF86 SVGA) !" " V GA16 " $N @a $G $O (XF86 VGA16) !" " VGA2 " $N @a $G $O (XF86 Mono) !" " MONO " $N @a $G $O (XF86 Mono, XF86 VGA16) $H " A CCEL " $N @a $G $O (XF86 S3, XF86 Mach32, XF86 Mach8, XF86 Mach64, XF86 8514, XF86 P9000, XF86 AGX, XF86 W32) $G $9 !# $= $l $> $l $N Screen @a $O ;H MQ $9 $k %b %K %? !< (Monitor) $N 5- =R $H %G %P %$ %9 (Device) $N 5- =R $r ;X Dj $7 $^ $9 !# Screen @a $O #1 $D $^ $? $O J# ?t $N " Display " $N 9‘ $r 4^ $s $G $$ $^ $9 !# #1 $D $N Displa y 9‘ $O %5 !< %P !< $, %5 %] !< %H $7 $F $$ $k $= $l $> $l $N ?< $5 $r M? $( $k $G $7 $g $& !# [ Lu Cm !’ ?< $5 $H $O ?’ ?t $d 3, D4 ?t $r I= $o $9 $N $K I, MW $J %S %C %H ?t $G $9 !# ] Display 9‘ $G $O !" ;H $$ $? $$ %5 !< %P !< $N 2> A[ %9 %/ %j !< %s $N Bg $- $5 $r ;X Dj $G $- $^ $9 !# 2> A[ %9 %/ %j !< %s $O %b %K %? !< $K I= <( $G $- $k %9 %/ %j !< %s $N Bg $- $5 $h $j $b !" Bg $- $$ %k !< %H %& %# %s %I %& ( " ro ot window " ) $r ;} $D $3 $H $, =P Mh $^ $9 !J Nc $( $P 800x600 $N %G %# %9 %W %l %$ $G 1280x1024 $N Bg $- $5 $N 2> A[ %9 %/ %j !< %s $r ;H $( $^ $9 !K !# Virtual $H $$ $& %- !< %o !< %I $r 2> A[ %9 %/ %j !< %s $N Bg $- $5 $r ;X Dj $9 $k $N $K ;H $$ $^ $9 !# B? $/ $N ?7 $7 $$ %" %/ %; %i %l !< %? %5 !< %P $O I= <( $K ;H $o $l $J $$ %a %b %j $r %- %c %C %7 %e $K ;H $& $3 $H $K Cm 0U $7 $F 2< $5 $$ !# %- %c %C %7 %e $O %a %b %j $N A4 $F $r 2> A[ %G %# %9 %W %l %$ $K ;H $& $h $& $J L% NO $O $" $j $^ $; $s $, !" %- %c %C %7 %e $K %a %b %j $r ;D $5 $J $$ $h $& $K $7 $F !" %a %b %j $N A4 $F $r 2> A[ %G %# %9 %W %l %$ $K ;H $& $H %5 !< %P !< $N @- G= $N 30 $+ $i 40% $[ $I $r >C Hq $7 $^ $9 !# :G 8e $K !" Display @a $N @_ Dj $O %G %# %9 %W %l %$ $N %b !< %I @_ Dj $G $9 !# %5 !< %P !< $N ;H MQ $7 $h $& $H $7 $F $$ $k J* M} E* $J %G %# %9 %W %l %$ $N 2r A| EY $N ;X Dj $, $" $j $^ $9 !# $= $N L> A0 $O G$ 0U $G $9 $, !" Monitor @a $K $" $k $I $l $+ $H 0l CW $7 $F $$ $J $1 $l $P $$ $1 $^ $; $s !# 0l HL $K !" $3 $l $i $N L> A0 $O %G %# %9 %W %l %$ $N 2r A| EY !J Nc $( $P " 1024x768 " !K $K $J $C $F $$ $k $G $7 $g $& $, !" $= $N DL $j $G $J $1 $l $P $$ $1 $J $$ Lu $G $O $" $j $^ $; $s !# I, MW $J ?t $@ $1 0l Mw 7A <0 $G ;X Dj $7 $^ $9 !# $^ $: :G =i $N Dj 5A $, I8 =‘ $G 5/ F0 $5 $l $k 2h LL $K $J $j !" 2r A| EY $N 0l Mw $O %3 %s %H %m !< %k %- !< (Ctrl) !" %* %k %? %M %$ %H %- !< (Alt) !" %F %s %- !< $N + $r F1 ;~ $K 2! $9 $+ !" %3 %s %H %m !< %k %- !< (Ctrl) !" %* %k %? %M %$ %H %- !< (Alt) !" %F %s %- !< $N - $r F1 ;~ $K 2! $9 $3 $H $G =d 2s $G $- $k 2h LL $N Dj 5A $K $J $j $^ $9 !# 0J >e $G @_ Dj $O =* $o $j $G $9 !# $5 $" !" ?7 $7 $$ XF ree86 $N F3 F~ %F %9 %H $r $9 $k =‘ Hw $, =P Mh $^ $7 $? !#

7. HF MQ %S %G %* %b !< %I $K $D $$ $F 7 7 HF MQ %S %G %* %b !< %I $K $D $$ $F [ Lu Cm : $3 $3 $O %G !< %? $N :F Mx MQ $N $? $a $K K] Lu $O $7 $^ $; $s !# $? $H $( !" %3 %a %s %H $K $G $b 4A ;z $, :. $8 $C $F 8m F0 :n $r 5/ $3 $9 $3 $H $O L5 $$ $H !" ?. $8 $F $$ $^ $9 $, $A $g $C $H I] $$ :-) ] # # Mode Refresh Hor. Sync Dot-clock Interlaced? VESA? # ------------------------------------------------------------ # 640x480 60Hz 31.5k 25.175M No No # 640x480 60Hz 31.5k 25.175M No No # 640x480 63Hz 32.8k 28.322M No No # 640x480 70Hz 36.5k 31.5M No No # 640x480 72Hz 37.9k 31.5M No Yes # 800x600 56Hz 35.1k 36.0M No Yes # 800x600 56Hz 35.4k 36.0M No No # 800x600 60Hz 37.9k 40.0M No Yes # 800x600 60Hz 37.9k 40.0M No No # 800x600 72Hz 48.0k 50.0M No Yes # 1024x768i 43.5Hz 35.5k 44.9M Yes No # 1024x768 60Hz 48.4k 65.0M No Yes # 1024x768 60Hz 48.4k 62.0M No No # 1024x768 70Hz 56.5k 75.0M No Yes # 1024x768 70Hz 56.25k 72.0M No No # 1024x768 76Hz 62.5k 85.0M No No # 1280x1024i 44Hz 51kHz 80.0M Yes No # 1280x1024i 44Hz 47.6k 75.0M Yes No # 1280x1024 59Hz 63.6k 110.0M No No # 1280x1024 61Hz 64.24k 110.0M No No # 1280x1024 74Hz 78.85k 135.0M No No # # 640x480@60Hz Non-Interlaced mode # Horizontal Sync = 31.5kHz # Timing: H=(0.95us, 3.81us, 1.59us), V=(0.35ms, 0.064ms, 1.02ms) # # name clock horizontal timing vertical timing flags "640x480" 25.175 640 664 760 800 480 491 493 525 # # Alternate 640x480@60Hz Non-Interlaced mode # Horizontal Sync = 31.5kHz # Timing: H=(1.27us, 3.81us, 1.27us) V=(0.32ms, 0.06ms, 1.05ms) # # name clock horizontal timing vertical timing flags "640x480" 25.175 640 672 768 800 480 490 492 525 #

7. HF MQ %S %G %* %b !< %I $K $D $$ $F 8 # 640x480@63Hz Non-Interlaced mode (non-standard) # Horizontal Sync = 32.8kHz # Timing: H=(1.41us, 1.41us, 5.08us) V=(0.24ms, 0.092ms, 0.92ms) # # name clock horizontal timing vertical timing flags "640x480" 28.322 640 680 720 864 480 488 491 521 # # 640x480@70Hz Non-Interlaced mode (non-standard) # Horizontal Sync = 36.5kHz # Timing: H=(1.27us, 1.27us, 4.57us) V=(0.22ms, 0.082ms, 0.82ms) # # name clock horizontal timing vertical timing flags "640x480" 31.5 640 680 720 864 480 488 491 521 # # VESA 640x480@72Hz Non-Interlaced mode # Horizontal Sync = 37.9kHz # Timing: H=(0.76us, 1.27us, 4.06us) V=(0.24ms, 0.079ms, 0.74ms) # # name clock horizontal timing vertical timing flags "640x480" 31.5 640 664 704 832 480 489 492 520 # # VESA 800x600@56Hz Non-Interlaced mode # Horizontal Sync = 35.1kHz # Timing: H=(0.67us, 2.00us, 3.56us) V=(0.03ms, 0.063ms, 0.70ms) # # name clock horizontal timing vertical timing flags "800x600" 36 800 824 896 1024 600 601 603 625 # # Alternate 800x600@56Hz Non-Interlaced mode # Horizontal Sync = 35.4kHz # Timing: H=(0.89us, 4.00us, 1.11us) V=(0.11ms, 0.057ms, 0.79ms) # # name clock horizontal timing vertical timing flags "800x600" 36 800 832 976 1016 600 604 606 634 # # VESA 800x600@60Hz Non-Interlaced mode # Horizontal Sync = 37.9kHz # Timing: H=(1.00us, 3.20us, 2.20us) V=(0.03ms, 0.106ms, 0.61ms) # # name clock horizontal timing vertical timing flags "800x600" 40 800 840 968 1056 600 601 605 628 +hsync +vsync

7. HF MQ %S %G %* %b !< %I $K $D $$ $F 9 # # Alternate 800x600@60Hz Non-Interlaced mode # Horizontal Sync = 37.9kHz # Timing: H=(1.20us, 3.80us, 1.40us) V=(0.13ms, 0.053ms, 0.69ms) # # name clock horizontal timing vertical timing flags "800x600" 40 800 848 1000 1056 600 605 607 633 # # VESA 800x600@72Hz Non-Interlaced mode # Horizontal Sync = 48kHz # Timing: H=(1.12us, 2.40us, 1.28us) V=(0.77ms, 0.13ms, 0.48ms) # # name clock horizontal timing vertical timing flags "800x600" 50 800 856 976 1040 600 637 643 666 +hsync +vsync # # 1024x768@43.5Hz, Interlaced mode (8514/A standard) # Horizontal Sync = 35.5kHz # Timing: H=(0.54us, 1.34us, 1.25us) V=(0.23ms, 0.23ms, 0.93ms) # # name clock horizontal timing vertical timing flags "1024x768i" 44.9 1024 1048 1208 1264 768 776 784 817 Interlace # # VESA 1024x768@60Hz Non-Interlaced mode # Horizontal Sync = 48.4kHz # Timing: H=(0.12us, 2.22us, 2.58us) V=(0.06ms, 0.12ms, 0.60ms) # # name clock horizontal timing vertical timing flags "1024x768" 65 1024 1032 1176 1344 768 771 777 806 -hsync -vsync # # 1024x768@60Hz Non-Interlaced mode (non-standard dot-clock) # Horizontal Sync = 48.4kHz # Timing: H=(0.65us, 2.84us, 0.65us) V=(0.12ms, 0.041ms, 0.66ms) # # name clock horizontal timing vertical timing flags "1024x768" 62 1024 1064 1240 1280 768 774 776 808 # # VESA 1024x768@70Hz Non-Interlaced mode # Horizontal Sync=56.5kHz # Timing: H=(0.32us, 1.81us, 1.92us) V=(0.05ms, 0.14ms, 0.51ms) #

7. HF MQ %S %G %* %b !< %I $K $D $$ $F 10 # name clock horizontal timing vertical timing flags "1024x768" 75 1024 1048 1184 1328 768 771 777 806 -hsync -vsync # # 1024x768@70Hz Non-Interlaced mode (non-standard dot-clock) # Horizontal Sync=56.25kHz # Timing: H=(0.44us, 1.89us, 1.22us) V=(0.036ms, 0.11ms, 0.53ms) # # name clock horizontal timing vertical timing flags "1024x768" 72 1024 1056 1192 1280 768 770 776 806 -hsync -vsync # # 1024x768@76Hz Non-Interlaced mode # Horizontal Sync=62.5kHz # Timing: H=(0.09us, 1.41us, 2.45us) V=(0.09ms, 0.048ms, 0.62ms) # # name clock horizontal timing vertical timing flags "1024x768" 85 1024 1032 1152 1360 768 784 787 823 # # 1280x1024@44Hz, Interlaced mode # Horizontal Sync=51kHz # Timing: H=(0.02us, 2.7us, 0.70us) V=(0.02ms, 0.24ms, 2.51ms) # # name clock horizontal timing vertical timing flags "1280x1024i" 80 1280 1296 1512 1568 1024 1025 1037 1165 Interlace # # Alternate 1280x1024@44Hz, Interlaced mode (non-standard dot-clock) # Horizontal Sync=47.6kHz # Timing: H=(0.42us, 2.88us, 0.64us) V=(0.08ms, 0.12ms, 0.96ms) # # name clock horizontal timing vertical timing flags "1280x1024i" 75 1280 1312 1528 1576 1024 1028 1034 1080 Interlace # # 1280x1024@59Hz Non-Interlaced mode (non-standard) # Horizontal Sync=63.6kHz # Timing: H=(0.36us, 1.45us, 2.25us) V=(0.08ms, 0.11ms, 0.65ms) # # name clock horizontal timing vertical timing flags "1280x1024" 110 1280 1320 1480 1728 1024 1029 1036 1077 # # 1280x1024@61Hz, Non-Interlaced mode # Horizontal Sync=64.25kHz

7. HF MQ %S %G %* %b !< %I $K $D $$ $F 11 # Timing: H=(0.44us, 1.67us, 1.82us) V=(0.02ms, 0.05ms, 0.41ms) # # name clock horizontal timing vertical timing flags "1280x1024" 110 1280 1328 1512 1712 1024 1025 1028 1054 # # 1280x1024@74Hz, Non-Interlaced mode # Horizontal Sync=78.85kHz # Timing: H=(0.24us, 1.07us, 1.90us) V=(0.04ms, 0.04ms, 0.43ms) # # name clock horizontal timing vertical timing flags "1280x1024" 135 1280 1312 1456 1712 1024 1027 1030 1064 $XConsortium: Config.sgml,v 1.3 95/01/23 15:34:40 kaleb Exp $ $XFree86: xc/programs/Xserver/hw/xfree86/doc/sgml/Config.sgml,v 3.6 1995/07/07 15:40:11 dawes Exp $ $3 $N %U %! %$ %k $O xc/programs/Xserver/h w/xfree86/doc/sgml/Con�g.sgml,v 3.6 1995/07/07 15:40:11 $r !" 2, K\ 0l 9, ( Kazuyuki Ok amoto < ikko-@p aci�c.rim.or.jp > (mailto:ikko-@pacific.rim.or.jp) ) $, XF ree86 3.1.2 $r F| K\ $G %$ %s %9 %H !< %k $9 $k ?M 8~ $1 $K OB Lu $7 $? $b $N $G $9 !# $3 $3 $, $* $+ $7 $$ $H $+ !" $3 $3 $O $3 $& $7 $? $[ $& $, $$ $$ $H $$ $C $? $4 0U 8+ $, $" $j $^ $7 $? $i !" EE ;R %a !< %k $G $* CN $i $; 2< $5 $$ !# 86 J8 $N Cx :n 8" $O XF ree86 %W %m %8 %’ %/ %H <R $K $" $j $^ $9 !# $3 $N OB Lu $N Cx :n 8" $O XF ree86 %W %m %8 %’ %/ %H <R $H 2, K\ !! 0l 9, $K $" $j $^ $9 $, !" $3 $N OB Lu $N IT 6q 9g $O ;d $K !" EE ;R %a !< %k $G Aw $C $F 2< $5 $$ !# $XFree86: xc/programs/Xserver/hw/xfree86/doc/sgml/Japanese/Config.sgml,v 3.5 1995/09/16 08:28:55 dawes Exp $ [EOF]