Cirrus %A %C %W %; %C %H %f !< %6 $N $? $a $N >p Js Copyrigh t c Harm Hanemaay er ( hhanemaa@cs.ruu.nl ), Randy Hendry ( r andy@sgi.c om ) F| K\ 8l Lu 2, K\ !! 0l 9, Kazuyuki Ok amoto < ikko-@paci�c.rim.or.jp >

L\ <! 1 L\ <! 1 %5 %] !< %H $7 $F $$ $k %A %C %W %; %C %H 2 2 4p K\ 9= @. 4 3 XF86Con�g %* %W %7 %g %s 4 4 %b !< %I $K 4X $9 $k 5D O@ 7 5 %j %K %" %" %I %l %C %7 %s %0 $H 16bpp/32bpp %b !< %I 7 6 \cl64xx" %I %i %$ %P 9 7 \cirrus" %I %i %$ %P $G $N >c 32 BP :v $N $^ $H $a 10 8 %I %i %$ %P $N JQ 99 E@ 12

1. %5 %] !< %H $7 $F $$ $k %A %C %W %; %C %H 2 1 %5 %] !< %H $7 $F $$ $k %A %C %W %; %C %H Cirrus $N %A %C %W %; %C %H MQ $K $O !" \cirrus" $H \cl64xx" $H 8F $P $l $k #2 $D $N 0[ $J $k SVGA %5 !< %P !< $, $" $j $^ $9 !# \cirrus" %I %i %$ %P $O 256 ?’ $N !J %" %/ %; %i %l !< %? IU $- !K SVGA %5 !< %P !< $H !J %" %/ %; %i %l !< %? L5 $7 !K Gr 9u %5 !< %P !< $G MQ $$ $i $l $F $$ $^ $9 !# SVGA %5 !< %P !< $O 16 $H 32 %T %/ %; %k Ev $j %S %C %H ?t $r %5 %] !< %H $7 !" $3 $N 9= @. $G E7 A3 ?’ (truecolor) %b !< %I $r %5 %] !< %H $7 $F $$ $^ $9 !# \cl64xx" %I %i %$ %P $O 256 ?’ SVGA, 16 ?’ $H Gr 9u %5 !< %P !< $G MQ $$ $i $l $F $$ $^ $9 !# $I $A $i $, 0B Dj $7 $F $$ $k $H $+ $O $3 $3 $G $O 5D O@ $7 $^ $; $s $, !" $3 $N J8 =q $G $O \cirrus" %I %i %$ %P $K $D $$ $F <g $K 8@ 5Z $7 $^ $9 !# 0J 2< $N Cirrus Logic $N %A %C %W %; %C %H $r %5 %] !< %H $7 $F $$ $^ $9 !# : CL-GD5420 ISA SVGA %A %C %W %; %C %H , 1M %P %$ %H ; :G Bg %I %C %H %/ %m %C %/ $O 45 MHz (256 ?’ %5 !< %P !< ) !# 3H D% =q $- 9~ $_ %b !< %I $K $h $k %" %/ %; %i %l !< %? 5! G= !J $3 $N %5 !< %P !< $G $O %9 %/ %m !< %k $H %Y %? EI $j $D $V $7 $K MQ $$ $F $$ $k !K !# $3 $N %A %C %W %; %C %H $O 256 ?’ $N 1024x768 %N %s %$ %s %? !< %l !< %9 $O %5 %] !< %H $7 $^ $; $s !# CL-GD5422 5420 $N 2~ NI HG (32 %S %C %H Fb B" %a %b %j %$ %s %? !< %U %’ !< %9 ) !# :G Bg %I %C %H %/ %m %C %/ $O 80 MHz !# CL-GD6205/6215/6225/6235 5420 $K $[ $\ 8_ 49 @- $N $" $k %i %C %W %H %C %W MQ %A %C %W %; %C %H !# %I %C %H %/ %m %C %/ $O 25 MHz $N $_ %5 %] !< %H $9 $k !J 30 It %G %# %9 %W %l %$ $O $= $l 0J >e 2D G= !K !# "noaccel" %* %W %7 %g %s $, I, MW $J $N $G Cm 0U $N ;v !# CL-GD6420/6440 $3 $l $i $N %A %C %W %; %C %H $O 542x %7 %j !< %: $H $O 8_ 49 @- $O $" $j $^ $; $s $, !" \cl64xx" %I %i %$ %P $G %5 %] !< %H $7 $^ $9 !# $3 $N %A %C %W %; %C %H $O :G 6a $N %i %C %W %H %C %W $K Ek :\ $5 $l $F $* $j !" @N $N Cirrus %A %C %W %; %C %H (5410/A V GA2) $H F1 MM $K Fb B" $7 $F $$ $^ $9 !# $3 $N %I %i %$ %P $O B> $N 64xx %A %C %W %; %C %H $G $b 2T F/ $7 $F $$ $^ $9 !# 9= @. >e $N <1 JL ;R $O "cl6420" $H "cl6440" $G $9 !# $3 $N %I %i %$ %P $K $D $$ $F $O 6 $N @a $G >\ :Y $K =R $Y $^ $9 !# CL-GD5424 4p K\ E* $K 5422 $N VLB HG $G $9 $, !" $$ $/ $D $+ $N E@ $G 5426 $K ;w $F $$ $^ $9 !# CL-GD5426 ISA %P %9 $H VLB N> J} $N 2M %P %$ %H 0J >e $N %a %b %j $r Ek :\ $7 $? $b $N $r %5 %] !< %H $7 $^ $9 !# $h $j $h $$ %" %/ %; %i %l !< %? $r 5a $a $k $J $i BitBL T %( %s %8 %s $r Ek :\ $7 $F $/ $@ $5 $$ (BitBL T $O 2h A| E> Aw $H %F %- %9 %H I= <( $K M- 8z ) !# %I %C %H %/ %m %C %/ $N >e 8B $O 85 MHz !# CL-GD5428 5426 $N 2~ NI HG !# CL-GD5429 5428 $N 2~ NI HG $G !" $h $j 9b $$ MCLK $r 8x <0 $K %5 %] !< %H $7 !" %a %b %j %^ %C %W %I I/O $r Ek :\ $7 $F $$ $^ $9 !# CL-GD5430 5429 $K ;w $F $$ $^ $9 $, !" 4p $O 543x (32 %S %C %H %[ %9 %H %$ %s %? !< %U %’ !< %9 ) $G $9 !# 64 %S %C %H %a %b %j %b !< %I $O ;} $C $F $$ $^ $; $s !#

1. %5 %] !< %H $7 $F $$ $k %A %C %W %; %C %H 3 CL-GD5434 64 %S %C %H Fb B" %a %b %j %$ %s %? !< %U %’ !< %9 $r ;} $C $? <! $N @$ Be $N ‘Alpine’ $N 7O Ns $N %A %C %W $G $9 !# Orchid Kelvin 64 $K Ek :\ $7 $F $$ $^ $9 !# $3 $N %A %C %W $O 2M %P %$ %H $N %a %b %j $r Ek :\ $7 $? $H $- 64 %S %C %H %b !< %I $N $_ %5 %] !< %H $7 $^ $9 !# 1M %P %$ %H %a %b %j $N $_ $N $N %+ !< %I $G $O 87 $7 $$ 8B 3& $, $" $j $^ $9 !# 110 MHz 0J >e $N %I %C %H %/ %m %C %/ $r %5 %] !< %H $7 $^ $9 !J :G 6a $N %A %C %W %; %C %H $O 135 MHz $r %5 %] !< %H $7 $F $$ $^ $9 !K !# CL-GD5436 9b EY $K :G E, 2= $7 $? 5434 !# 4p K\ E* $K 5434 $H $7 $F 07 $( $^ $9 $, !" %F %9 %H $7 $F $^ $; $s !# 3F !9 $N %5 %] !< %H $7 $F $$ $k ?< $5 Kh $K :G Bg $N %I %C %H %/ %m %C %/ $r 0l Mw $K $7 $^ $9 !# : mono 8 bpp (256c) 16 bpp____ 32 bpp CL-GD62x5 45 MHz 45 MHz____ CL-GD5420 80 MHz 45 MHz (1) CL-GD542x/512K 80 MHz 45 MHz____ CL-GD5422/24 80 MHz 80 MHz____ 40 MHz____ CL-GD5426/28 85 MHz 85 MHz____ 45 MHz (2) CL-GD5429 85 MHz 85 MHz____ 50 MHz____ CL-GD5430 85 MHz 85 MHz____ 45 MHz (2) CL-GD5434/1Mb 85 MHz 85 MHz____ 45 MHz (2) CL-GD5434/2Mb 85 MHz 110/135 MHz 85 MHz____ 45/50 MHz (2) CL-GD5436/1Mb 85 MHz 110 MHz (3) 60 MHz (3) CL-GD5436/2Mb 85 MHz 135 MHz 85 MHz 60 MHz (3) (1) 512K %a %b %j $G $9 !# (2) 9b $$ MCLK $r @_ Dj $9 $k $H 50 MHz !# (3) %a %b %j %/ %m %C %/ $K 0M B8 $9 $k !# Bg $^ $+ $K 8@ $C $F 2> A[ E* / J* M} E* $J 2h LL 2r A| EY $O %S %G %* %a %b %j $N NL $N 0c $$ $K @) Ls $5 $l $^ $9 !# mono 8bpp 16 bpp 32 bpp 256K_ 800x600__ 640x400__ _________ ________ 512K_ 1152x900_ 800x600__ 640x400__ ________ 1024K 1600x1200 1152x900_ 800x600__ ________ 2048K 2304x1728 1600x1200 1152x900_ 800x600_ 4096K 2304x1728 2272x1704 1600x1200 1152x900 %" %/ %; %i %l !< %? 5! G= $r ;H $C $? >l 9g !" 2> A[ 2h LL $N I} $O 32 $N G\ ?t $K $J $j $^ $9 !# %b %K %? !< $N ?e J? J} 8~ $N D4 @0 ?t CM $O 2048 0J 2< $K $7 $J $1 $l $P $$ $1 $^ $; $s !# 16 $+ 32 bpp $G XF86 SVGA $r F0 :n $5 $; $k $K $O !" 0J 2< $N %* %W %7 %g %s $r X %5 !< %P !< $K IU 2C $7 $F 2< $5 $$ !# startx -- -bpp 16 5-6-5 RGB (’64K color’, XGA) startx -- -bpp 16 -weight 555 5-5-5 RGB (’Hicolor’) startx -- -bpp 32 8-8-8 XRGB truecolor (5434)

2. 4p K\ 9= @. 4 2 4p K\ 9= @. ‘ xf86config ’ %W %m %0 %i %‘ $r ;H MQ $7 $F XF86Con�g %U %! %$ %k $r @8 @. $9 $k $3 $H $r $* 4+ $a $7 $F $$ $^ $9 $, !" $3 $N %W %m %0 %i %‘ $O 2T F/ 2D G= $J 9b 2r A| EY $N 8bpp $N 9= @. $r :n @. $7 $^ $9 !# ;H MQ $9 $k %b %K %? !< $K !" $h $j E, 1~ $7 $? %b !< %I D4 @0 CM $r Monitor @a $K 5- F~ $7 $? $/ $J $k $G $7 $g $& !# %I %i %$ %P $N %* %W %7 %g %s $K $D $$ $F $O <! $N @a $G >\ :Y $K =R $Y $^ $9 $N $G !" $3 $3 $G $O 7Z $/ ?( $l $k $@ $1 $K $7 $^ $9 !# A4 $F $N $N %A %C %W %; %C %H MQ $K Clockchip "cirrus" 9T $r Device @a $K =q $- $^ $7 $g $& !# $3 $& $d $C $F $* $/ $H %5 !< %P !< $, %5 %] !< %H $7 $F $$ $k BP :v :Q $_ $N %I %C %H %/ %m %C %/ $N AH $_ 9g $o $; $N Cf $+ $i E, @Z $J %I %C %H %/ %m %C %/ $r ;H MQ 2D G= $K $7 $^ $9 !# Dc 2r A| EY $N %b %K %? !< BP 1~ $G 12.6 MHz $N %I %C %H %/ %m %C %/ $r ;H $$ $? $$ >l 9g $K I, MW $K $J $j $^ $9 !# %0 %i %U %# %C %/ 2h LL $N :F IA 2h $, $& $^ $/ F0 :n $7 $J $$ >l 9g $O !" %A %C %W %; %C %H $, BitBL T %( %s %8 %s $r ;} $C $F $$ $k >l 9g $K @h $: "no bitblt" %* %W %7 %g %s $r ;n $7 $F $/ $@ $5 $$ !# $3 $l $, $& $^ $/ F0 :n $7 $J $$ $H $- $O "noaccel" %* %W %7 %g %s $r ;n $7 $F $_ $F $/ $@ $5 $$ !# A4 $F $N %" %/ %; %i %l !< %? 5! G= $r L5 8z $K $7 $^ $9 !# "no imageblt" %* %W %7 %g %s $G =< J, $+ $b $7 $l $^ $; $s !# 16bpp $+ 32bpp $N ?< $5 $G <B 9T $9 $k $+ !" 8bpp $G @- G= $r 8~ >e $5 $; $k $K $O %j %K %" %" %I %l %C %7 %s %0 5! G= $r ;H $( $k $h $& $K $7 $J $1 $l $P $$ $1 $^ $; $s !# %m !< %+ %k %P %9 $N 543x %+ !< %I $^ $? $O !" %a %b %j $, 16M %P %$ %H 0J 2< $N %7 %9 %F %‘ $G %m !< %+ %k %P %9 $N 542x %+ !< %I $b $7 $/ $O ISA $N 543x %+ !< %I $r Ek :\ $7 $F $$ $k $H $- $K 0l HL $K ;H MQ 2D G= $G $9 !# "linear" %* %W %7 %g %s $, I, ?\ $G !" $* $= $i $/ Membase $G %" %I %l %9 $r ;X Dj $9 $k I, MW $, $" $k $G $7 $g $& !# 0J 2< $N @a $G >\ :Y $K @b L@ $7 $^ $9 !# :G 8e $K 534x $G %G %P %$ %9 @a $K "mmio" %* %W %7 %g %s $r =q $$ $F $* $/ $H 99 $K NI 9% $J %" %/ %; %i %l !< %? $K $J $j $^ $9 < $3 $N %* %W %7 %g %s $O 5429 $G $b E, MQ 2D G= $H ;W $$ $^ $9 $, !" L$ $@ %F %9 %H $7 $F $$ $^ $; $s > !# 3 XF86Con�g %* %W %7 %g %s ‘ Clocks ’ %3 %^ %s %I $O ;H $o $J $$ $G $/ $@ $5 $$ !# !J $D $^ $j !" C5 :: $7 $J $$ $G !K %/ %m %C %/ $r =$ @5 $7 $? >l 9g !" !J 3F !9 $N %A %C %W %; %C %H $N %5 %] !< %H $7 $F $$ $k :G Bg %/ %m %C %/ 0J 30 $N !K %+ !< %I Kh $N 0c $$ $O H? 1G $G $- $^ $; $s !# 0J 2< $N %* %W %7 %g %s $O FC $K Cirrus %I %i %$ %P $G $O =E MW $G $9 !# 3F !9 $N %* %W %7 %g %s $O XF86Config $N ‘ svga ’ %I %i %$ %P @a $K Screen 9‘ $N Cf $K E, 1~ $9 $k A4 $F $N ?< $5 $r ;X Dj $9 $k I, MW $, $" $j $^ $9 !J Device @a $K A4 $F $N Screen $r ;X Dj $9 $k $3 $H $, 2D G= $G $9 !K !# \noaccel" %* %W %7 %g %s $3 $N %* %W %7 %g %s $O %" %/ %; %? %l !< %? 5! G= $r L5 8z $K $7 $^ $9 !# DRAM $N B. EY $d 9b $$ %I %C %H %/ %m %C %/ $d %" %/ %; %i %l !< %? 5! G= $N IT 6q 9g $K $h $k Ld Bj $r 2r 7h $9 $k ;Y 1g $r 8z N( NI $/ !J VLB $G $O 0l CJ $H BE Ev $K !K 9T $$ $^ $9 !# \fast dram" \med dram" \slow dram" (5424/6/8/9, 543x) %* %W %7 %g %s "fast dram" %* %W %7 %g %s $O %S %G %* %\ !< %I $N Fb B" %a %b %j %/ %m %C %/ (MCLK) %l %8 %9 %? $K $h $j 9b $$ CM $r @_ Dj $7 $^ $9 !# DL >o !" $3 $N %l %8 %9 %? $O $$ $8 $k $3 $H $O $J $$ $N $G $9 $, !" I8 =‘ $N CL-GD542x BIOS $N =i 4| 2= $K $h $C $F 9b $$ %I %C %H %/ %m %C %/ %b !< %I $G $N @- G= $K NI $/ $J $$ 1F 6A $r M? $( $k $h $& $J !J %A %C %W %; %C %H $N ;E MM $K @) 8B $5 $l $? !K Dc $$ J} $N CM $K @_ Dj $5 $l $^ $9 !# $3 $l $O 3H D% RAS D4 @0 $r ;H $& >l 9g $K $O FC $K 1F 6A $r <u $1 $^ $9 !J $3 $l $O %5 !< %P !< $N C5 :: $G ;X E& $5 $l $^ $9 !K !# DRAM $N <B :] $N B. EY $O $3 $N %* %W %7 %g %s $, E, @Z $@ $m $& $H $J $+ $m $& $H %+ !< %I G’ <1 $K $* $$ $F 4m 81 $J MW AG $K $O $J $j $^ $; $s !# 80ns $N DRAM $r Ek :\ $7 $F $$ $k $" $k %+ !< %I $, 3H D% RAS D4 @0 $r ;H $C $F DOS $N %I %i %$ %P %f !< %F %# %j %F %# $G MCLK $r (0x22) $N $h $& $J CM $K @_ Dj $7 $? >l 9g $O 9b $$ MCLK $G 0B Dj $7 $F F0 :n $7 $F $$ $k MM $K 8+ $( $k $G $7 $g $& !# %+ %9 %? %^ %$ %: $5 $l $? BIOS $, $h $j 9b $$ I8 =‘ CM 0J 30 $N CM $K =i 4| 2= $7 $? !J <g $K M- L> $I $3 $m $N !K %+ !< %I $, $" $j $^ $9 !# $3 $N >l 9g $O !" $3 $N %* %W %7 %g %s $r ;H $& $H E, @Z $G $O $J $$ $+ $b $7 $l $^ $; $s !#

3. XF86CONFIG %* %W %7 %g %s 5 "slow dram" %* %W %7 %g %s $O MCLK $r I8 =‘ $N CL-GD542x BIOS $N CM (0x1c) $K @_ Dj $7 $^ $9 !# 9b $9 $. $k MCLK $N CM $O ?b D> J} 8~ $N 2h LL $N $A $i $D $/ BS !" %F %- %9 %H $K 8m $C $? 2h AG !" %F %- %9 %H %b !< %I $N 2h AG $N H4 $1 $r X $N F0 :n 8e $K 0z $- 5/ $3 $7 $^ $9 !J MCLK $N @_ Dj $, Dc $9 $. $k >l 9g $b F1 MM $N 8= >] $r 5/ $3 $7 $^ $9 $N $G Cm 0U $7 $^ $7 $g $& !K !# 3+ ;O ;~ $K !" %I %i %$ %P !< $O MCLK $N CM $r I= <( $9 $k $G $7 $g $& !J @h $: !" $3 $l $r 3N G’ $7 $F 2< $5 $$ !K !" $= $7 $F $3 $N CM $O %b !< %I $K $h $C $F JQ 2= $7 $^ $9 !# E5 7? E* $J MCLK $N CM : 0x1c (50 MHz) $3 $l $O BIOS $N I8 =‘ CM $G MQ $$ $i $l $^ $9 !# "slow dram" %* %W %7 %g %s $G 6/ @) ;X Dj $G $- $^ $9 !# 0x1f (55 MHz) "med dram" %* %W %7 %g %s $G ;H MQ $9 $k CM $G $9 !# 542x $r ;H $C $F $$ $k %+ !< %I $G $N :G 9b $N CM $O %j %K %" %" %I %l %C %7 %s %0 $, M- 8z $K $J $C $F $$ $J $$ $H 07 $( $J $$ $h $& $G $9 !# 0x22 (60 MHz) KX $I $N !J 3H D% RAS !K 542x %+ !< %I $G $O "fast dram" %* %W %7 %g %s $r ;H $& $H M- 8z $K $J $j $^ $9 !# 8x <0 $J 542x %A %C %W $N :G Bg <~ GH ?t $O 50 MHz $G $9 !# 5434 $N 8x <0 ;E MM $O $^ $? 50 MHz (0x1c) $G !" 5429 $H 5430 $N %0 %i %U %# %C %/ %b !< %I $G $O 60 MHz (0x22) $N MCLK $r %5 %] !< %H $7 !" %I %i %$ %P $O <+ F0 E* $K $3 $l $r AH $_ 9~ $_ $^ $9 !# $3 $l $, Ld Bj $r 0z $- 5/ $3 $7 $? >l 9g $O " slow dram " %* %W %7 %g %s $r ;H MQ $7 $F $/ $@ $5 $$ !# %I %i %$ %P $O G’ <1 $7 $? DRAM BS 0h I} $N %/ %m %C %/ $N >e 8B $r MCLK $K <h $j 9~ $_ $^ $9 !# FC $K !J 9b $$ %I %C %H %/ %m %C %/ $G @- G= $d 0B Dj EY $N !K Ld Bj $, $J $+ $C $? $i !" "fast dram" %* %W %7 %g %s $r ;H $& I, MW $O $" $j $^ $; $s !# \no bitblt" %* %W %7 %g %s $3 $N %* %W %7 %g %s $r 5426/28/29/3x $G ;H MQ $9 $k >l 9g !" %" %/ %; %i %l !< %? 5! G= $r J] ;} $9 $k 4V !" !J 5424 $G $O ;} $C $F $$ $J $$ !K BitBL T %( %s %8 %s $r L5 8z $K $7 $^ $9 !# BitBL T %( %s %8 %s $r ;H MQ $9 $k $3 $H $K 4X O" $7 $F @8 $8 $k 5! G= >e $N Ld Bj $K BP $7 $F M- 8z $G $9 !# @- G= $O $+ $J $j Cx $7 $/ Mn $A $^ $9 !# \no imageblt" %* %W %7 %g %s $3 $N %* %W %7 %g %s $r 5426/28/29/3x $G ;H MQ $9 $k >l 9g !" %7 %9 %F %‘ %a %b %j $+ $i %S %G %* %a %b %j $K E> Aw $9 $k BitBL T 5! G= $r L5 8z $K $7 $^ $9 !# FC $K B. $$ CPU $G VLB 5426 $H 5434 $r ;H $C $? $$ $/ $D $+ $N %7 %9 %F %‘ 9= @. $G G’ $a $i $l $F $$ $k !" 2h LL $N :8 >e $9 $_ $N >. $5 $$ Gr $$ @~ <c $/ $O %5 !< %P !< $K La $C $? 8e $N OD $s $@ 2h A| $N MM $J 2h A| =q $- 9~ $_ $N Ld Bj $K M- 8z $G $9 !# $3 $N %* %W %7 %g %s $r ;H $& $H @- G= $, Dc 2< $7 $^ $9 $N $G Cm 0U $7 $F $/ $@ $5 $$ !# \clgd54xx" %A %C %W %; %C %H Ek :\ $5 $l $F $$ $k %A %C %W %; %C %H $r 6/ @) C5 :: $5 $; $^ $9 !# %5 %] !< %H $7 $F $$ $k %A %C %W %; %C %H $, @5 3N $K G’ <1 $5 $l $J $$ $H $+ !" %5 %] !< %H $7 $F $$ $J $$ %A %C %W %; %C %H $r %5 %] !< %H $7 $F $$ $k %A %C %W %; %C %H 8_ 49 IJ $H $7 $F G’ <1 $5 $; $? $$ >l 9g $K M- 8z $G $9 !# videoram 1024 ( Kt $O B> $N CM ) $3 $N %* %W %7 %g %s $O %S %G %* %a %b %j $N C5 :: Ek :\ NL $N 6/ @) ;X Dj $H 8= 9T $N %+ !< %I $K %a %b %j $r DI 2C $9 $k $U $j $r $9 $k >l 9g $K ;X Dj $7 $^ $9 !# $3 $N %* %W %7 %g %s $O 2M %P %$ %H $N %a %b %j 9= @. ;~ $K %I %i %$ %P $N MW 5a %a %b %j NL $H 8_ 49 @- $, J] $F $J $$ >l 9g $K #1 MB 0J >e $r 8+ $; $? $/ $J $$ !" $H $+ %a %b %j $N C5 :: $, $& $^ $/ F0 :n $7 $J $$ $H $- $K M- 8z $G $9 !# $3 $l $O Device @a $K I, $: ;X Dj $7 $F $/ $@ $5 $$ !#

3. XF86CONFIG %* %W %7 %g %s 6 \�fo conserv ativ e" %* %W %7 %g %s (5424/6/8/9/30 $N >l 9g $K ;X Dj ) $3 $N %* %W %7 %g %s $O CR T FIFO $N I_ 5o CM $r 9b $$ %I %C %H %/ %m %C %/ $N 95 $( L\ $J CM ( > = 65 MHz) $K @_ Dj $9 $k $b $N $G !" ‘ 6Z !& 0p :J ’(‘streaks’) , ‘ %8 %C %? !& IT 0B Dj ’(‘jitter’) <c $/ $O 2h LL $N ?e J? NN 0h $N 7+ $j JV $7 I= <( ( FC $K BitBL T A‘ :n $r 9T $C $? $H $- , Nc $( $P %9 %/ %m !< %k ) $H 7A MF $5 $l $k Ld Bj $r @- G= $, Mn $H $7 $F $b 7Z 8: $7 $? $$ >l 9g $K M- 8z $G $9 !# \�fo aggressive" %* %W %7 %g %s (5424/6/8/9/30 $N >l 9g $K ;X Dj ) $3 $N %* %W %7 %g %s $O CR T FIFO $N I_ 5o CM $r 9b $$ %I %C %H %/ %m %C %/ $N @Q 6K E* $J CM $K @_ Dj $9 $k $b $N $G !" Dc $$ J} $N %I %C %H %/ %m %C %/ MQ $K ;H MQ $9 $k $b $N $H F1 $8 $G $9 !# $3 $N %* %W %7 %g %s $O 9b $$ %I %C %H %/ %m %C %/ $G $N @- G= $r 8~ >e $5 $; $^ $9 !# \no 2mb banksel" %* %W %7 %g %s (542x $N >l 9g $K ;X Dj ) $3 $N %* %W %7 %g %s $O 2M %P %$ %H $N %a %b %j $r Ek :\ $7 $? %+ !< %I $G 1M %P %$ %H 0J >e $N %a %b %j $r M- 8z $K $9 $k ‘DRAM bank select’ %S %C %H $r @_ Dj $7 $J $$ $b $N $G $9 !# $3 $N %* %W %7 %g %s $O 512Kx8 $N DRAM 9= @. $G M- 8z $G !" 1M %P %$ %H 0J >e $r 2> A[ 2h LL $K ;H $C $F $$ $k 256Kx4/16 $N DRAM 9= @. $N >l 9g $O L5 8z $G $9 !# \prob e clo cks" %* %W %7 %g %s $3 $N %* %W %7 %g %s $O %+ !< %I $N %I %C %H %/ %m %C %/ $r 6/ @) C5 :: $7 $^ $9 !# %/ %m %C %/ $, 8G Dj $G A4 $F $N Cirrus $N %A %C %W %; %C %H $G F1 $8 $J $i I, MW $" $j $^ $; $s !# $7 $+ $7 8= >u I8 =‘ $N 14.31818 MHz $N <~ GH ?t $r %P %9 $K 6! 5k $9 $k %^ %6 !< %\ !< %I $K 0M B8 $7 $^ $9 !# 4V 0c $C $F @_ 7W $5 $l $? VLB $N %^ %6 !< %\ !< %I $O E, @5 $J %P %9 <~ GH ?t $N $? $a $N $3 $N <~ GH ?t $r @5 $7 $/ 6! 5k $7 $^ $; $s !J Nc $( $P 33 MHz $+ $i 3H D% $7 $? $b $N !K !# $b $7 4V 0c $C $F $$ $? $i !" $3 $N %* %W %7 %g %s $r IU $1 $F ‘ X -probeonly $r <B 9T $7 $F $/ $@ $5 $$ !# %/ %m %C %/ $, 0J 2< $K <( $9 @5 $7 $$ %/ %m %C %/ $+ $i $H $F $b 0[ $J $C $F $$ $? >l 9g !" XF86Config $N Clocks 9T $K JP $C $F $$ $k J} $N %/ %m %C %/ $r 5- F~ $7 $F $/ $@ $5 $$ !# $3 $N >l 9g !" MCLK $b Lr $K $? $A $^ $; $s !# @5 $7 $$ %/ %m %C %/ : 25.2 28.3 41.1 36.1 31.5 40.0 45.1 49.9 65.0 72.2 75.0 80.0 85.2 \cirrus" %/ %m %C %/ %A %C %W $3 $N %* %W %7 %g %s $O %W %m %0 %i %^ %V %k %/ %m %C %/ $r 2D G= $K $7 $^ $9 !# Device @a $K ;X Dj $9 $k I, MW $, $" $j $^ $9 !# $3 $N %* %W %7 %g %s $r IU $1 $k $H !" %/ %m %C %/ %b !< %I $, <+ F0 $G A* Br $5 $l $^ $9 !# Clo cks 9T $O 5- F~ $7 $J $$ $G $/ $@ $5 $$ !# $3 $N %* %W %7 %g %s $O 320x200 $N %@ %V %k %9 %- %c %s %b !< %I $N $? $a $N 12.5 MHz $N %/ %m %C %/ $r 2D G= $K $7 $^ $9 !# $$ $/ $D $+ $N <~ GH ?t $O IT 0B Dj $K $J $k $+ $b $7 $l $J $$ !J ‘ GH BG $D ’ 2h LL $, =P $k $+ $b $7 $l $^ $; $s !K $N $G Cm 0U $7 $F $/ $@ $5 $$ !# ;n $7 $F !" %F %9 %H $7 $? <~ GH ?t !J I8 =‘ CM $N $h $& $K !K $@ $1 $, 0B Dj $J $N $O J] >Z $7 $^ $9 !# \linear" %* %W %7 %g %s $3 $N %* %W %7 %g %s $O SVGA %P %s %/ @Z $j BX $( $G $O I, MW $N $J $$ A4 %U %l !< %‘ %P %C %U %! $r %7 %9 %F %‘ %a %b %j $N HO 0O $r D6 $( $? 9b 0L $N %" %I %l %9 $^ $G 3d $j IU $1 $k %j %K %" %" %I %l %C %7 %s %0 $r M- 8z $K $7 $^ $9 !# 256 ?’ ;~ $N @- G= $, 8~ >e $7 16bpp $H 32bpp $G $O I, ?\ $K $J $C $F $$ $^ $9 !# >\ :Y $O 5 $N @a $r ;2 >H $7 $F $/ $@ $5 $$ !# Membase 0x00e00000 ( Kt $O 0[ $J $k %" %I %l %9 ) $3 $N %* %W %7 %g %s $O J* M} E* $J %j %K %" %U %l !< %‘ %P %C %U %! $N %a %b %j 4p Dl %" %I %l %9 $r @_ Dj $7 $^ $9 !# $3 $l $O Device @a $K ;X Dj $9 $k I, MW $, $" $j $^ $9 !# KX $I $N %j %K %" %" %I %l %C %7 %s %0 $N 9= @. $K I, MW $G $9 !#

4. %b !< %I $K 4X $9 $k 5D O@ 7 \fav our bitblt" %* %W %7 %g %s (5426 $N $_ ) $3 $N %* %W %7 %g %s $O BitBL T %( %s %8 %s $r M- 8z $K $7 $F %U %l !< %‘ %P %C %U %! $N ?’ ?t $r A} $d $9 5! G= $r 0l HL E* $K B. $/ $9 $k $N $K MQ $$ $^ $9 !# $3 $N %* %W %7 %g %s $O CPU $K Ii 2Y $N $+ $+ $C $? %7 %9 %F %‘ !J Nc $( $P !" gcc $H B> $N %W %m %0 %i %‘ $, F1 ;~ $K <B 9T $7 $F $$ $k >l 9g $J $I !K Ey !" 0l Dj $N >r 7o $G @- G= $N 8~ >e $r $O $+ $j $^ $9 !# \mmio" %* %W %7 %g %s (543x) $3 $N %* %W %7 %g %s $O >/ $7 B. $/ $J $k %a %b %j %^ %C %W %I I/O $r ;H $& 543x/5429 >e $N BitBL T %( %s %8 %s $H $N @\ B3 $r M- 8z $K $7 $^ $9 !# IU ?o $7 $F %a %b %j %^ %C %W %I I/O $r ;H $& %" %/ %; %i %l !< %? 5! G= $b M- 8z $K $J $j $^ $9 !# $3 $N IU 2C 5! G= $O BitBL T %( %s %8 %s $r ;H $o $J $$ $H $- !J Nc $( $P !" " no bitblt " $r ;H $C $? >l 9g !K $O 8z 2L $, $" $j $^ $; $s !# \sw cursor" %* %W %7 %g %s (542x/3x) $3 $N %* %W %7 %g %s $O %A %C %W $, Ds 6! $9 $k %O !< %I %& %’ %" %+ !< %= %k $r M- 8z $K $7 $^ $9 !# %+ !< %= %k $K Ld Bj $, $" $k $H $- $K ;n $7 $F $/ $@ $5 $$ !# FC $K !" 5434/6 $G 85 MHz 0J >e $N %I %C %H %/ %m %C %/ $r ;H $& $H $- $K M- 8z $G $9 $, !" %A %C %W $, $= $N %/ %m %C %/ $G %O !< %I %& %’ %" %+ !< %= %k $N A4 $F $N 5! G= $r %5 %] !< %H $7 $F $$ $J $$ $3 $H $K Cm 0U $7 $F $/ $@ $5 $$ !# \clgd6225 lcd" %* %W %7 %g %s $$ $/ $D $+ $N 62x5 %i %C %W %H %C %W MQ %A %C %W %; %C %H $G :G 9b $K Gr $$ ?’ $r LCD 2h LL $K I= <( $9 $k $H $- $N Ld Bj $K BP $9 $k BP :v $r Ds 6! $7 $^ $9 !# 4 %b !< %I $K 4X $9 $k 5D O@ 256 ?’ %" %/ %; %i %l !< %? %I %i %$ %P $O %S %G %* %a %b %j Fb $N 256 %P %$ %H !" %O !< %I %& %’ %" %+ !< %= %k $O 1K %P %$ %H $r :n 6H NN 0h $K ;H $$ $^ $9 !# 7k 2L E* $K 1M %P %$ %H $N %+ !< %I $G $O 1024x1024 $N 2> A[ 2r A| EY $O ;H MQ =P Mh $^ $; $s !# FC $K BitBlt $r IA 2h MQ $N DRAM I} $, >. $5 $$ >l 9g $K ;H MQ $7 $? $H $- !" $h $j 9b $$ %I %C %H %/ %m %C %/ <~ GH ?t $O %0 %i %U %# %C %/ A‘ :n $N @- G= $K H] Dj E* $J 8z 2L $r 5Z $\ $7 $^ $9 !J $= $N NL $O 5/ F0 ;~ $K I= <( $5 $l $^ $9 !K !# I8 =‘ $N MCLK $N @_ Dj (0x1c) $H 32- %S %C %H %a %b %j %$ %s %? !< %U %’ !< %9 $r ;H MQ $7 $? $H $- !" 65 MHz $N %I %C %H %/ %m %C %/ $G $N @- G= $O 25 MHz $N %I %C %H %/ %m %C %/ ;~ $N @- G= $N H> J, $K $J $k >l 9g $, $" $j $^ $9 !# DRAM I} $, >/ $J $$ $H $- !" $H $F $b CY $/ 46 $8 $? $i %I %C %H %/ %m %C %/ $r :G $b CY $$ MF G’ $G $- $k CM $K $7 $F $_ $F $/ $@ $5 $$ !# Nc $( $P 9b $$ :F IA 2h B. EY !J 50MHz $N %I %C %H %/ %m %C %/ !K $r ;H $C $F 14 " Kt $O 15 " $N %b %K %? !< $K Bg $- $J 2> A[ 2h LL $G 800x600 $N 2h LL $r I= <( $9 $k $N $O $= $s $J $K 0- $/ $" $j $^ $; $s !# 1024x768 $G :G $b 9b $$ %/ %m %C %/ (85 MHz) $r 542x $N 76 Hz $G ;H MQ $7 $? >l 9g !" @- G= 8~ >e ;X 8~ $K $O $J $j $^ $; $s !# %+ !< %I $O Bg Dq Dd ;_ $7 $^ $9 !# 75 MHz $N %I %C %H %/ %m %C %/ $r 70 Hz $G ;H $C $? >l 9g $O K~ B- $G $- $k $G $7 $g $& !# 85 MHz $N %I %C %H %/ %m %C %/ $K $* $$ $F 76 Hz $G 1024x768 $r %5 %] !< %H $7 $F $$ $k %b %K %? !< $r ;} $C $F $$ $k >l 9g $O !" I8 =‘ E* $J 5426/5428 $r 4p $K $7 $? %+ !< %I $H $O Aj @- $, NI $/ $J $$ $G $7 $g $& !# 2M $N %a %b %j $r @Q $s $@ 5434 $r 4p $K $7 $? %+ !< %I $O 9b $$ %I %C %H %/ %m %C %/ $H Aj @- $, NI $/ !" 542x %7 %j !< %: $K Hf $Y DRAM I} $O 4p K\ E* $K 2 G\ $" $j $^ $9 !# Kt !" 543x %A %C %W $N N‘ $O ;H MQ 2D G= $J DRAM I} $, 0l CJ $H 8z 2L E* $K 3N J] $G $- $^ $9 !# 5 %j %K %" %" %I %l %C %7 %s %0 $H 16bpp/32bpp %b !< %I 8= :_ !" SVGA %5 !< %P !< $, Hs %" %/ %; %i %l !< %? $N 16- %S %C %H $H 32- %S %C %H %T %/ %; %k $r %5 %] !< %H $9 $k $K $O %j %K %" %" %I %l %C %7 %s %0 $, I, ?\ $G $9 !# $3 $N @) Ls $O $& $^ $/ $$ $1 $P >- Mh E* $K $O $: $5 $l $k $G $7 $g $& !# " linear " %* %W %7 %g %s $O ?< $5 $r ;X Dj $9 $k screen @a $G ;X Dj $9 $k $3 $H $G %j %K %" %" %I %l %C %7 %s %0 $r M- 8z $K $7 !" Kt MemBase $r (device @a $G ) @_ Dj $9 $k I, MW $, $" $k $G $7 $g $& !# %+ !< %I $K $h $C $F 0[ $J $k 9= @. $, $$ $/ $D $b $" $j $^ $9 !#

5. %j %K %" %" %I %l %C %7 %s %0 $H 16BPP/32BPP %b !< %I 8 ISA %P %9 MQ $N 542x/543x $H 16M %P %$ %H $+ $= $l 0J >e $N %7 %9 %F %‘ %a %b %j $N >l 9g $O %j %K %" %" %I %l %C %7 %s %0 $O IT 2D G= $G $9 !# 16bpp $O ;H $( $^ $; $s !" $9 $$ $^ $; $s !# 14M %P %$ %H 0J 2< $N %a %b %j $N >l 9g $O ‘ MemBase 0x00e00000 ’ $r ;H $& $3 $H $G %U %l !< %‘ %P %C %U %! $r 14M %P %$ %H $K 3d $j IU $1 $k $3 $H $, 2D G= $G $9 !# ‘e’ $N 8e $m $K %< %m $r #5 $D IU $1 $F $/ $@ $5 $$ !# ;D G0 $J $, $i B? $/ $N ISA %+ !< %I $O %j %K %" %" %I %l %C %7 %s %0 $r %5 %] !< %H $7 $F $$ $^ $; $s !# VESA %m !< %+ %k %P %9 MQ $N 5424/26/28/29 $N >l 9g $O !" >u 67 $O $b $C $H I| ;( $G $9 !# %j %K %" %" %I %l %C %7 %s %0 $K $D $$ $F #2 <o N‘ $N 0[ $J $k %? %$ %W $N %+ !< %I $, $" $j $^ $9 : � ISA %P %9 >e $N %+ !< %I $N $h $& $K 16M %P %$ %H 0J 2< $K 3d $j IU $1 $k %+ !< %I !# KX $I $3 $N $h $& $J %+ !< %I $G $7 $g $& !# F1 MM $J @) Ls !J Nc $( $P 16M %P %$ %H $h $j >/ $J $$ %a %b %j $G $J $1 $l $P $$ $1 $J $$ !K $, E, MQ $5 $l $^ $9 !# � A26 $N %" %I %l %9 %i %$ %s $K @\ B3 $7 64M %P %$ %H + 14M %P %$ %H $b $7 $/ $O 64M %P %$ %H $K >o $K 3d $j IU $1 $k %+ !< %I !# $3 $N >l 9g !" ‘ MemBase 0x04e00000 ’ $+ Kt $O ‘ MemBase 0x04000000 ’ $r ;X Dj $7 $^ $7 $g $& !# A26 $r ;} $C $F $$ $k VLB %^ %6 !< %\ !< %I $r 2> Dj $7 $F $$ $^ $9 !# $^ $? $O %+ !< %I $, 0x2000000 $K 3d $j IU $1 $k $H $+ !" 5429 $N $h $& $J :G 6a $N %+ !< %I $O DL >o 0x03e00000 (62M %P %$ %H ) $K 3d $j IU $1 $F $$ $^ $9 !# B? J, !" ;n 9T :x 8m $K Mj $i $J $$ $H $$ $1 $J $$ $G $7 $g $& !# 16M %P %$ %H $h $j >/ $J $$ %a %b %j $J $i $P ‘ 8m $C $? ’ membase $r @_ Dj $9 $k $H %0 %i %U %# %C %/ 2h LL $O I= <( $G $- $^ $; $s $, !" B? J, %3 %s %H %m !< %k !\ %* %k %? %M !< %H !\ %P %C %/ %9 %Z !< %9 $r F1 ;~ $K 2! $9 $H La $C $F $3 $l $^ $9 !# 16M %P %$ %H 0J >e $N %a %b %j $N >l 9g $O !" :G =i $N %? %$ %W $N %+ !< %I !J $H 4V H4 $1 $J VLB %^ %6 !< %\ !< %I $N #2 HV L\ $N %? %$ %W $b !K $G %O %s %0 $7 $^ $9 !J B? J, %O !< %I %j %V !< %H $, <+ H/ E* $K 5/ $j $^ $9 !K !# %+ !< %I $N %? %$ %W $O L\ $G 3N G’ $7 $F J, $+ $j $^ $9 !# %+ !< %I $K A26 %T %s $, $" $l $P !" 64M %P %$ %H 0J >e $K 3d $j IU $1 $k $b $N $G $7 $g $& !# 3N G’ $r 9T $& $K $O !" %+ !< %I $r H4 $$ $F 2< $5 $$ !# VESA %m !< %+ %k %P %9 $N %T %s !J %+ !< %I $N %9 %m %C %H $G $J $$ B& $+ $i 8+ $F %3 %M %/ %? %T %s $N >. $5 $$ J} $N :Y D9 $$ >. JR !K $G !" 1& B& !J A4 $F $N %A %C %W $, <B Au $5 $l $F $$ $k LL !K $r >\ $7 $/ $_ $F $/ $@ $5 $$ !# $3 $3 $K 45 8D $N %T %s $, $" $j $^ $9 !# Fb B& $+ $i 1 $+ $i 45 $^ $G HV 9f $r ?6 $j $^ $9 !J %+ !< %I $N C< $N J} $, 45 HV $G $9 !K !# Fb B& $+ $i ?t $( $F !" 17 HV L\ $N %T %s $, L5 $/ !" 18 HV L\ $+ $i 20 HV L\ $^ $G $O $" $k $H ;W $$ $^ $9 !# 21 HV L\ $, A30 $G !" 22 HV L\ $, A28 !" 23 HV L\ $, A26 $G $9 !# $= $7 $F !" 21 HV L\ $+ $i 23 HV L\ $N %T %s $, L5 $$ >l 9g !" %+ !< %I $O 64M %P %$ %H 0J >e $K 3d $j IU $1 $k $3 $H $O =P Mh $^ $; $s !# 21 HV L\ $H 22 HV L\ $, 6u $$ $F $$ $F !J $^ $? $O N> J} $" $j !K 3n $D 23 HV L\ $, %T %s $, $" $k >l 9g !" 64M %P %$ %H 0J >e $K B? J, 3d $j Ev $F $^ $9 !# %+ !< %I >e $N %T %s $N $= $P $K >. $5 $J 2s O) $, $" $k >l 9g !" $+ $J $j 8+ 9~ $_ $, $" $k $H ;W $$ $^ $9 !# %m !< %+ %k %P %9 >e $N 543x %+ !< %I $O $h $j C1 =c !J Cirrus Logic <R $N winsows $N %I %i %$ %P $, $3 $l $r $D $+ $C $F $$ $^ $9 !K $G $9 $, !" Ld Bj $, L5 $$ $o $1 $G $O $" $j $^ $; $s !# PCI %P %9 >e $N %+ !< %I $G $O !" PCI %+ !< %I $r C5 :: $7 $? $H $- $K <+ F0 E* $K %I %i %$ %P $, FI $_ 9~ $‘ %U %l !< %‘ %P %C %U %! $N 4p Dl %" %I %l %9 $r 3J G< $7 $F $$ $k PCI 9= @. %l %8 %9 %? $r ;} $C $F $$ $^ $9 !# $" $k %7 %9 %F %‘ $G %F %9 %H $7 $? $H $3 $m !" %l %8 %9 %? $O 0xa0000000 $K 3d $j IU $1 $i $l $F $$ $F !" PCI %\ !< %I $+ $i 0x08000000 $r A} J, ;X Dj $G 3d $j Ev $F $k $h $& $K $J $C $F $$ $^ $7 $? !# ‘scanp ci’ %W %m %0 %i %‘ $O PCI 9= @. $r FI $_ =P $7 4p Dl %" %I %l %9 $r 8+ $^ $9 !# VESA %m !< %+ %k %P %9 >e $G $O !" KX $I $N 543x %+ !< %I $O 64M %P %$ %H $N I8 =‘ E* $J 3d $j IU $1 %" %I %l %9 $r ;} $C $F $$ $F !" %* %W %7 %g %s $G 2048M %P %$ %H $H 32M %P %$ %H $r %8 %c %s %Q %T %s $G @_ Dj $7 $^ $9 !# $3 $l $O %+ !< %I $K F1 :- $N ;q NA $K =q $+ $l $F $$ $k $+ !" MS- Windows $N system.ini %U %! %$ %k $K (linearaddr = < o�set in megabytes > Ey $H ) =q $+ $l $F $$ $k $G $7 $g $& !# Cirrus Logic $, B? $/ $N VLB %^ %6 !< %\ !< %I $N <B Au >u 67 $r D4 :: $7 2C $( $? $b $N $G !" $3 $l $i $H 0[ $J $k %" %I %l %9 %T %s $K $O <B Au $7 $J $$ $N $G $9 !J $7 $+ $7 $J $, $i !" H‘ Ey $N =i $a $F $N Windows $N %I %i %$ %P $O $3 $N %+ !< %I $r =g D4 $K $O 07 $( $^ $; $s $G $7 $? !K !# %I %i %$ %P $O MemBase $N ;X Dj $, L5 $$ >l 9g $O I8 =‘ $N 64M %P %$ %H $r 2> Dj $7 $^ $9 !# MemBase $N Nc $r >/ $7 <( $7 $^ $9 : MemBase 0x02000000 32Mb MemBase 0x04000000 64Mb MemBase 0x80000000 2048Mb

6. \CL64XX" %I %i %$ %P 9 16bpp $H 32bpp %b !< %I $O 8B Dj $7 $? !J %9 %/ %m !< %k !" %F %- %9 %H !K $N %" %/ %; %i %l !< %? 5! G= $r ;} $C $F $$ $^ $9 $, $= $l $G $b CY $$ $H 46 $8 $k $+ $b $7 $l $^ $; $s $, !" $= $l $G $b !J 543x $, ;} $C $F $$ $k $h $& $J !K M% =( $J %m !< %+ %k %P %9 %$ %s %? !< %U %’ !< %9 $, == J, =u $1 $K $J $k $G $7 $g $& !# XF86Config $N "Screen" @a $N $J $+ $N !" "Display" 9‘ (subsection) $K Mo des $H 2> A[ 2h LL $N Bg $- $5 $r J, $1 $F F0 $+ $7 $? $$ ?< $5 Kh $K Dj 5A $7 $J $1 $l $P $$ $1 $^ $; $s !# Nc !J 2M %P %$ %H $N %S %G %* %a %b %j $N >l 9g !K $O : Section "screen" SubSection "Display" Depth 8 Virtual 1152 900 ViewPort 0 0 Modes "640x480" "800x600" "1024x768" Option "linear" EndSubSection SubSection "Display" Depth 16 Virtual 1152 900 ViewPort 0 0 Modes "640x480" "800x600" "1024x768" Option "linear" EndSubSection SubSection "Display" Depth 32 Virtual 800 600 ViewPort 0 0 Modes "640x480" "800x600" Option "linear" EndSubSection EndSection 6 \cl64xx" %I %i %$ %P cl64xx %I %i %$ %P $O B? $/ $N %i %C %W %H %C %W MQ $N cl-gd6440 $r %5 %] !< %H $7 $^ $9 !# Nc $( $P !" Sager, ProStar Ey $H T exas Instruments TI4000 %7 %j !< %: $K OEM Ds 6! $5 $l $F $$ $k Nan T an %3 %s %T %e !< %? $N NP9200,NP3600 Ey $r %5 %] !< %H $7 $F $$ $^ $9 !# %I %i %$ %P $O LCD @l MQ %b !< %I !" CR T @l MQ %b !< %I $H LCD $H 30 It CR T %G %# %9 %W %l %$ $r F1 ;~ $K ;H $( $k $h $& $K $9 $k %A %C %W $N ;} $D SimulScan %b !< %I $G F0 :n $7 $^ $9 !# LCD $H SimulScan %b !< %I $N 2r A| EY $O 640x480 $, !" CR T @l MQ %b !< %I $G $O 640x480, 600x800 $H 1024x768 $N I8 =‘ VESA %b !< %I $, %F %9 %H :Q $_ $G $9 !# 1024x768 %$ %s %? %l !< %9 %b !< %I $O %G %P %C %0 $7 $F $^ $; $s $7 !" %F %9 %H MQ 5! $G $b F0 :n $7 $F $^ $; $s !# ;q NA $K $J $C $F $$ $k 6n F0 EE 05 $K 0M B8 $9 $k %I %C %H %/ %m %C %/ $N :G Bg 2T F/ >e 8B $, $" $j $^ $9 !# FC $K 5.0V $G $N :G Bg %I %C %H %/ %m %C %/ $O 65MHz $G 3.3V $G $N :G Bg %I %C %H %/ %m %C %/ $O 40MHz $G $9 !# %I %i %$ %P $O 6n F0 EE 05 $r 3N G’ $7 $F E, @5 $J CM $K :G Bg %I %C %H %/ %m %C %/ $r @) 8B $7 $^ $9 !# $3 $l $, 60Hz $N :F IA 2h B. EY ;~ $N Ls 1024x768 $N :G Bg 2r A| EY $K JQ 49 $5 $l $^ $9 !# Fb B" H/ ?6 4o (frequency generator) $O $3 $l $i $N >e 8B $h $j 9b $$ CM $K %W %m %0 %i %‘ $5 $l $F $$ $F !" %5 !< %P !< $N 5/ F0 ;~ $K =V 4V E* $K %A %C %W $N 2T F/ >e 8B $r D6 $( $k $h $& $J %/ %m %C %/ $r C5 :: $5 $; $^ $9 !# 0l C6 M- 8z $J %/ %m %C %/ $N AH $_ 9g $o $; $, F@ $i $l $? $i !" XF86Config $N Clo cks 9T $K =q $$ $F $* $/ $3 $H $r $* 4+ $a $7 $^ $9 !# $3 $l $r 9T $& $H 5/ F0 $K $+ $+ $k ;~ 4V $, Cx $7 $/ 8: >/ $7 $^ $9 !# %/ %m %C %/ $O X %5 !< %P !< $K -prob eonly $r IU $1 $F <B 9T $9 $k ;v $K $h $C $F F@ $i $l $^ $9 !J -prob eonly $K $D $$ $F >p Js $r $b $C $H CN $j $? $$ >l 9g $O XF ree86 $N %* %s %i %$ %s %^ %K %e %" %k $r ;2 >H $N $3 $H !K !# %G !< %? %V %C %/ $K $O %A %C %W $, %5 %] !< %H $7 $F $$ $k 1 %a %, %P %$ %H $N %S %G %* %a %b %j $N 9= @. $@ $1 $, <( $5 $l $F $$ $^ $9 !# $3 $N Bg $- $5 $O %I %i %$ %P $G D> @\ @_ Dj $7 $F $$ $^ $9 !# I, MW $K 1~ $8 $F !" =i 4| CM $N %a %b %j %5 %$ %: $r XF86Config $K =q $$ $F $* $/ $3 $H $b =P Mh $^ $9 !# $^ $? !" 1M %P %$ %H $N %S %G %* %a %b %j $G Nc $( $P 1024x1024 $N $h $& $J Bg $- $5 $N 2> A[ 2h LL $r ;} $D $3 $H $, $G $- !" $3 $l $O CR T @l MQ $N 2h LL %b !< %I $G ;H MQ 2D G= $G $9 !# $7 $+ $7 !" LCD (LCD $H SimulScan) $r ;H $& $H $- $O $$ $D $G $b %A %C %W $O %S %G %* %a %b %j $N >e 0L $N 0l It $r $= $l <+ ?H $N Fb It $N 2C B. =h

7. \CIRRUS" %I %i %$ %P $G $N >c 32 BP :v $N $^ $H $a 10 M} $N $? $a $K ;H MQ $7 $^ $9 !# => $C $F !" LCD %b !< %I $G 2> A[ 2h LL $r ;H MQ $9 $k $H $- $N :G Bg $N %S %G %* %a %b %j $O Ls 0.75M %P %$ %H $J $N $G Nc $( $P 1024x768 $N $h $& $J 2r A| EY $K $J $k $N $G $9 !# >e 5- $N $h $& $J 2> A[ 2r A| EY $r @_ Dj $7 $? >l 9g $K >. $5 $/ @Z $j <h $i $l $? 2h LL $K 2C B. 2= $5 $l $? NN 0h $, I= <( $5 $l $^ $9 !# 8= :_ !" LCD, CR T $H SimulScan $N 3F 2h LL %b !< %I 4V $N @Z $j BX $( $r %5 %] !< %H $7 $F $$ $^ $; $s $, !" >/ $J $/ $H $b NP9200 $G $O OS $N %V !< %H ;~ !J Nc $( $P Linux $N LILO $G !K BIOS $, L$ $@ ;O F0 $9 $k A0 $K %b !< %I $N A* Br $, =P Mh $k $h $& $K $J $C $F $^ $9 !# XF86Config $K Mo deLine %* %W %7 %g %s $r DI 2C $9 $l $P 2h LL %b !< %I $N A* Br $, X %5 !< %P !< $N Fb It $+ $i F0 E* $K 2D G= $K $J $j $^ $9 !# :G 8e $K !" %I %i %$ %P $O 8= >u $G %A %C %W $N Dc >C Hq EE NO 5! G= $H %9 %/ %j !< %s %; !< %P !< $K $h $C $F 2h LL $, >C $( $F $$ $k $H $- $N LCD $N %P %C %/ %i %$ %H $N >C Et $r %5 %] !< %H $7 $F $$ $^ $; $s !# >- Mh $N %P !< %8 %g %s $G $3 $l $i A4 $F $N 5! G= $, <B 8= $9 $k $3 $H $r 4| BT $7 $F $$ $^ $9 !# CL-GD6420 $K 4X $9 $k Cm 0U ;v 9‘ : %S %G %* %a %b %j $N NL $, ;~ !9 @5 $7 $/ C5 :: $G $- $J $$ >l 9g $, $" $j $^ $9 !# #2 $D $N 2r 7h J} K! $, %I %i %$ %P $N %= !< %9 %3 !< %I $K $" $j !" #1 $D $O Dj 5A $7 $F $7 $^ $& $3 $H $G $9 !# $b $C $H NI $$ J} K! $O Device @a $N VideoRam 9T $K %S %G %* %a %b %j $N NL $r ;X Dj $9 $k $3 $H $G $9 !# CR T Kt $O SIMulscan %b !< %I $G $O I8 =‘ E* $J 640x480 60Mhz $G 25.175 MHz $N %I %C %H %/ %m %C %/ $G $N I8 =‘ %b !< %I D4 @0 $r 9T $C $F 2< $5 $$ !# LCD @l MQ $N %b !< %I $G $O F1 MM $N %b !< %I D4 @0 $r 9T $( $^ $9 $, !" 16.257 MHz $N %I %C %H %/ %m %C %/ $r MQ $$ $F $/ $@ $5 $$ !# I8 =‘ $N 56 Hz 800x600 $b CR T $G %5 %] !< %H $7 $F $$ $^ $9 !# \cl64xx" %I %i %$ %P $G $N cl6440 $K 4X $9 $k Ld Bj $O Randy Hendry < r andy@sgi.c om > ;a $^ $G @h $: :G =i $K O" Mm $7 $F $/ $@ $5 $$ !# 7 \cirrus" %I %i %$ %P $G $N >c 32 BP :v $N $^ $H $a @h $: :G =i $K !" XF86Config $G A* Br $7 $? %b !< %I $r %b %K %? !< $, %5 %] !< %H $7 $F $$ $k $3 $H !" $D $^ $j ?e J? F1 4| $N >e 8B $, @5 $7 $$ $3 $H $r 3N G’ $7 $F $/ $@ $5 $$ !# 25.175 MHz $N %/ %m %C %/ $G I8 =‘ E* $J 640x480x256 !J C1 0l $N ?e J? F1 4| $r 31.5 $K ;X Dj $7 $? >l 9g !K $, 9= @. >e %I %i %$ %P $, F0 :n $9 $k $3 $H $N 3N G’ $+ $i $O $8 $a $k $N $, $* 4+ $a $G $9 !# timing @a $K $3 $N 2r A| EY MQ $N :G 9b $N %I %C %H %/ %m %C %/ $r CV $$ $F !" mo de 9T $N :G =i $K =q $$ $? %b !< %I $, >o $K =i 4| CM $N %b !< %I $H $7 $F MQ $$ $i $l $^ $9 !# $$ $/ $D $+ $N VESA I8 =‘ %b !< %I $N D4 @0 $, $$ $/ $D $+ $N %b %K %? !< $G Ld Bj $r 5/ $3 $7 $^ $9 $N $G Cm 0U $7 $F $/ $@ $5 $$ !J ?e J? F1 4| ?. 9f $r A} $d $7 $F $_ $^ $7 $g $& !" $D $^ $j ?? $s Cf $N #2 $D $N ?t CM $N :9 $r 9- $2 $k !" <c $/ $O A4 $F $N ?e J? F1 4| $N D4 @0 ?t CM $r 16 Kt $O 32 $N G\ ?t $K $J $k $h $& $K A} $d $9 !K !# %S %G %* ?. 9f $, FO $$ $F $$ $k $, !" 2h LL $, F1 4| =P Mh $J $$ >l 9g !# %b %K %? !< $, 07 $( $J $$ %b !< %I $r ;H $C $F $$ $k $N $G $9 !# I8 =‘ $G $J $$ %b !< %I $r ;H $C $F $$ $k >l 9g !" >/ $7 ?t CM $r D> $9 I, MW $, $" $k $+ $b $7 $l $^ $; $s !# %b %K %? !< $, <h $j 07 $( $k I8 =‘ %b !< %I $H I8 =‘ <~ GH ?t $N >l 9g !" ;w $? $h $& $J %b !< %I $H <~ GH ?t $G 0[ $J $k ?t CM $N AH $_ 9g $o $; $r 8+ $D $1 $F $/ $@ $5 $$ !# 9b $$ %I %C %H %/ %m %C %/ $G $N ?e J? %8 %C %? !J IT 0B Dj 46 !K FC $K >e $K %9 %/ %m !< %k $9 $k $h $& $J IA 2h A‘ :n $r 9T $& ;~ $K $3 $N Ld Bj $, 8+ $i $l $^ $9 !# "fifo conservative" %* %W %7 %g %s $r ;n $7 $F $/ $@ $5 $$ !# $3 $l $, <: GT $7 $? $H $- $O !" "fast dram" %* %W %7 %g %s $r ;n $9 $+ !" $h $j Dc $$ %I %C %H %/ %m %C %/ $r ;H $C $F $_ $F $/ $@ $5 $$ !# $3 $l $G $b K~ B- $$ $+ $J $$ >l 9g $O !" "noaccel" %* %W %7 %g %s $+ !" "no bitblt" %* %W %7 %g %s $, B? J, =u $1 $K $J $k $G $7 $g $& !# ‘ GH BG $D ’(‘W a vy’) 2h LL !# 2h LL $N ?e J? MI $l Kt $O A4 BN $N %8 %C %? $, !J IA 2h A‘ :n $K 0M B8 $7 $J $$ $G !K 4V CG $J B3 $/ 8= >] $G $9 !# B? J, !" 9b $9 $. $k %I %C %H %/ %m %C %/ $r ;H $C $F $$ $k $; $$ $G !" 6a $$ <~ GH ?t $N MCLK $H 43 >D $, 5/ $- $F $$ $k 2D G= @- $, $" $j $^ $9 !# $b $C $H Dc $$ %I %C %H %/ %m %C %/ $r ;n $7 $F 2< $5 $$ !# $^ $? !" %b !< %I $N ?t CM D4 @0 $r 9T $C $F !" #2 HV L\ $N ?e J? J} 8~ $N ?t ;z $r $$ $/ $i $+ A} $d $7 $F $_ $F $/ $@ $5 $$ !# <! $O 65MHz $N %I %C %H %/ %m %C %/ $G 1024x768 !J Ls 60 Hz !K $N %b !< %I $, =u $1 $K $J $k $O $: $G $9 !# :

7. \CIRRUS" %I %i %$ %P $G $N >c 32 BP :v $N $^ $H $a 11 "1024x768" 65 1024 1116 1228 1328 768 783 789 818 Clo ck c hip "cirrus" $r MQ $$ $F %W %m %0 %i %^ %V %k %/ %m %C %/ $r ;H MQ $7 $F $$ $k >l 9g $O !" $3 $l $r L5 8z $K $7 $F I8 =‘ CM $N %/ %m %C %/ $N AH $_ 9g $o $; $r ;H $C $F $/ $@ $5 $$ !# 5/ F0 $7 $? 8e $G 2h LL $, Jx $l $k !" ;_ $^ $k !J 2h LL $, ?? $C 0E $K $J $k $+ $b !K !# "noaccel" %* %W %7 %g %s $r ;n $7 $F $_ $^ $7 $g $& !# $b $7 F0 $+ $J $+ $C $? >l 9g !" $$ $/ $i $+ @- G= 8~ >e $N 0Y $K "no bitblt" $r ;n $7 $F $_ $F $/ $@ $5 $$ !# BIOS $N @_ Dj $, Bg >f IW $+ $I $& $+ 3N G’ $7 $F !" FC $K 0xa0000- 0xa� $r %- %c %C %7 %s %0 $7 $J $$ $h $& $K $7 $F $/ $@ $5 $$ !# N" DRAM $N 99 ?7 (hidden DRAM refresh) $r L5 8z $K $7 $F $b NI $$ $G $7 $g $& !# %0 %i %U %# %C %/ A‘ :n $N 8e $N 2h LL $, Jx $l $k !" ;_ $^ $k Kt $O $4 $_ $, ;D $k !# %" %/ %; %i %l !< %? 5! G= $N 0l $D !" Kt $O BitBL T 5! G= $r ;H $C $? $H $- $N %W %m %0 %i %‘ $N %P %0 $K 4X O" $7 $F $$ $k $+ $b $7 $l $^ $; $s !# "noaccel" %* %W %7 %g %s Kt $O "no bitblt" %* %W %7 %g %s $r ;n $7 $F $_ $F $/ $@ $5 $$ !# $^ $? !" BIOS $N @_ Dj $r 3N G’ $7 $F $/ $@ $5 $$ !# %5 !< %P !< $, ‘Blitter timeout’ $H $$ $& %a %C %; !< %8 $r =P NO $9 $k !# F1 $8 @_ Dj $, %@ %V $C $F $$ $^ $9 !# 2h LL $, ?b D> J} 8~ $K <~ $j 9~ $s $G (‘wrapp ed’) $$ $k !# DRAM 9= @. $K Ld Bj $, $" $k $3 $H $r <( $7 $F $$ $^ $9 !# %+ !< %I $K #2 %a %, %P %$ %H $N %a %b %j $r Ek :\ $7 $F $$ $k >l 9g $O !" "no 2mb banksel" %* %W %7 %g %s $+ !" #1 %a %, %P %$ %H $N %a %b %j $@ $1 $r 2> A[ 2h LL $K ;H $& >l 9g !" videoram "1024" $r ;n $7 $F $/ $@ $5 $$ !# C< Kv %& %# %s %I %& $N J8 ;z $, $K $8 $‘ !# I8 =‘ $G $J $$ %S %G %* $N <B Au $K $F Js 9p $5 $l $F $$ $^ $9 !# "no bitblt" %* %W %7 %g %s $r ;H $C $F 2< $5 $$ !# %i %C %W %H %C %W MQ %A %C %W %; %C %H $G 0p :J $, Av $k Kt $O ;_ $^ $k %I %C %H %/ %m %C %/ $, 9b $9 $. $k $? $a !" IA 2h MQ $N BS 0h I} $, $H $F $b >/ $J $/ $J $C $F !J Nc $( $P !" 512K %P %$ %H $N %+ !< %I $G 40MHz $r ;H $& >l 9g !K $$ $k $+ !" !J 5422 $N $h $& $J !K %" %/ %; %i %l !< %? 5! G= $r ;H $C $F $$ $k >l 9g $K 5/ $3 $j $^ $9 !# ;~ !9 J8 ;z $N %I %C %H $, H4 $1 $k !" Ak OH $r F0 $+ $9 $H %I %C %H $N $4 $_ $, =P $k !# B? J, !" 9b $9 $. $k MCLK $N @_ Dj $, 4X 78 $7 $F $$ $^ $9 !J %P %s %/ %b !< %I $, Bg >f IW $G $b %j %K %" %" %I %l %C %7 %s %0 $, 0z $- 5/ $3 $9 $G $7 $g $& !K !# %A %C %W %; %C %H $, G’ <1 $G $- $J $$ !# ;H $* $& $H $7 $F $$ $k %A %C %W %; %C %H $K ;w $? $b $N $r 6/ @) ;X Dj $9 $k $3 $H $r ;n $7 $^ $7 $g $& !# ;~ !9 !" 4V 0c $C $? >. $5 $$ @~ J, !J KX $I $, Gr $$ !K $, 8= $o $l $k %7 %9 %F %‘ $+ $i %S %G %* %a %b %j $X $N BitBL T A‘ :n $K 4X $9 $k Ld Bj $K 4X 78 $7 $F $$ $^ $9 !# $$ $i $$ $i $9 $k >l 9g $O "no imageblt" %* %W %7 %g %s $r ;n $7 $F $_ $^ $7 $g $& !# %F %- %9 %H %b !< %I $, E, @Z $K 2s I| $7 $J $$ $$ $/ $D $+ $N 9= @. $G Js 9p $5 $l $F $$ $^ $9 !# XF ree86 3.1 $N SV GA %5 !< %P !< $N C5 :: $, !" Chipset 9T $G MW 5a $7 $? 543x $N %l %8 %9 %? $N Fb MF $r 2u $7 $? $+ $b $7 $l $^ $; $s !# Ia DL $O %f !< %F %# %j %F %# ( Lin ux $N setfont , runx , restorefont ) $G %F %- %9 %H %b !< %I $O 2s I| 2D G= $G $7 $g $& !#

8. %I %i %$ %P $N JQ 99 E@ 12 Hs >o $K 9b $$ %I %C %H %/ %m %C %/ $G ;6 L! $J %7 %9 %F %‘ 5s F0 $r 5/ $9 %+ !< %I 3n $D !? Kt $O %^ %6 !< %\ !< %I $N @_ 7W $K IT NI $N $" $k >l 9g !" %S %G %* %+ !< %I >e $N 9b $$ %I %C %H %/ %m %C %/ $H %7 %9 %F %‘ Fb $N B> $N It J, !J Nc $( $P %G %# %9 %/ I/O !K $H $N %$ %s %? !< %U %’ !< %9 $, $& $^ $/ $$ $+ $J $$ ;~ $K H/ @8 $9 $k 2D G= @- $, $" $j $^ $9 !# !J $4 $/ $^ $l $K !" 5428 %A %C %W $, PCI $r %5 %] !< %H $7 $J $$ ;~ $K !K $$ $/ $D $+ $N PCI $N 5428 $r 4p $K $7 $? %+ !< %I $G 4Q B, $5 $l $^ $9 !# $= $N B> $N 2h LL IA 2h $K 4X $9 $k Ld Bj $, @8 $8 $? >l 9g $O !" ( "no bitblt" $, =u $1 $K $J $i $J $$ >l 9g $K ) "noaccel" %* %W %7 %g %s $r ;n $7 $F $_ $^ $7 $g $& !# $3 $N J8 =q $K 5- =R $N L5 $$ %I %i %$ %P $K 4X $9 $k Ld Bj !" Kt $O %" %/ %; %i %l !< %? 5! G= $K $D $$ $F %P %0 $r H/ 8+ $7 $? >l 9g $O XF ree86 %A !< %‘ !J 8= :_ !" %I %i %$ %P $N J] <i $O hhanemaa@cs.ruu.nl $G 9T $C $F $$ $^ $9 !K $K O" Mm $r 2< $5 $k $+ !" " c omp.windows.x.i386unix " $H $$ $& %K %e !< %9 %0 %k !< %W $K Ej 9F $7 $F 2< $5 $$ !# 8 %I %i %$ %P $N JQ 99 E@ XF ree86 3.1 $+ $i 0J 2< $N %P %0 $r =$ @5 $7 $^ $7 $? : � %" %/ %; %i %l !< %? 5! G= $N 14 %T %/ %; %k $N I} $N %U %) %s %H $N I= <( $N %P %0 � 8bpp $G %j %K %" %" %I %l %C %7 %s %0 5! G= $r ;H $C $? $H $- $K B> $N VC $+ $i @Z $j BX $( $? $H $- %5 !< %P !< $, 2u $l $k !# � 542x >e $G 16bpp $N ;~ VC @Z $j BX $( $r 9T $C $? $H $- DA C %W %m %0 %i %‘ $, 8G $^ $C $F $7 $^ $& !# � %I %i %$ %P $, %5 !< %P !< $N C5 :: $7 $? >p Js $r 85 $K La $7 $F 543x $N %l %8 %9 %? $N Fb MF $r GK 2u $9 $k !# � 543x $G 8bpp $N ;~ $N %j %K %" %" %I %l %C %7 %s %0 !J 16/32bpp $r 9= @. $7 $h $& $H $9 $k $H <: GT $9 $k !K � 16/32bpp $G $N %O !< %I %& %’ %" %+ !< %= %k $N ?’ IU $1 XF ree 3.1.1 $G $N ?7 5! G= : � $$ $/ $i $+ $N I= <( B. EY $N @- G= 8~ >e !# � 16/32bpp $G $N %9 %/ %m !< %k !? %F %- %9 %H !? EI $j $D $V $7 $N 2C B. 2= !# � %W %m %0 %i %^ %V %k %/ %m %C %/ $N %5 %] !< %H !# � 543x $G $N %a %b %j %^ %C %W %I I/O $N %5 %] !< %H !# � 5434 $G $N 110 MHz $X $N %I %C %H %/ %m %C %/ 8~ >e $N %5 %] !< %H !# � \cl64xx" %I %i %$ %P $G CL6440 $N %5 %] !< %H !# XF ree86 3.1.1 $+ $i $N JQ 99 E@ : � J8 ;z I= <( 5! G= $G $N %a %b %j GK 2u $N =$ @5 !# � CL-GD5434 %l %S %8 %g %s E 0J 9_ $G $N %I %C %H %/ %m %C %/ $r 135 MHz $K 8~ >e !# � 9b %I %C %H %/ %m %C %/ $G $N 2h LL :F I= <( %( %i !< !J %8 %C %? !K $r 2r 7h $9 $k $? $a $N $h $j %P %i %s %9 $N $H $l $? FIF O $N @_ Dj !# � %a %b %j %^ %C %W %I I/O ( " mmio " %* %W %7 %g %s ) $N A‘ :n @- 8~ >e (5429 BP 1~ $N I{ :n MQ $N GS =| ) !# � Ii $N Bg $- $5 $N 6k 7? EI $j $D $V $7 $r 9T $C $? $H $- $N @x :_ E* $J %5 !< %P !< GK 2u $r 2s Hr $9 $k @5 Ev @- %A %’ %C %/ $r DI 2C !#

8. %I %i %$ %P $N JQ 99 E@ 13 � BitBL T %( %s %8 %s $r ;H $o $J $$ $G %9 %/ %m !< %k $r $7 $? ;~ H/ @8 $9 $k I= <( %( %i !< $r =$ @5 !# � 543x PCI $N 4p Dl %" %I %l %9 $N G’ <1 !# � CL-GD5436 $N 8B Dj %5 %] !< %H !# � 5429 BP 1~ $N VLB $N =i 4| CM $N 4p Dl %" %I %l %9 $r 0x03e00000 $H $7 $? !# $XConsortium: cirrus.sgml,v 1.4 95/01/27 16:14:36 kaleb Exp $ $XFree86: xc/programs/Xserver/hw/xfree86/doc/sgml/cirrus.sgml,v 3.10 1995/07/03 08:50:57 dawes Exp $ $3 $N %U %! %$ %k $O xc/programs/Xserver/h w/xfree86/doc/sgml/cirrus.sgml,v 3.10 1995/07/03 08:50:57 $r !" 2, K\ 0l 9, ( Kazuyuki Ok amoto < ikko-@p aci�c.rim.or.jp > (mailto:ikko-@pacific.rim.or.jp) ) $, XF ree86 3.1.2 $r F| K\ $G %$ %s %9 %H !< %k $9 $k ?M 8~ $1 $K OB Lu $7 $? $b $N $G $9 !# $3 $3 $, $* $+ $7 $$ $H $+ !" $3 $3 $O $3 $& $7 $? $[ $& $, $$ $$ $H $$ $C $? $4 0U 8+ $, $" $j $^ $7 $? $i !" EE ;R %a !< %k $G $* CN $i $; 2< $5 $$ !# 86 J8 $N Cx :n 8" $O XF ree86 %W %m %8 %’ %/ %H <R $K $" $j $^ $9 !# $3 $N OB Lu $N Cx :n 8" $O XF ree86 %W %m %8 %’ %/ %H <R $H 2, K\ !! 0l 9, $K $" $j $^ $9 $, !" $3 $N OB Lu $N IT 6q 9g $O ;d $K !" EE ;R %a !< %k $G Aw $C $F 2< $5 $$ !# $XFree86: xc/programs/Xserver/hw/xfree86/doc/sgml/Japanese/cirrus.sgml,v 3.1 1995/09/16 08:31:09 dawes Exp $ [EOF]