NORDUnet – The Nordic Backbone Network

Address:

NORDUnet B c/o UNI-C ygn. 305, DTH y D DK-2800 Lyngb

ENMARK

Email: Peter.Villemoes@uni-c.dk

Phone: +45 45 938355

FAX: +45 45 930220

N Description

ORDUnet is a collaboration between the national research networks in Denmark, Finland, c Iceland, Norway and Sweden. Its purpose is to provide the national research and education ommunities with an efficient networking service which ensures coherence of the national R & N D networks and connects these to similar networks in the rest of Europe and the world.

ORDUnet is organized as a consortium agreement between the national networks DENet, D FUNET, SUNET, SURIS and UNINETT. The administration is an integral part of UNI-C in enmark.

NORDUnet has contracted its work mainly to the national organizations. The network opera- - v tions center has been contracted to KTH/SUNET. It is their responsibility to monitor the ser ice, configure the Cisco routers (IP) as well as coordinate operational issues. The X.25 opera- l c tions have been contracted to UNINETT and DECNET operations to UNI-C. Overall technica oordination has been contracted to VTKK/FUNET. . NORDUnet has five points of presence, one in each of the Nordic countries

UNI-C Building 305 DTH D DK-2800 Lyngby

ENMARK K T FUNET/VTK ietotie 6 F Espoo inland U SURIS

niversity of Iceland k I Dunhaga 5 IS-107 Reykjavi celand SINTEF/DELAB T N-7034 rondheim Norway

The information in this section is provided in accordance with the copyright notice appearing at the front of this guide.

September 4, 1992 NNSC Section 5.19, Page

KTH/SUNET S S-100 44 tockholm N Sweden ORDUnet provides IP, DECNET, X.25 and CLNS layer 3 services, in this order of volume. p NORDUnet leases bandwidth in form raw lines and adds value by providing the network layer rotocols in a coordinated fashion with equipment operated through various contracts. The p national networks which are the NORDUnet customers see it as a "NORDUnet plug" which rovides different service "pins".

NJE traffic is transported over TCP/IP. The CLNS (including DECNET Phase V) pilot traffic b is carried by the same Cisco’s as the production traffic. The external connections are mainly ased on Cisco routers. NORDUnet runs IP and CLNS protocols to the US and IP, CLNS and e I DECNET IV to Europe. X.25 connectivity to Europe is provided via a direct connection to th XI network.

There are app. 60.000 IP hosts, 5000 DECnet hosts, and 100 EARN hosts in the Nordic l N national networks that are interconnected by NORDUnet. NORDUnet connects the nationa ordic networks to Internet, Ebone, EASInet, EARN/BITNET, EUnet, HEPnet, SPAN and

W IXI.

ho Can Use the Network NORDUnet can only be used for academic and research traffic.

D References

ocuments available by anonymous ftp and gopher from nic.nordu.net

September 4, 1992 NNSC Section 5.19, Page