Stable Implementation

Agreements for Open Systems

Interconnection Protocols:

Part 4 - Transport

Output from the June 1991 NIST Workshop for

Implementors of OSI

SIG Chair: Fred Burg

SIG Editor: Kristy Brown Workshop Editor: Brenda Gray

Foreword

This part of the Stable Implementation Agreements was prepared by the Lower Layers Special Interest

Group (LLSIG) of the National Institute of Standards and Technology (NIST) Workshop for Implementors

of Open Systems Interconnection (OSI). See Procedures Manual for Workshop charter.

Text in this part has been approved by the Plenary of the above-mentioned Workshop. This part replaces

the previously existing chapter on this subject.

Future changes and additions to this version of these Implementor Agreements will be published as change

pages. Deleted and replaced text will be shown as strikeout. New and replacement text will be shown as

shaded.

Table of Contents

Part 4 - Transport . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1

0 Introduction . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1

1 Scope . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1

2 Normative References . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1

2.1 CCITT . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1

2.2 ISO . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1

3 Status . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 2

4 Errata . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 2

5 Provision of Connection Mode Transport Service . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 2

5.1 Transport Class 4 . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 2

5.1.1 Transport Class 4 Overview . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 2

5.1.2 Protocol Agreements . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 3

5.1.2.1 General Rules . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 3

5.1.2.2 Transport Class 4 Service Access Points or Selectors . . . . . . . . . . . . . 5

5.1.2.3 Retransmission Timer . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 5

5.1.2.4 Keep-Alive Function . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 6

5.1.2.5 Congestion Avoidance Policies . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 8

5.1.2.6 Use of Priority . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 9

5.2 Transport Class 0 . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 10

5.2.1 Transport Class 0 Overview . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 10

5.2.2 Protocol Agreements . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 10

5.2.2.1 General Rules . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 10

5.2.2.2 Transport Class 0 Service Access Points . . . . . . . . . . . . . . . . . . . . . . . 10

5.2.3 Rules for Negotiation . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 10

5.3 Transport Class 2 . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 11

5.3.1 Transport Class 2 Overview . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 11

5.3.2 Protocol Agreements . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 11

6 Provision of Connectionless Transport Service . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 11

6.1 Connectionless Transport Overview . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 12

6.2 Protocol Agreements . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 12

6.2.1 General Rules . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 12

6.2.2 Connectionless Transport Service Access Points or Selectors . . . . . . . 12

7 Transport Protocol Identification . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 12

List of Figures

Figure 1 - AK exchange on idle connection. . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 7

List of Tables

Table 1 - Protocol Identification TPDU Values . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 12

Part 4 - Transport

0 Introduction

These agreements support the integration of LANs, packet networks, and other WANs with the smallest

possible set of mandatory protocol sets, in accordance with the other agreements already reached. Nothing

here shall preclude vendors from implementing protocol suites in addition to the ones described in this

document.

1 Scope

This chapter presents agreements for providing the OSI Transport layer services over both connection

mode and connectionless mode services.

2 Normative References

2.1 CCITT

[1] Recommendation X.214 (Blue Book, 1988), Transport Service Definition for Open Systems

Interconnection for CCITT Applications.

[2] Recommendation X.224 (Blue Book, 1988), Transport Protocol Specification for Open Systems

Interconnection for CCITT Applications.

2.2 ISO

[3] ISO 8072, Information processing systems - Open systems interconnection - Transport service

defintion.

[4] ISO 8072 Addendum 1, Information processing systems - Open systems interconnection -

Addendum 1: Transport service definition - Connectionless-mode transmission.

[5] ISO 8073 Edition 2, Information processing systems - Open systems interconnection - Connection

oriented transport protocol specification.

[6] ISO 8073 Addendum 1, Information processing systems - Open systems interconnection -

Connection oriented transport protocol specification - Addendum 1: Network connection

management subprotocol.

[7] ISO 8073 Addendum 2, Information processing systems - Open systems interconnection -

Connection oriented transport protocol specification - Addendum 2: Class four operation over

connectionless network service.

[8] ISO 8602, Information processing systems - Open systems interconnection - Protocol for providing the connectionless-mode transport service.

3 Status

Completed December 1990.

4 Errata

NOTE - This clause may contain "defect report" and resolutions material, and the versions of implementor

agreements to which this material applies.

5 Provision of Connection Mode Transport Service

Three connection mode protocol classes have been identified for implementation. Transport classes 0, 2

and 4 of X.224 (1988)

1

have been endorsed for use over CONS. Only Transport Class 4 of ISO 8073/Add.

2

2

has been endorsed for use over CLNS. The following class combinations are endorsed for CONS: (0),

(0,2) or (0,2,4).

5.1 Transport Class 4

5.1.1 Transport Class 4 Overview

Transport Class 4 is mandatory for communication between systems using the OSI CLNS and may also

be used for systems using the OSI CONS (e.g., a private MHS, etc.).

1

Where a CR TPDU proposing Class 2 or 4 is initiated, Class 0 shall be explicitly indicated as an

alternative class except if there is already one (or several) transport connection(s) assigned to the

network connection (multiplexing being possible).

2

In general, references to ISO 8073 in ISO 8073/Add. 2 should be interpreted as applying to X.224

(1988); however, the reference to Clause 14.6.a in Clause 14 of ISO 8073/Add. 2 should be

interpreted as a reference to Clause 14.5.a of X.224(1988).

5.1.2 Protocol Agreements

A disconnect request shall be issued in response to a connect request when the maximum number of

Transport connections is reached or exceeded.

5.1.2.1 General Rules

The rules are as follows:

a) All implementations shall request "use of extended formats" in the CR TPDU. Implementations

shall accept the "use of extended formats" in the CC TPDU if it was proposed in the CR TPDU.

Implementations shall accept "use of normal formats" if it was proposed in the CR TPDU;

b) Negotiation of protection is outside the scope of these agreements. If negotiation of protection

is not supported, receipt of the protection parameters in CR TPDU and CC TPDU shall be ignored;

c) Implementations shall be capable of proposing and accepting the non-use of checksums;

d) Use of the acknowledgment time parameter is optional. If an implementation is operating any

policy which delays the transmission of AK TPDUs, the maximum amount of time by which a single

AK TPDU may be delayed shall be indicated to the peer Transport service provider using the

acknowledgment time parameter. The value transmitted should be expressed in units of

milliseconds and rounded up to the nearest whole millisecond;

e) QoS negotiation is outside the scope of these agreements. If QoS negotiation is not supported,

receipt of the parameters "throughput", "residual error rate", "priority", and "transit delay" in the CR

and CC TPDUs shall be ignored;

f) It is recommended that implementations not send user data in the CR TPDU or the CC TPDU.

The disposition of any user data received in a CR TPDU or CC TPDU is implementation

dependent;

g) It is recommended that implementations not send user data in the DR TPDU. The disposition

of any user data received in a DR TPDU is implementation dependent;

h) An unknown parameter in any received CR TPDU shall be ignored;

i) A Transport entity shall accept a DR TPDU and a corresponding DC TPDU with or without a

checksum in response to a CR or CC TPDU;

j) Transmitted DR TPDUs shall carry a disconnect reason code which pertains to the actual cause

of the disconnect. A DR TPDU may carry a reason code of "0" (unspecified) if an appropriate

reason code is not defined;

k) Known parameters with valid lengths but with invalid values in a CR TPDU shall be handled

as follows:

1) Parameter; 2) Action:

a) TSAP id a) Send DR TPDU

b) TPDU size b) ignore parameter, use default

c) Version c) ignore parameter, use default

d) Checksum d) discard CR TPDU

e) Alternate Protocol Classes e) Protocol Error

l) Unrecognized or not applicable bits of the Additional Options parameter shall be ignored.

m) It is recommended that the capability of request acknowledgments be supported and proposed

in CR TPDUs. If request acknowledgments are supported, then if the implementation delays

acknowledgments it shall:

1) request use of request acknowledgments in the CR TPDU;

2) accept the use of request acknowledgments in the CC TPDU if it was proposed in the

CR TPDU.

n) It is recommended that implementations send both the preferred and existing TPDU size

parameters in the CR TPDU.

o) It is recommended that inactivity timer values be exchanged during connection establishment.

This may be mandatory in the future. If the "exchange of inactivity timers" capability is supported,

the implementation shall send its minimum inactivity timer in the CR TPDU. If a CR TPDU is

received with this timer value and the capability is supported, the responding CC TPDU shall

contain the inactivity time.

If the Inactivity time is received and the capability is supported, the following shall be used as an upper

bound for W:

(I

R

-E

LR

)/N > W N > 2

5.1.2.2 Transport Class 4 Service Access Points or Selectors

If present, the TSAP Id. field in the CR and CC TPDUs shall be encoded as a variable length field and will

be interpreted as an octet string. The length of the string cannot exceed 32 octets.

5.1.2.3 Retransmission Timer

It is recommended that the value used for the retransmission timer be based upon the round-trip delay

experienced on a transport connection. The implementation should maintain, and continually update, an

estimate of the round-trip delay for the TC. From this estimate, a value for the retransmission timer is

calculated each time it is started. Example techniques for maintaining the estimate and calculating the

retransmission timer are described below. Example 1 represents a simple retransmission strategy and

example 2 is particularly suitable for networks subject to high traffic loads.

Example 1

The value of the retransmission timer may be calculated according to the following formula:

T1 < kE + AR.

In this formula, E is the current estimate of the round-trip delay on the transport connection, AR is the value

of the acknowledgment time parameter received from the remote transport service provider during

connection establishment, and k is some locally administered factor.

A value for k should be chosen to keep the retransmission timer sufficiently small such that lost TPDUs will

be detected quickly, but not so small that false alarms are generated causing unnecessary retransmission.

The value of E may be calculated using an exponentially weighted average based upon regular sampling

of the interval between transmitting a TPDU and receiving the corresponding acknowledgment. Samples

are taken by recording the time of day when a TPDU requiring acknowledgment is transmitted and

calculating the difference between this and the time of day when the corresponding acknowledgment is

received. New samples are incorporated with the existing average according to the following formula:

E < E + (1 - a)(S - E).

In this formula, S is the new sample and a is a parameter which can be set to some value between 0 and 1. The value chosen for a determines the relative weighting placed upon the current estimate and the new

sample. A large value of a weights the old estimate more heavily causing it to respond only slowly to

variations in the round-trip delay. A small value weights the new sample more heavily causing a quick

response to variations. (Note that setting a to1willeffectivelydisablethealgorithmandresultinaconstant

value for E, being that of the initial seed.) If a is set to 1-2^{-n}for some value of n, the update can be reduced to a subtract and shift as shown below:

E < E + 2-n(S - E).

When sampling, if an AK TPDU is received which acknowledges multiple DT TPDUs, only a single sample should be taken being the round-trip delay experienced by the most recently transmitted DT TPDU. This

attempts to minimize in the sample any delay caused by the remote transport service provider withholding

AK TPDUs.

Example 2

As network load increases, the variability of round-trip delay also increases. In environments where load

fluctuates widely, it is therefore useful to estimate the variability of round-trip delay measurements and use

this estimate in the calculation of retransmission timer values. An estimate of the variability of round-trip

delay measurements can be efficiently calculated as an exponentially weighted average of the differences

between round-trip delay measurements and the average round-trip delay. This represents the mean

deviation of the round-trip delays, which is a useful approximation of the standard deviation and can be

much more efficiently computed. The formula is

D <-- D + (1 - a)(|S - E| - D)

where D is the estimate of variability in round-trip delays. S, E, and a are as defined for the preceding

formula. As before the value of a must be between 0 and 1 and the choice of a value of 1 - 2

-N allows for efficient update of the average. The value of a for the variability estimation, though, does not need to be the same as that used for the round-trip delay estimate. A smaller value for a is useful in the variability estimation to cause a more rapid response to changes in round-trip delays. D can then be used to calculate

retransmission timer values according to the formula:

T1 <-- E + AR + kD

where T1 is the retransmission timer value, E is the estimated average round-trip delay, AR is the value

of the acknowledgment timer parameter received from the remote transport service provider during

connection establishment, and k is a locally administered factor. Since D approximates the standard

deviation of the round-trip delays, but is greater than or equal to the standard deviation, round-trip delays within k standard deviations of the mean would be accounted for by the retransmission timer value (e.g.,

k = 2, if round-trip delays were normally distributed, would account for 95% of the variability).

Round-trip time measurements based on acknowledgment of any retransmitted data should not be used

to update the round-trip delay estimate or the estimate of variability. Such measurements are not reliable

since it is ambiguous which transmission of the data is being acknowledged.

One strategy for handling a retransmission timeout is to retransmit the PDU and reset the timer with a value

that is twice the previous value. In this case, a new roundtrip delay estimate and estimate of variability

should be calculated only when an acknowledgment of data is received where none of the acknowledged

data has been retransmitted. This calculation uses the new round-trip delay measurement and the last

estimate before the retransmission timeout(s).

5.1.2.4 Keep-Alive Function

The Class 4 protocol detects a failed Transport connection by use of an ’inactivity timer’. This timer is reset each time a TPDU is received on a connection. If the timer ever expires, the connection is terminated.

The Class 4 protocol maintains an idle connection by periodically transmitting an AK TPDU upon expiration of the ’window timer’. Thus, in a simple implementation, the interval of one transport entity’s window timer

must be less than that of its peer’s inactivity timer, and vice versa. The following agreements permit

communicating transport entities to maintain an idle connection without shared information about timer

values:

a) In accordance with ISO 8073/X.224, Clause 12.2.3.9.a, all implementations must respond to

the receipt of a duplicate AK TPDU not containing FCC by transmitting an AK TPDU containing the

’flow control confirmation’ parameter;

b) Implementations must always transmit duplicate AK TPDUs without FCC on expiration of the

local window timer (see ISO 8073/X.224, Clause 12.2.3.8.1). Receipt of this TPDU by the remote

Transport entity will cause it to respond with an AK TPDU containing the ’flow control confirmation’

parameter. When this is received by the local transport entity, it will reset its inactivity timer. See

figure 1;

c) It is a local matter for an implementation to set the intervals of its timers to appropriate relative

values. Specifically:

1) The window timer must be greater than the round-trip delay. See 5.1.2.3;

2) The inactivity timer must be greater than two times the window timer; and should

normally be an even greater multiple if the Transport connection is to be resilient to the

loss of an AK TPDU.

A duplicate AK TPDU (see figure 1) is one which contains the same values for YR-TU-NR, credit, and

subsequence number as the previous AK TPDU transmitted. A duplicate AK TPDU does not acknowledge

any new data, nor does it change the credit window. I W

duplicate expire AKAK + FCC reset duplicate expire AK

AK + FCC reset expire

Figure 1 - AK exchange on idle connection. 7

5.1.2.5 Congestion Avoidance Policies

This clause defines both mandatory and optional requirements relating to avoiding congestion in OSI networksandrecoveringfromitwhenitisexperienced.Themandatoryrequirementsspecifyaminimum approachtocongestionavoidance/recoverywhichcanbetunedbaseduponthespecificrequirementsof thenetwork.Theoptionalrequirementsspecifyadynamicwindowsizingschemewhich,ifimplemented, willcontributefurthertotheavoidanceofcongestioninthenetwork.

MandatoryRequirementsareasfollows:

a) A maximum size for the "receive credit window", the value of which is locally configurable, shouldbeprovided.A"receivecreditwindow"reflectsthenumberofcreditssentbyaTransport entity for a Transport connection. The maximum size of the "receive credit window" shall be referredtoasWR 1; b) Amaximumsizeforthe"sendingcreditwindow",thevalueofwhichislocallyconfigurable,shall beprovided.A"sendingcreditwindow"reflectsthenumberofdataTPDUsthataTransportentity is willing to send on a Transport connection. The maximum size of the "sending credit window" shallbereferredtoasWS 1

. As specified in ISO 8073, the "sending credit window" shall also be

less than or equal to the remote "receive credit window" as conveyed in the last CDT field;

c) It is strongly recommended that an implementation use a retransmission timer per Transport

connection. If, upon expiration of the retransmission timer, an implementation allows more than "1"

TPDU to be transmitted a means to locally adjust the maximum number shall be provided;

d) All implementations shall have the capability of operating without delaying ACKs of data TDPUs

received in-sequence (i.e., A

L essentially equals zero). If an implementation optionally chooses to

explicitly delay ACKs, a means to locally adjust A Lshall be provided.

Optional Requirements are as follows:

Forsystemsimplementingthedynamicwindowsizingschemethefollowingrulesapplyasdescribedbelow:

1. RECEIVING TRANSPORT ENTITY (RTE) RULES:

a) Rule 1 - Initialization of Window:

1) The initial value of WR (knownas WR 0) shall have alocally configurable upper bound.

Thiswindowissenttothesendingtransportentity(STE)inthenextCDTfieldtransmitted;

a) Rule 2 - Required Sampling Period:

1) All RTEs shall maintain a fixed value for WR until the next 2WR DT TPDU arrive since the last CDT field was transmitted by the RTE;

b) Rule 3 - Required Counting of Received TPDUs in a Sampling Period:

1) All RTEs shall maintain a count, N, equal to the total number of TPDUs received and a count, NC, equal to the total number of TPDUs 8

received which had the CE Flag set. All types of TPDUs are included in the counts for N and NC, not just DT TPDUs;

c) Rule 4 - Required Action upon the end of a Sampling Period: All RTEs shall take the following actions at the end of each sampling period:

1) If the count NC is less than 50 percent of the count N, the RTE shall increase WR by adding 1 up to a maximum, WR1, (that is based on the local buffer management policy); otherwise, it shall decrease WR by multiplying by 0.875 (a minimum of 1); 2) Reset N and NC to zero; 3) Transmit the new window WR in the next CDT field sent to the sending transport entity;

2) SENDING TRANSPORT ENTITY (STE) RULES:

a) Rule 1: Initialization of Window:

1) All STEs shall maintain a sending window size (WS). Initially and also as long as there is no loss, WS is set equal to the receiving window value WR received from the remote RTE in the last CDT field;

b) Rule 2: Required Action on a Timeout;

1) All STEs shall reset WS to one when the retransmissions timer expires and indicates a lost TPDU. WS now limits the number of DT TPDUs that may be transmitted or retransmitted without further acknowledgments;

c) Rule 3: Required Counting of Acknowledged TPDU:

1) All STEs shall maintain a count, ACKRCVD of the number of DT TPDUs acknowledged, by the RTE, since WS was last adjusted. Therefore each time WS is adjusted, the count ACKRCVD shall be reset to zero;

d) Rule 4: Increase Window Policy:

1) All STEs shall increase WS by one each time ACKRCVD is equal to or greater than the current value of WS, unless WS exceeds the window permitted by the remote RTE.

5.1.2.6 Use of Priority

(Refer to the Working Implementation Agreements).

PART 4 - TRANSPORT June 1991 (Stable)

5.2 Transport Class 0

5.2.1 Transport Class 0 Overview

TransportClass0overX.25ismandatory(seeX.400)foruseincommunicatingwithpublicMHSsystems operatinginaccordancewiththeCCITTX.400seriesrecommendations.Thepurposeoftheagreements concerningTransportClass0istoallowconnectiontothesepublicservices.TransportClass0overX.25 canalsobeusedincommunicatingbetweenPRMDs(thischoiceisprevalentoutsideNorthAmerica).

5.2.2Protocol Agreements

5.2.2.1 General Rules

Transport Class 0 agreements are as follows:

a) The Error (ER) TPDU may be used at any time and upon receipt requires that the recipient

disconnect the network connection, and by extension the transport connection;

b) The allowed values for the maximum TPDU size are 128, 256, 512, 1024, and 2048;

c) The Class 0 protocol does not support multiplexing. At any instant, one Transport corresponds

to one Network connection;

d) It is recommended that the optional timers TS1 and TS2, if implemented, be settable by local

system management. Values in the order of minutes should be supported;

e) An unlimited TSDU length must be supported.

f) It is recommended that implementations send both the preferred and existing TPDU size

parameters in the CR TPDU.

5.2.2.2 Transport Class 0 Service Access Points

For communicating with public MHS systems, section 5 of X.410 specifies the use and format of TSAP identifiers.

5.2.3 Rules for Negotiation

The rules for class negotiation shall be used.

PART 4 - TRANSPORT June 1991 (Stable)

5.3 Transport Class 2

5.3.1 Transport Class 2 Overview

TransportClass2isapplicableinOSIendsystemswhichprovidetheConnection-modeNetworkService.

5.3.2ProtocolAgreements TransportClass2agreementsfollow:

a) ThevaluesoftheTS1andTS2timersshallbeconfigurable.Therecommendedtimervalues are:

1) TS1:60seconds; 2) TS2:60seconds;

b) Ifpresent,theTSAP-idfieldintheCRandCCTPDUsshallbeencodedasavariablelength fieldandwillbeinterpretedasanoctetstring.Thelengthofthestringcannotexceed32octets; c) Therulesforclassnegotiationshallbeused; d) QoSnegotiationisoutsidethescopeoftheseagreements.IfQoSnegotiationisnotsupported, receiptoftheparameters"throughput","residualerrorrate","priority",and"transitdelay"intheCR andCCTPDUshallbeignored.

NOTE - If Class 0 is indicated in the Alternative Protocol Class field and QoS parameters are conveyed and

the responding end system chooses Class 0, then the QoS parameters have been ignored by the responding

system.

e) It is recommended that implementations send both the preferred and existing TPDU size

parameters in the CR TPDU.

6 Provision of Connectionless Transport Service

ISO 8072/Add. 2 is the Transport Service Definition covering Connectionless-mode Transmission. ISO 8602 is the Protocol for providing the Connectionless-Mode Transport Service.

6.1 Connectionless Transport Overview When providing the connectionless Transport Service, the protocol shall be implemented as specified in ISO 8602.

6.2 Protocol Agreements

6.2.1 General Rules

The connectionless Transport protocol is a relatively simple protocol providing little opportunity for conflicting interpretations. A few relevant agreements follow:

a) The optional elements of procedure for use of CLTS over CONS (i.e., clause 6.3 of ISO 8602) will not be supported;

b) A Unitdata TPDU that is received that contains a protocol error or an unknown destination TSAP ID shall be discarded.

6.2.2 Connectionless Transport Service Access Points or Selectors

The TSAP selector field in the UD TPDU shall be encoded as a variable length field and will be interpreted as an octet string. The length of the string cannot exceed 32 octets.

7 Transport Protocol Identification

The absence of Call User Data (CUD) in an X.25/ISO 8208 Call Request/Incoming Call packet indicates

the operation of ISO 8073/CCITT X.224.

Protocol Identification TPDU values applicable to these agreements are given in table 1. These TPDUs,

when used, are conveyed as N-connect user data.

Table 1 - Protocol Identification TPDU ValuesTPDUValue

Protocol 03 01 01 00*

ISO8073/Add.1 (seenote1) 03 01 02 00**

ISO8602 (seenote2)

NOTES 1 CorrespondstoanISO8073/Add.1UN-TPDUandaX.224AnnexBPI-TPDU. 2 CorrespondstoanISO8073/Add.1UN-TPDU.

Thefollowingagreementsapply:

a) AnyadditionalTPDU,whichfollows(byconcatenation)aProtocolIdentificationTPDUshallbe ignoredifISO8073/Add.1isnotsupported; b) WhenusingISO8208,usageofaProtocolIdentificationTPDUnotcorrespondingtothose listedintable1isoutsidethescopeoftheseagreements.