

	To INSTALL the new version 5.5 MDTS program and support files
	Place the distribution disk number ONE in your floppy drive.

	Enter the DOS command to "change" to the floppy drive.
	 - such as entering A: (type A: and press enter key)

	Enter the command INSTALL to start the installation program.

	READ ALL OF THE MESSAGES ON THE SCREEN AND FOLLOW INSTRUCTIONS.

	Install version 5 into the same directory as version 4 -- the
	new version uses the same data files as the old version.  Get
	back to your hard disk and change to your MDTS directory, and
	then enter the command M5 to start the new program.

	After (AND ONLY AFTER!) you are sure version 5 will run on your
	computer, you may delete the M4.EXE program.  Version 5 requires
	DOS 3.1 or later, and more memory than version 4 does, so don't
	delete version 4 until you are SURE version 5 runs OK.

	To print the manual, enter (must have your printer ON) the DOS
	command COPY M5.TXT PRN.  (approximately 125 pages long)

	M5 is compiled with Clipper 5.2c, and has "internal" overlays
	in the 700000+ bytes program.  According to the Clipper manual,
	and the compiler messages, this program should run with 512k
	of AVAILABLE memory.  Enter CHKDSK to find your available memory.

	If the M5 program does NOT run in your computer, return all of
	the disks and materials, along with a note, for a refund.

