             INSTALL OS/2 2.1 for a B: 3 1/2" diskette
           for the UN-COMPRESSED version (BLUE diskettes)

You will find 2 files in the package. You will ONLY need them if your
ORIGINAL diskettes are BLUE colored. If they are SALMON, you need the
INS21M.ZIP file.

These are 5.25" diskette images of the install disk and disk 1 for installing
from B where the user has a 5.25 A drive but a 3.5 B drive.

You will also need the IBM LOADDF.ZIP file as that utility is need to
uncompress the .DSK files. Create the 5 1/4" diskettes from the following
DSK images, and then boot the system with the INS diskette, and follow
directions. You will need to use both drives, the newly created ones in the
A: drive, and the original shipped 3 1/2" diskettes in the B: drive.

INSTL_L  DSK  1012240   6-16-93   1:02p <---- Install Diskette
BINSTL_L DSK   877920   6-16-93  12:57p <---- Diskette #1
