<  Installation instructions for Warp FixPak XR_W017















  

  
  



  Build level 8.241  (2nd release)
  
  
  Supported CSD levels
  
  XR_3000 Warp for Windows
  XR_3001 Warp with WIN-OS/2
  XR_3002 Warp for Windows Manufacturing Refresh
  XR_3003 Warp with WIN-OS/2 Connect
  XR_3004 Warp for Windows Manufacturing Refresh Connect
  XR_3005 Warp with WIN-OS/2 Server
  
  
  OS/2 Fix Distribution
  Personal System Products
  Boca Raton, Fl
  
  
  (c) Copyright International Business Machines Corporation, 1996.
  All rights Reserved.

  January 25 1996 Warp FixPak XR_W017



                    January 25 1996 Warp FixPak XR_W017

  CONTENTS


    Terms and Conditions ............................................. 1

    Who should not install this FixPak ............................... 2

    Installation Notes ............................................... 3
      Do not use your system once the FixPak installation is started . 3
      What is the SIQ (Single Input Queue) feature ................... 3
        How it works ................................................. 3
      Popup message about newer file on harddisk than is in FixPak ... 4
      Common File Dialog Interface changes ........................... 4
      Dell machines and font editing ................................. 4
    Corrective Service Facility Boot Diskettes ....................... 5
    Read-Only files .................................................. 6

    Relocated OS/2 file support ...................................... 7

    Installation Process ............................................. 8
    Method 1: Install from booted OS/2 partition.  ................... 8
    Method 2: Boot from Corrective Service Disk 1.  ................. 10
    Additional Corrective Service Facility information .............. 10

    Recovering from Installation problems ........................... 11
      No files to service ........................................... 11
      Previous installation interrupted ............................. 12
      Unable to open Archive directory .............................. 12

    System problems after FixPak installation ....................... 13
      OS/2 is unable to operate your hard disk or diskette drive.  .. 13
      RIPL failure .................................................. 14
      Updating systems with the CMD chipset ......................... 15
      RZ1000 and CMD640 Data Problems (APAR=PJ19409) ................ 15
      SYS3175 when opening LS 4.0 Lan Server Administration ......... 17
      Traps when canceling print jobs after FixPak is installed ..... 18
      Novell Requester .............................................. 18
      CC:Mail for OS/2 .............................................. 18
      Rapid Resume Fix .............................................. 18
      No Window list when you press Ctrl+Esc ........................ 19
      IBM CODE/400 at V3R1M0 level .................................. 19
      Problems with Visual REXX applications ........................ 19
      TCP/IP at level WR08152 ....................................... 20
      DOSCALL1.DLL Error ............................................ 20

    CSD level of SYSLEVEL.OS2 ....................................... 21
    List of problems fixed in the FixPak ............................ 21

    Where Fixes can be found ........................................ 22

    FixPak Corrective Service levels and disk layouts ............... 23

  
                                                            Contents  ii


                    January 25 1996 Warp FixPak XR_W017


    Space Utilization ............................................... 32


















































  
                                                           Contents  iii


                    January 25 1996 Warp FixPak XR_W017

  TERMS AND CONDITIONS

                          IMPORTANT
                          ---------
  IMPORTANT - PLEASE READ THE FOLLOWING TERMS AND CONDITIONS.
  DOWNLOADING THE FixPak XR_W017 SERVICE FIXES THAT FOLLOW
  INDICATES YOUR ACCEPTANCE OF THE FOLLOWING TERMS AND CONDITIONS:


   A)  YOU MUST BE, AND AGREE THAT YOU ARE, A CURRENT LICENSEE OF
        OS/2;

   B)  YOU MAY MAKE COPIES OF THE OS/2 SERVICE FIXES EQUAL TO THE
        NUMBER OF LICENSED COPIES OF OS/2 YOU POSSESS;

   C)  YOU MAY ONLY USE THE SERVICE FIXES INCLUDED WITH FixPak XR_W017
        FOR MAINTENANCE PURPOSES;

   D)  YOU MAY ONLY USE THE WIN-OS/2 SERVICE FIXES INCLUDED WITH FixPak
        XR_W017 TO MAINTAIN COPIES OF OS/2 WITH WIN-OS/2;

   E)  ALL OTHER TERMS AND CONDITIONS OF YOUR OS/2 LICENSE
       AGREEMENTS APPLY TO THE SERVICE FIXES; HOWEVER, THIS DOES NOT
       EXTEND ANY WARRANTY AND/OR SERVICES, INCLUDING BUT NOT LIMITED
       TO THE "GETTING STARTED" PERIOD, OUTLINED IN SUCH AGREEMENTS.



























  
                                                 Terms and Conditions  1


                    January 25 1996 Warp FixPak XR_W017

  WHO SHOULD NOT INSTALL THIS FIXPAK

  Do not install this FixPak if either of the following applies to you:

  APTIVA M Series

  OS/2 FixPaks can not be installed on Aptiva M series models that were
  preloaded with OS/2 Warp.  However, if you installed (or reinstalled)
  a shrinkwrapped version of OS/2 Warp on these models, you can install
  the FixPak.  Contact OS/2 Technical Support if you need assistance in
  this process.

  DCF/2 users

  DCF/2 will not work with this FixPak or any FixPak since XR_W009. If
  you must apply this FixPak then you have to uncompress your harddisk
  and not use DCF/2.

  IBM is working with the DCF/2 developers to resolve this problem.

































  
                                   Who should not install this FixPak  2


                    January 25 1996 Warp FixPak XR_W017

  INSTALLATION NOTES



  DO NOT USE YOUR SYSTEM ONCE THE FIXPAK INSTALLATION IS STARTED

  Once you begin a FixPak installation, do not try to use your system
  for any other purpose. Doing so may yield unexpected problems which
  can cause the FixPak installation to fail.


  WHAT IS THE SIQ (SINGLE INPUT QUEUE) FEATURE

  The "SIQ" feature is new with FixPak XR_W017. It allows the user to
  take focus away from an application that is monopolizing the message
  queue.  When the FixPak is installed, the SIQ feature is disabled
  (OFF).


  How it works

  When you request a focus change for example, by clicking on another
  application or pressing Ctl+Esc the application that has the focus
  should respond to the message in x milliseconds.  If the application
  does not respond within that time, OS/2 determines that the
  application is not responding to messages and flags the application
  queue as bad. It then switches focus to the desired application.

  OS/2 will monitor the queue marked as bad to see when it does start
  responding to messages. It will mark the queue as good when this
  occurs.

  To enable the SIQ feature, put a SET PM_ASYNC_FOCUS_CHANGE statement
  in CONFIG.SYS and reboot.

  The parameters to the SET command are:

         SET PM_ASYNC_FOCUS_CHANGE=ON | ON x | OFF

         The default is OFF (disabled).


  To turn it on (enable) put the following in the CONFIG.SYS file and
  reboot:

         SET PM_ASYNC_FOCUS_CHANGE=ON


  To change the timeout value put the following in the CONFIG.SYS file
  and reboot:


  
                                                   Installation Notes  3


                    January 25 1996 Warp FixPak XR_W017

         SET PM_ASYNC_FOCUS_CHANGE=ON x

         where x is in milliseconds (default is 2000 (2 seconds))



  If you think you are having problems with SIQ, a way to isolate a
  problem is to raise the timeout to 5000 milliseconds (5 seconds).  If
  that does not help, turn it off.  If there is a SIQ feature problem,
  this will help us (IBM) isolate it.


  POPUP MESSAGE ABOUT NEWER FILE ON HARDDISK THAN IS IN FIXPAK

  If you get a popup stating that a newer file exists on your harddisk
  than is in the FixPak, and it is one of the following files, select
  the "No" button so you DO NOT replace the newer file with the older
  one.

  þ   AUTODRV2.SYS  6-09-95  4:24p

  þ   IBM2SS01.SYS  7-09-95  2:03p

  þ   PCM2ATA.ADD   6-10-95  3:30p

  þ   PCMCIA.SYS    6-09-95  4:23p



  COMMON FILE DIALOG INTERFACE CHANGES

  The Common File Dialog interface has been rearranged to improve
  usability.  The changes are:

  þ   "Type of file" field moved below the Open filename.

  þ   "Drive" and "Directory" controls were swapped with the "File"
      control.



  DELL MACHINES AND FONT EDITING

  When editing fonts, users of Dell machines may discover a slight
  regression.  When a font size is edited, the Font Palette is updated
  correctly; however, should users browse (select around) the palette,
  they might, at times, notice an inconsistency between the font size
  displayed on the palette and the one that is displayed on the font
  editor.  In all cases, the font size displayed on the Font Palette is
  the correct size for the font when it is dragged to the target (for
  example, the desktop, folder, or application).

  
                                                   Installation Notes  4


                    January 25 1996 Warp FixPak XR_W017

  CORRECTIVE SERVICE FACILITY BOOT DISKETTES

  You will need the OS/2 Warp 3.0 Corrective Service Facility Boot
  Diskettes to install this FixPak. These files should be available from
  the same place you got this FixPak.

     CSFBOOT.1DK - Corrective Service Facility disk 1
     CSFBOOT.2DK - Corrective Service Facility disk 2

        - or -

     WKICKR.ZIP   - File compressed with PKZIP. Contains both of the
                    above disk images. Requires PKUNZIP or UNZIP to
                    extract original files from the compressed file.


  To create diskettes from the disk image files, you need LOADDSKF.EXE.
  This is also available from the same place you obtained this FixPak.

     LDF.COM      - Self-extracting file that will create LOADDSKF.EXE.
                    Place in a separate directory on your hard disk
                    and then enter LDF.

        - or -

     LOADDF.ZIP   - File compressed with PKZIP that contains LOADDSKF.EXE.
                    Requires PKUNZIP or UNZIP to extract original files
                    from the compressed file.

  Note: LOADDSKF.EXE is also on any CD-ROM version of OS/2.


  Use LOADDSKF.EXE to create the diskettes. For each disk image, place a
  2MB HD (1.44MB formatted) diskette in A:. DO NOT use a 1MB (720KB
  formatted) diskette because you might have problems trying to install
  this FixPak.

  1.  Enter LOADDSKF CSFBOOT.1DK A: /F. Label the diskette as CSF DISK
      Diskette 1 (SP DISK 1).

  2.  Enter LOADDSKF CSFBOOT.2DK A: /F. Label the diskette as CSF DISK
      Diskette 2 (SP DISK 2).

  3.  Enter LOADDSKF XR_W017.1DK A: /F. Label the diskette as FixPak
      XR_W017 Corrective Service Diskette 1 (CSF DISK 1).

  4.  Enter LOADDSKF XR_W017.2DK A: /F. Label the diskette as FixPak
      XR_W017 Corrective Service Diskette 2 (CSF DISK 2).

  5.  Enter LOADDSKF XR_W017.3DK A: /F. Label the diskette as FixPak
      XR_W017 Corrective Service Diskette 3 (CSF DISK 3).

  
                                                   Installation Notes  5


                    January 25 1996 Warp FixPak XR_W017

  6.  Enter LOADDSKF XR_W017.4DK A: /F. Label the diskette as FixPak
      XR_W017 Corrective Service Diskette 4 (CSF DISK 4).

  7.  Enter LOADDSKF XR_W017.5DK A: /F. Label the diskette as FixPak
      XR_W017 Corrective Service Diskette 5 (CSF DISK 5).

  8.  Enter LOADDSKF XR_W017.6DK A: /F. Label the diskette as FixPak
      XR_W017 Corrective Service Diskette 6 (CSF DISK 6).

  9.  Enter LOADDSKF XR_W017.7DK A: /F. Label the diskette as FixPak
      XR_W017 Corrective Service Diskette 7 (CSF DISK 7).

  10. Enter LOADDSKF XR_W017.8DK A: /F. Label the diskette as FixPak
      XR_W017 Corrective Service Diskette 8 (CSF DISK 8).



  READ-ONLY FILES

  If you installed OS/2 Warp 3.0 from a CD-ROM, some files being updated
  might have the Read-Only attribute set. This will cause the update
  program to ask you if you want the files replaced. Answer OK.






























  
                                                   Installation Notes  6


                    January 25 1996 Warp FixPak XR_W017

  RELOCATED OS/2 FILE SUPPORT

  This FixPak will service directories based on the location of
  supported SYSLEVEL.OS2 and SYSLEVEL.MPM files.  Please check your
  system to make sure extra copies of these files are not located in
  directories other than:

    \OS2\INSTALL\SYSLEVEL.OS2 on the boot drive of your OS/2 partition(s)
    \MMOS2\INSTALL\SYSLEVEL.MPM on any partition


  If additional copies of these files are found in other locations on
  your hard disk then CSF will try to service files as follows:

  For SYSLEVEL.OS2

    ..\..\   all files in a directory two levels above (toward the root).
             This should be the root directory of your boot drive.
    ..\*     all files in a directory one level above (toward the root) and
             all subdirectories below. This should be the OS2 directory and
             subdirectories.


  For SYSLEVEL.MPM

    ..\*     all files in a directory one level above (toward the root) and
             all subdirectories below. This should be the MMOS2 directory and
             subdirectories.


  If you have moved OS/2 files or directories, do the following in order
  to have them serviced:

  1.  Create a file named USERDIRS.OS2 in the \OS2\INSTALL directory of
      the OS\2 Warp partition to be serviced.

      In this file, place the full path to the directory you want to be
      serviced. Examples would be:

       C:\JSI\*
       D:\JSI\SH\*


      Be sure to include the trailing * (asterisk) after the last
      backslash.

  Note: Leave this file for any future OS/2 Warp FixPaks you might
  apply.




  
                                          Relocated OS/2 file support  7


                    January 25 1996 Warp FixPak XR_W017

  INSTALLATION PROCESS

  Before installing any FixPak, run CHKDSK /F against all drives on your
  system to correct any file system errors that might be present. You
  cannot do this while OS/2 is active. You must shut down and run CHKDSK
  by one of the following methods:

  þ   Boot from your Installation and DISK 1 diskettes you used to
      install OS/2 with.  If your file system is HPFS, then put the
      diskette with CHKDSK and UHPFS.DLL on it in your A: drive before
      issuing the CHKDSK command.

  þ   Boot from the Utilities disk you created via the "Create Utility
      Diskettes" icon in the System Setup folder.

  þ   Boot from a different OS/2 partition.

  To Install this FixPak use one of the following methods:


  METHOD 1: INSTALL FROM BOOTED OS/2 PARTITION.

  This method allows you to select the products (partitions) to be
  serviced.

  This is the method you should use if you have more than one OS/2
  partition and want to control which one is serviced.

  Note: You can use a diskette drive other than A: with this method. If
  your 3.5" diskette drive is B:, use B: where A: is mentioned in the
  following steps.  (this method only).

  1.  Insert CSF DISK Diskette 1 in drive A.

  2.  Open an OS/2 window or full-screen session.

  3.  Type A:\SERVICE and press the Enter key.

  4.  Follow the displayed instructions. When prompted to insert
      Corrective Service Diskette 1 (not CSF DISK Diskette 1), place
      FixPak XR_W017 Corrective Service Diskette 1 in drive A. Repeat
      for the rest of the FixPak disks when requested to do so.

      Note: It can take a considerable length of time for the Corrective
      Service Facility to scan your hard disk for serviceable files. In
      some cases, it has taken as long as 40 minutes. Please be patient
      and allow this process to complete.

  5.  If this is the first OS/2 Warp FixPak you have applied to this
      system, then enter the path to the ARCHIVE directory where a copy
      of replaced files will be stored (for example, D:\ARCHIVE).

  
                                                 Installation Process  8


                    January 25 1996 Warp FixPak XR_W017


      Note: This ARCHIVE directory is not related to the ARCHIVES
      directory built into OS/2 Warp 3.0. Please specify a different
      path.  You must specify a different ARCHIVE directory for each
      product to be serviced.

      If this is not the first OS/2 Warp FixPak, then enter the path to
      the BACKUP directory where a copy of replaced files will be stored
      (for example, D:\BACKUP).

      Note: You must specify a different BACKUP directory for each
      product to be serviced.

      For either case, make sure there is sufficient space available on
      the drive you specify. Even though these files are kept in
      compressed (PACK2) format, they require between 7 and 12 MB of
      disk space.

  6.  Click on "OK".

  7.  You will see an "Application in use" dialog box showing a list of
      locked files that cannot be serviced while the system is running.
      You are given two choices - to Continue or Reboot. Select
      Continue.

  8.  During the installation process you might see messages about
      Archiving, Updating and Deferring service.

      þ   Archiving saves a compressed copy of the original file in the
          ARCHIVE or BACKUP path you specified. This occurs only if you
          apply service to the OS/2 partition you are booted from.

      þ   Updating means the original files are replaced with the new
          ones from this FixPak.

      þ   Deferring service means the file to be updated is currently in
          use by the system and cannot be updated. The new files from
          the FixPak are placed in unpacked format in the
          \OS2\INSTALL\IBMCSFLK\FIX directory on your Warp boot drive.
          They are processed by the locked file device driver during
          reboot after you shut down the system.

  9.  Select NO for a redisplay of the "Product List" after the first
      part of the FixPak application process has completed if this
      message is displayed.

  10. Click Cancel and Exit to close the Corrective Service Facility
      window if necessary.

  11. Shut down and reboot your system.


  
                                                 Installation Process  9


                    January 25 1996 Warp FixPak XR_W017

      You will see the following during reboot of the system if you
      applied service to the OS/2 partition you were booted from.

     The locked file driver is loaded.

            Processing locked files

            Processing complete


      The system might then do an automatic reboot. In some cases, it
      might do an additional reboot.



  METHOD 2: BOOT FROM CORRECTIVE SERVICE DISK 1.

  This method does not prompt the user for any information. No
  interaction with the user takes place other than requests to put the
  next diskette in drive A.  All serviceable partitions on your system
  will be updated automatically. Be especially careful of extra
  SYSLEVEL.OS2 or SYSLEVEL.MPM files when using this method because they
  can cause CSF to apply service to directories you do not want
  serviced.

  1.  Shut down your OS/2 system.

  2.  Insert CSF DISK Diskette 1 in drive A.

  3.  Press Ctrl+Alt+Del to boot the disk in drive A.

  Service will be applied to ALL partitions that contain a version of
  OS/2 that is supported by this FixPak. See the section "FixPak
  Corrective Service Notes" for the CSD levels this FixPak applies to.

  Note: It can take a considerable length of time for the Corrective
  Service Facility to scan your hard disk for serviceable files. In some
  cases it has taken as long as 40 minutes. Please be patient and allow
  this process to complete.


  ADDITIONAL CORRECTIVE SERVICE FACILITY INFORMATION

  Additional information on the Corrective Service Facility is available
  from the README.INF file on the first Corrective Service Facility
  disk. To view this file, place CSF disk 1 in drive A and enter VIEW
  A:\README.INF.





  
                                                Installation Process  10


                    January 25 1996 Warp FixPak XR_W017

  RECOVERING FROM INSTALLATION PROBLEMS

  This section describes some procedures you can follow to recover from
  problems found while trying to install a FixPak.


  NO FILES TO SERVICE

  If you see a "No files to service" message while applying this FixPak,
  the Current CSD level or Component ID of the "IBM OS/2 Base Operating
  System" might not be supported by this FixPak.

  Correct values must be:

  OS/2 Version        OS/2 Base Operating System  Multimedia Presentation Manager
  ------------------  --------------------------  --------------------------
  Warp for Windows    Current CSD level: XR_3000  Current CSD level: XR_3000
                      Component ID: 562260100     Component ID: 562137400

  Warp with WIN-OS/2  Current CSD level: XR_3001  Current CSD level: XR_3001
                      Component ID: 562274700     Component ID: 562274700

  Warp for Windows    Current CSD level: XR_3002  Current CSD level: XR_3002
  Mfg Refresh         Component ID: 562260100     Component ID: 562260100

  Warp with WIN-OS/2  Current CSD level: XR_3003  Current CSD level: XR_3003
  Connect             Component ID: 562274700     Component ID: 562274700

  Warp for Windows    Current CSD level: XR_3004  Current CSD level: XR_3004
  Mfg Refresh Connect Component ID: 562260100     Component ID: 562260100

  Warp with WIN-OS/2  Current CSD level: XR_3005  Current CSD level: XR_3005
  Server              Component ID: 562274700     Component ID: 562274700


  If these values are correct, check for the following files on any OS/2
  boot drive in the \OS2\INSTALL directory.

     LOGF0000.OS2
     LOGSTART.OS2
     LOGARCH.OS2


  Check for the following files in your MMOS2\INSTALL directory.

     LOGF0000.MPM
     LOGSTART.MPM
     LOGARCH.MPM




  
                               Recovering from Installation problems  11


                    January 25 1996 Warp FixPak XR_W017

  Also check for the following file:

     C:\CSF_SEL.000


  If these files exist, rename them and try the FixPak installation
  again.  If the installation is successful, delete the renamed files.


  PREVIOUS INSTALLATION INTERRUPTED

  If you get a message that the previous installation of a FixPak was
  interrupted (whether true or not), check for the following file:

     C:\FIXSTART


  If it exists, rename it and try the FixPak installation again.  If it
  works, delete the renamed file. If this does not resolve the problem,
  follow the procedure "Recovering from Installation problems".


  UNABLE TO OPEN ARCHIVE DIRECTORY

  If you get a message about problems with the Archive directory (for
  example, cannot find or unable to open), then the most probable cause
  is that you applied a previous FixPak and deleted the FixPak ARCHIVE
  or BACKUP directory.

  To recover from this, follow the "No files to service" and "Previous
  installation interrupted" steps.





















  
                               Recovering from Installation problems  12


                    January 25 1996 Warp FixPak XR_W017

  SYSTEM PROBLEMS AFTER FIXPAK INSTALLATION

  This section describes problems that can occur after applying this
  FixPak.  It also describes how to recover from these problems.


  OS/2 IS UNABLE TO OPERATE YOUR HARD DISK OR DISKETTE DRIVE.

  If, after installing this FixPak, you get the following message:

     OS/2 is unable to operate your hard disk or diskette drive.
     The system is stopped.  Correct the preceding error and
     restart the system.


  Do the following:

  1.  Boot your system in one of the followin ways

      þ   With your OS/2 Warp Installation "Install disk" and "DISK 1".

      þ   From another bootable OS/2 partition.

      þ   From a bootable DOS partition or DOS bootable diskette if your
          OS/2 Warp partition uses the FAT file system and not the HPFS
          file system.

      þ   From your Utility disks if you created them via the "Create
          Utility Disks" Icon in "System Setup folder".

  2.  Edit the CONFIG.SYS file on your Warp boot drive. Add /FL to the
      end of the BASEDEV=IBM1S506.ADD line.

      Note: You can use the TEDIT editor which is a text editor and does
      not require the Workplace Shell to be running.

      a.  CD x:                       (x: is your Warp boot drive)

      b.  \OS2\TEDIT CONFIG.SYS

      c.  /IBM1S506                   (locate the IBM1S506 line, case
          sensitive)

      d.  Press the Esc key           (this move the cursor into the
          edit area)

      e.  Add /FL to the end of the BASEDEV=IBM1S506.ADD line. Leave a
          space between the last character of the existing line and the
          /FL

      f.  Press F2 to save the change

  
                           System problems after FixPak installation  13


                    January 25 1996 Warp FixPak XR_W017

      g.  Press F3 to quit

  3.  Press Ctrl+Alt+Del to reboot your system.

  If this resolves your problem then please read "Updating systems with
  the CMD chipset" and "RZ1000 and CMD640 Data Problems (APAR=PJ19409)"
  (the next two sections of this document) for additional changes you
  can make to your CONFIG.SYS file.


  RIPL FAILURE

    If RIPL (Remote IPL) of a work station fails after the FixPak is
    applied when it worked prior to applying the FixPak, the probable
    cause is a downlevel SOM.DLL in the \IBMLAN\RPL\IBMLAN\NETLIB
    directory.

    After applying fixpack 17 to the \IBMLAN\RPL\OS2.30 directory
    tree on a LAN Server 4.0 RIPL server, the following procedure
    must be followed to complete the update:

    1. Change to the d:\IBMLAN\RPL\IBMLAN\NETLIB directory.
       Where d: is the drive where \IBMLAN\RPL is installed.

    2. Create a new sub-directory, SOMBAK.

       MD SOMBAK

    3. Copy the SOM*.DLL files to the SOMBAK directory.

       COPY SOM*.DLL SOMBAK\

    4. Erase the SOM*.DLL files in the d:\IBMLAN\RPL\IBMLAN\NETLIB
       directory.

         ERASE SOM*.DLL

    5. Determine if there are any other versions of OS/2 installed
       in the Remote IPL tree.  Look for the following
       sub-directories:

         d:\IBMLAN\RPL\OS2.20      (OS/2 2.0)
         d:\IBMLAN\RPL\OS2.21      (OS/2 2.10/2.11)

    6. If any other versions of OS/2 are installed in the Remote
       IPL tree, do the following:

       a. Change to the d:\IBMLAN\RPL\OS2.2x\OS2\DLL (where x is 0
          and/or 1) directory.

       b. Compare the date/timestamp of the SOM.DLL file with

  
                           System problems after FixPak installation  14


                    January 25 1996 Warp FixPak XR_W017

          the file d:\IBMLAN\RPL\IBMLAN\NETLIB\SOMBAK\SOM.DLL.

       c. If the ..\OS2\DLL\SOM.DLL is older than the one in
          d:\IBMLAN\RPL\IBMLAN\NETLIB\SOMBAK, copy the files
          saved in step 3.

          COPY d:\IBMLAN\RPL\IBMLAN\NETLIB\SOMBAK\*.DLL

  Note: If the RIPLINST.EXE utility is subsequently used to
        reload the d:\IBMLAN\RPL\OS2.2x directory tree(s),
        the saved SOM*.DLL files will have to be re-copied
        from d:\IBMLAN\RPL\IBMLAN\NETLIB\SOMBAK.



  UPDATING SYSTEMS WITH THE CMD CHIPSET

  If you are installing this FixPak on a machine that has the CMD PCI
  IDE chipset, you must modify your CONFIG.SYS after the FixPak has been
  installed.

  Add the following statements to your CONFIG.SYS file:

     BASEDEV=CMD640X.ADD     (add this line below BASEDEV=IBM1S506.ADD)
     BASEDEV=CMDATAPI.FLT    (add this line below BASEDEV=IBMIDECD.FLT)




  RZ1000 AND CMD640 DATA PROBLEMS (APAR=PJ19409)

  Problem Description: IDE disks can incur possible data read conflicts
  that can cause data problems.

  OS/2 Versions: All versions of OS/2 Warp

  To verify the existence of this problem on your system, turn on the
  verbose option on the IBM1S506.ADD.  After installing the update per
  the instructions above, edit CONFIG.SYS and add the /V (verbose)
  switch option to the IBM1S506.ADD line:

          BASEDEV=IBM1S506.ADD /V


  If your CONFIG.SYS file does not have this line, add it any place
  before the line:

          BASEDEV=CMD640X.ADD




  
                           System problems after FixPak installation  15


                    January 25 1996 Warp FixPak XR_W017

  After adding the /V and rebooting your system, you might see the
  following on the third line of disk information during start-up:

     PCI Rev: 02.00  RZ1000 PCI to IDE IC, Rev: 0x01  VID:0x1000 DID:0x1042
                             or
     PCI Rev: 02.00  CMD640 PCI to IDE IC, Rev: 0x01  VID:0x1095 DID:0x0640


  If this information is displayed your system does contain an RZ1000 or
  CMD640 chip and is susceptible to the above problem.

  Note: On some systems this message might be displayed for only a brief
  time during system boot.

  If no such line appears, then you can revert to the originally shipped
  device drivers or leave the new drivers installed.

  Note: This fix has no effect on other IDE systems.

  Remove the /V option from the CONFIG.SYS file if you no longer want
  the verbose information displayed.

  Fix Description:

  To fix data problems with the RZ1000 and CMD640 chips, disable
  Read-ahead mode in the OS/2 IBM1S506.ADD and CMD640X.ADD device
  drivers.  These are generic device drivers which fix all the above
  releases and are compatible with systems that DO NOT use the RZ1000 or
  CMD640x chips.

  The new IBM1S506 device driver detects the RZ1000 and disables
  read-ahead for both RZ1000 IDE channels.  The IBM1S506 device driver
  also detects the CMD640x chip and disables read-ahead for the primary
  IDE channel.

  The new CMD640X device driver detects the CMD640 chip and disables
  read-ahead mode for both IDE channels.

  Also included with this fix distribution are the corresponding ATAPI
  CD-ROM device drivers so as to remain synchronized with IDE drivers.

          IBM1S506.ADD   -> Generic IDE/ATA Device Driver
          IBMIDECD.FLT   -> Generic IDE/ATAPI Device Driver

          CMD640X.ADD    -> CMD Optimized IDE/ATA Device Driver
          CMDATAPI.FLT   -> CMD Optimized IDE/ATAPI Device Driver


  Performance Impact:



  
                           System problems after FixPak installation  16


                    January 25 1996 Warp FixPak XR_W017

  IBM's benchmarks show no system performance degradation from disabling
  the read-ahead mode in either the RZ1000 or CMD640 IDE PCI interface
  chips.


  SYS3175 WHEN OPENING LS 4.0 LAN SERVER ADMINISTRATION

  Contact IBM LAN support and request the fix for APAR IC11718 which is
  IP08169 (LS40GUI.ZIP on Internet and BBSes).

  If you need a temporary solution while waiting to obtain the fix,
  backout SOM.DLL to the pre-FixPak level as follows

  1.  Shut down your system.

  2.  Reboot and press Alt-F1 when you see "OS/2" and a white block in
      the top left corner of the screen.

  3.  Press C to goto a command prompt.

  4.  Rename x:\OS2\DLL\SOM.DLL to SOMFP.DLL (x: is your OS/2 boot
      drive)

  5.  Change to the FixPak archive directory

  6.  Enter  UNPACK SOM.DL_ x:\OS2\DLL       (x: is your OS/2 boot
      drive)

  7.  Enter  EXIT

  Your system will reboot with the pre-FixPak version of SOM.DLL in
  place. The SYS3175 problem should be resolved.

  Once you receive and apply the fix for APAR IC11718 you should do the
  following to reinstall SOM.DLL from this FixPak.

  1.  Shut down your system.

  2.  Reboot and press Alt-F1 when you see "OS/2" and a white block in
      the top left corner of the screen.

  3.  Press C to goto a command prompt.

  4.  Delete x:\OS2\DLL\SOM.DLL              (x: is your OS/2 boot
      drive)

  5.  Rename x:\OS2\DLL\SOMFP.DLL to SOM.DLL (x: is your OS/2 boot
      drive)

  6.  Enter  EXIT


  
                           System problems after FixPak installation  17


                    January 25 1996 Warp FixPak XR_W017

  TRAPS WHEN CANCELING PRINT JOBS AFTER FIXPAK IS INSTALLED

  If you experience a trap when canceling print jobs using a LaserJet
  driver, download the LaserJet driver FixPak XR0P012, revision level
  30.453 or later from any of the sites listed in the "Where fixes can
  be found" section of this document.

  If you are using the IBMNULL printer driver, call service for APAR
  PJ19995.


  NOVELL REQUESTER

  If you are using Novell Requester for OS/2, you need to obtain the
  latest version of OS2C1.EXE. The number for the Novell BBS is
  801-221-5197.


  CC:MAIL FOR OS/2

  If you are unable to open the settings notebook for any CC:Mail object
  (Mouse button 2 on a CC:Mail object and click on "Settings"), then you
  need CC:Mail for OS/2 client 1.03C (or later).


  RAPID RESUME FIX

  If you are using the IBM Rapid Resume function, you need to update a
  module on your system.  On the last diskette of this FixPak are two
  directories named DIR_ONE and DIR_TWO.  Depending on your machine
  type, you need the files in one of these directories.  Put the
  diskette with these directories into drive A.

  On IBM machine types PC100, PC300, PC700 and Aptiva 2144-Pxx (xx = the
  different model numbers), enter the following command:

     COPY A:\DIR_ONE\VCMOS.SYS ?:\OS2\MDOS
         (? = the OS/2 drive being serviced)


  On IBM machine type Aptiva 2144-Mxx (xx = the different model
  numbers), enter the following command:

     COPY A:\DIR_TWO\VCMOS.SYS ?:\OS2\MDOS
         (? = the OS/2 drive being serviced)


  During the next boot, this update will take effect.




  
                           System problems after FixPak installation  18


                    January 25 1996 Warp FixPak XR_W017

  NO WINDOW LIST WHEN YOU PRESS CTRL+ESC

  If after applying this FixPak you no longer get the Window list when
  you press Ctrl+Esc, check the CONFIG.SYS file on your OS/2 boot
  partition for the following line:

  SET AUTOSTART=PROGRAMS,TASKLIST,FOLDERS,LAUNCHPAD


  If you are missing the TASKLIST keyword, that is the cause of this
  problem.  Add it to the line as shown above.

  Until OS/2 Warp FixPak XR_W014, the removal of TASKLIST from the SET
  AUTOSTART line in CONFIG.SYS had no effect. This was a problem that
  was fixed in FixPak 14 and all subsequent FixPaks.


  IBM CODE/400 AT V3R1M0 LEVEL

  You will experience a problem if you attempt to install IBM CODE/400
  after applying the fixpack. Please ensure that IBM CODE/400 is
  installed BEFORE the fixpack is applied.

  For users of the IBM CODE/400 product at the V3R1M0 level, you need to
  ensure you have the PTF SF28110 for product 5763CD1 installed or you
  will encounter a problem in file EVFWLIST.EXE when running CODE/400
  with this fixpack.


  PROBLEMS WITH VISUAL REXX APPLICATIONS

  If you have problems with visual REXX applications like VX/REXX or
  VisPro/Rexx try backing out the REXX DLLs applied by this FixPak as
  follows:

  Note: x: means your OS/2 Warp boot drive.

  1.  Shut down your system.

  2.  Reboot and press Alt-F1 when you see "OS/2" and a white block in
      the top left corner of the screen.

  3.  Press C to goto a command prompt.

  4.  Rename x:\OS2\DLL\REXX.DLL to REXX.DLO

  5.  Rename x:\OS2\DLL\REXXAPI.DLL to REXXAPI.DLO

  6.  Rename x:\OS2\DLL\REXXUTIL.DLL to REXXUTIL.DLO

  7.  Change to the FixPak archive directory

  
                           System problems after FixPak installation  19


                    January 25 1996 Warp FixPak XR_W017

  8.  Enter  UNPACK REXX.DL_ x:\OS2\DLL

  9.  Enter  UNPACK REXXAPI.DL_ x:\OS2\DLL

  10. Enter  UNPACK REXXUTIL.DL_ x:\OS2\DLL

  11. Enter  EXIT



  TCP/IP AT LEVEL WR08152

  A problem can occur in TCP/IP file TCPIPDLL.DLL at service level
  WR08152.  Contact IBM LAN Support for a fix to this problem.


  DOSCALL1.DLL ERROR

  If after installation of the Fixpack and upon REBOOT an error is
  received "C0000005" from DOSCALL1.DLL (there may be two DOSCALL1.DLL
  errors received), make the following adjustments to the RUN statements
  in CONFIG.SYS.  REBOOT after each adjustment to check if the error has
  been removed.

  Note - start with RUN statements that are not associated with IBM LAN
  Requester or MPTS. The error has been found with the RUN statement for
  COMETRUN.EXE (no PATH) and MWSTART.EXE (move to STARTUP.CMD).

  1).Verify that all RUN statements have the fully qualified PATH to the
  file.

  2).REM the RUN statement out of CONFIG.SYS and place it in the
  STARTUP.CMD
     file (remember to leave off the "RUN=" and only put the PATH and
  file name).

  These changes can be made in the following manner: If the system
  continues to boot after the error(s) open an OS/2 window and edit
  CONFIG.SYS using the command "TEDIT CONFIG.SYS".  If the system halts,
  either reboot, press Alt-F1 when the white rectangle is in the upper
  left corner, select "C" from the menu and edit CONFIG.SYS using the
  command "TEDIT CONFIG.SYS", or reboot from the Installation diskettes,
  go to a command prompt and edit CONFIG.SYS using the command "TEDIT
  CONFIG.SYS".

  TEDIT can also be used to edit STARTUP.CMD after making changes to
  CONFIG.SYS.





  
                           System problems after FixPak installation  20


                    January 25 1996 Warp FixPak XR_W017

  CSD LEVEL OF SYSLEVEL.OS2

  The Current CSD level for the "IBM OS/2 Base Operating System" will
  not be changed by installation of this FixPak even though the
  SERVICE.LOG file states it will. This FixPak is not a Service Level
  change. It upgrades the existing service level (XR_300n); therefore
  the SYSLEVEL is not changed. All fix information is recorded in the
  SERVICE.LOG file.

  Look at the file

     \OS2\INSTALL\SERVICE.LOG


  for information relating to the installation of this (or any) FixPak
  on your system. To see the current level and other related information
  use the SYSLEVEL command.

  Use the VER /R command to see the current revision of OS/2 installed.
  The response will look like the following for this FixPak:

  The Operating System/2 Version is 3.00
  Revision 8.241

             -- or --

  The Operating System/2 Version is 3.01
  Revision 8.241


  Look at the README.1ST file on the first FixPak disk of any FixPak for the
  "Build Level: n.nnn" line.  That is the number you should see for that
  FixPak when you issue the VER /R command.




  LIST OF PROBLEMS FIXED IN THE FIXPAK

  See the README2 file on the first FixPak disk for a list of APARs
  fixed.











  
                                           CSD level of SYSLEVEL.OS2  21


                    January 25 1996 Warp FixPak XR_W017

  WHERE FIXES CAN BE FOUND

  You can find other files, such as new drivers or fixes for specific
  video cards, from the following locations:

  þ   CompuServe - Subscribers can download fixes from the OS/2 Support
      Forum (GO OS2SUPPO).

  þ   IBM OS/2 BBS - Subscribers can download fixes from the Software
      Download Library. U.S. customers who are not subscribers can call
      1-800-547-1283 for information on how to subscribe.

  þ   Internet - Customers with access to Internet services can download
      fixes using the following methods:

        Anonymous FTP to "ftp.software.ibm.com" (IP Address 198.17.57.67)
        FixPaks are located in the "/ps/products/os2/fixes" directory.

        World Wide Web (WWW) access via:
          IBM Software Manufacturing Solutions  ftp://service.boulder.ibm.com
          Full path is ftp://service.boulder.ibm.com/ps/products/os2/


  þ   Prodigy - Subscribers can download fixes from the OS2CLUB in the
      Download Library, IBM Files, Fixes area. Files are updated weekly
      and are available on Friday.

  þ   PCC BBS - Customers can call the IBM Personal Computer Company BBS
      in Raleigh, NC, and download fixes from the public area. You can
      access this BBS at 1-919-517-0001.

  þ   America On Line - Subscribers can download fixes from the OS/2
      Area.



















  
                                            Where Fixes can be found  22


                    January 25 1996 Warp FixPak XR_W017

  FIXPAK CORRECTIVE SERVICE LEVELS AND DISK LAYOUTS

  Build Level: 8.241

  Product location on CSD:  A:\FIX\OS2.1
  Product name:  "IBM OS/2 Base Operating System"
  Standard Edition  3.00
  Fixpak name:   XR_W017_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3000_
  System Id:  1000
  Component Id:  562260100
  Archive is ON for this product.
  _____________________________________________________________
  Product name:  "IBM OS/2 Base Operating System"
  Standard Edition  3.00
  Fixpak name:   XR_W017_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3001_
  System Id:  1000
  Component Id:  562274700
  Archive is ON for this product.
  _____________________________________________________________
  Product name:  "IBM OS/2 Base Operating System"
  Standard Edition  3.01
  Fixpak name:   XR_W017_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3002_
  System Id:  1000
  Component Id:  562260100
  Archive is ON for this product.
  _____________________________________________________________
  Product name:  "IBM OS/2 Base Operating System"
  Standard Edition  3.00
  Fixpak name:   XR_W017_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3003_
  System Id:  1000
  Component Id:  562274700
  Archive is ON for this product.
  _____________________________________________________________
  Product name:  "IBM OS/2 Base Operating System"
  Standard Edition  3.01
  Fixpak name:   XR_W017_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3004_
  System Id:  1000
  Component Id:  562260100
  Archive is ON for this product.
  _____________________________________________________________
  Product name:  "IBM OS/2 Base Operating System"
  Standard Edition  3.01
  Fixpak name:   XR_W017_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3005_
  System Id:  1000
  Component Id:  562274700

  
                   FixPak Corrective Service levels and disk layouts  23


                    January 25 1996 Warp FixPak XR_W017

  Archive is ON for this product.
  _____________________________________________________________

  Default directories:

          ..\..\
          ..\*

  Files contained in Fixpak for product:

  Filename      Name on CSD   Disk#  Date      Time   Size
  ------------  ------------  -----  --------  -----  -------
  AHA152X.ADD   AHA152X.AD_     6    10/30/95  14:54    38060
  AHA164X.ADD   AHA164X.AD_     6    10/30/95  14:52    19716
  AIC7770.ADD   AIC7770.AD_     5    10/30/95  14:54    42428
  AIC7870.ADD   AIC7870.AD_     5    10/30/95  14:55    34124
  APM.SYS       APM.SY_         6    10/30/95  15:16     6704
  ARCINST.EXE   ARCINST.EX_     6    12/05/95  02:15    21358
  ARCRECOV.EXE  ARCRECOV.EX_    6    12/05/95  02:16    24635
  AUTODRV2.SYS  AUTODRV2.SY_    6    06/09/95  16:24    10862
  BTSCSI.ADD    BTSCSI.AD_      6    10/30/95  15:01    22485
  BVHVGA.DLL    BVHVGA.DL_      5    12/04/95  19:44    31054
  BVHWNDW.DLL   BVHWNDW.DL_     6    12/04/95  19:45    12664
  CDFS.IFS      CDFS.IF_        6    12/04/95  21:34    41795
  CDROM.TBL     CDROM.TB_       6    05/19/95  17:16     3949
  CHKDSK.COM    CHKDSK.CO_      5    12/04/95  23:07    68656
  CMD.EXE       CMD.EX_         5    01/12/96  12:38    79360
  CMD640X.ADD   CMD640X.AD_     5    10/30/95  17:35    35924
  CMDATAPI.FLT  CMDATAPI.FL_    6    10/30/95  15:03    21554
  COM.SYS       COM.SY_         6    10/30/95  15:15    16912
  COMMAND.COM   COMMAND.CO_     5    12/04/95  23:16    52972
  DATABASE.DAT  DATABASE.DA_    5    12/05/95  00:19    83419
  DATABASE.TXT  DATABASE.TX_    5    08/17/95  09:30   609497
  DETNE2.SYS    DETNE2.SY_      6    10/30/95  14:41     5640
  DISPLAY.DLL   DISPLAY.DL_     5    12/04/95  22:32    44196
  DOSCALL1.DLL  DOSCALL1.DL_    4    12/04/95  22:44   123186
  DOSKRNL       DOSKRNL.___     6    12/04/95  19:53    30077
  DPT20XX.ADD   DPT20XX.AD_     6    10/30/95  14:59    24254
  DSPINSTL.EXE  DSPINSTL.EX_    5    12/05/95  00:35   170424
  E.EXE         E.EX_           5    12/04/95  22:57    70917
  EAUTIL.EXE    EAUTIL.EX_      5    12/04/95  23:23    37984
  FD16-700.ADD  FD16-700.AD_    6    11/29/95  21:59    31260
  FD7000EX.ADD  FD7000EX.AD_    6    11/29/95  22:01    20848
  FD8XX.ADD     FD8XX.AD_       6    11/29/95  22:02    30030
  FDISK.COM     FDISK.CO_       5    12/04/95  21:50   110245
  FORMAT.COM    FORMAT.CO_      5    12/04/95  23:34    68880
  FSFILTER.SYS  FSFILTER.SY_    6    01/06/96  08:53    12988
  HELPMGR.DLL   HELPMGR.DL_     4    12/04/95  23:30   176108
  HELPMSG.EXE   HELPMSG.EX_     5    12/04/95  23:34    36256
  HPFS.IFS      HPFS.IF_        5    12/09/95  15:17   143938
  IBM16AFS.EXE  IBM16AFS.EX_    6    11/29/95  22:03     3177

  
                   FixPak Corrective Service levels and disk layouts  24


                    January 25 1996 Warp FixPak XR_W017

  IBM1FLPY.ADD  IBM1FLPY.AD_    6    10/30/95  14:47    31170
  IBM1S506.ADD  IBM1S506.AD_    6    10/30/95  15:13    30636
  IBM2AMB1.SYS  IBM2AMB1.SY_    6    11/29/95  22:18    12437
  IBM2AST1.SYS  IBM2AST1.SY_    6    11/29/95  22:18    10047
  IBM2CAD1.SYS  IBM2CAD1.SY_    6    11/29/95  22:20    12479
  IBM2CMQ1.SYS  IBM2CMQ1.SY_    6    11/29/95  22:18    10085
  IBM2FLPY.ADD  IBM2FLPY.AD_    6    10/30/95  14:47    13754
  IBM2IDE.ADD   IBM2IDE.AD_     6    10/30/95  15:13    31396
  IBM2MAT1.SYS  IBM2MAT1.SY_    6    11/29/95  22:20    10067
  IBM2NCR1.SYS  IBM2NCR1.SY_    6    11/29/95  22:19    10047
  IBM2NEC1.SYS  IBM2NEC1.SY_    6    11/29/95  22:19    10047
  IBM2SCSI.ADD  IBM2SCSI.AD_    6    10/30/95  14:50    32691
  IBM2SS01.SYS  IBM2SS01.SY_    6    07/09/95  14:03    13203
  IBM2SS02.SYS  IBM2SS02.SY_    6    11/29/95  22:17    10477
  IBM2TOS1.SYS  IBM2TOS1.SY_    6    11/29/95  22:17    10054
  IBM2ZEN1.SYS  IBM2ZEN1.SY_    6    11/29/95  22:17    10047
  IBM2ZOS1.SYS  IBM2ZOS1.SY_    6    11/29/95  22:19    10063
  IBMIDECD.FLT  IBMIDECD.FL_    6    10/30/95  15:14    20358
  IBMKBD.SYS    IBMKBD.SY_      6    07/18/95  09:31     5612
  ICMEMCDD.SYS  ICMEMCDD.SY_    6    11/29/95  22:22    13932
  ICMEMFMT.EXE  ICMEMFMT.EX_    5    11/29/95  22:24    51031
  ICMEMMTD.SYS  ICMEMMTD.SY_    6    11/29/95  22:23     8300
  KBDBASE.SYS   KBDBASE.SY_     6    10/30/95  15:17    28501
  KEYBOARD.DCP  KEYBOARD.DC_    6    12/04/95  23:36   157804
  LINK386.EXE   LINK386.EX_     4    12/04/95  23:53   154164
  LMS205.ADD    LMS205.AD_      6    10/30/95  15:14    36380
  LMS206.ADD    LMS206.AD_      6    10/30/95  15:14    38732
  MIGRATE.EXE   MIGRATE.EX_     3    12/05/95  00:12   173644
  MINXOBJ.DLL   MINXOBJ.DL_     6    12/05/95  00:30    37543
  MIRRORS.DLL   MIRRORS.DL_     3    11/07/95  16:36   705196
  MITFX001.ADD  MITFX001.AD_    6    10/30/95  15:08    20488
  MOUSE.SYS     MOUSE.SY_       6    10/30/95  15:15    18169
  NPXEMLTR.DLL  NPXEMLTR.DL_    6    12/04/95  23:58    20692
  NWIAPI.DLL    NWIAPI.DL_      6    12/04/95  18:56    10075
  OS2ASPI.DMD   OS2ASPI.DM_     6    10/30/95  14:45    10970
  OS2CDROM.DMD  OS2CDROM.DM_    6    10/30/95  15:05    26580
  OS2CHAR.DLL   OS2CHAR.DL_     6    12/04/95  22:37      512
  OS2DASD.DMD   OS2DASD.DM_     6    10/30/95  14:44    34228
  OS2DUMP       OS2DUMP.___     6    12/04/95  19:02    16909
  OS2KRNL       OS2KRNL.___     2    01/11/96  17:23   571508
  OS2LDR        OS2LDR.___      6    12/04/95  18:59    30208
  OS2LDR.MSG    OS2LDR.MS_      6    12/04/95  19:02     8430
  OS2MM.DLL     OS2MM.DL_       4    11/27/95  20:21   366710
  OSO001.MSG    OSO001.MS_      5    12/04/95  18:21   174390
  OSO001H.MSG   OSO001H.MS_     5    12/04/95  18:22   240113
  PCM2ATA.ADD   PCM2ATA.AD_     6    06/10/95  15:30    23110
  PCMCIA.SYS    PCMCIA.SY_      5    11/29/95  22:10    47622
  PCMCIA.TBL    PCMCIA.TB_      6    01/24/95  19:28     1681
  PMCTLS.DLL    PMCTLS.DL_      3    01/25/96  11:43   612218
  PMDDE.DLL     PMDDE.DL_       6    12/05/95  00:25    24008
  PMDRAG.DLL    PMDRAG.DL_      6    12/16/95  13:10     1731

  
                   FixPak Corrective Service levels and disk layouts  25


                    January 25 1996 Warp FixPak XR_W017

  PMGPI.DLL     PMGPI.DL_       4    12/08/95  22:38   335438
  PMGRE.DLL     PMGRE.DL_       6    12/12/95  21:15     2231
  PMMERGE.DLL   PMMERGE.DL_     1    01/19/96  19:39  1186306
  PMMLE.DLL     PMMLE.DL_       6    12/08/95  16:06      673
  PMPRINT.QPR   PMPRINT.QP_     6    12/04/95  19:13    12249
  PMSDMRI.DLL   PMSDMRI.DL_     6    12/08/95  16:06    12800
  PMSHAPI.DLL   PMSHAPI.DL_     6    11/14/95  14:04     4549
  PMSPL.DLL     PMSPL.DL_       4    12/04/95  19:35   211690
  PMVDMP.DLL    PMVDMP.DL_      5    12/22/95  14:34    45851
  PMVIOP.DLL    PMVIOP.DL_      5    12/22/95  14:33    54070
  PMWIN.DLL     PMWIN.DL_       6    01/18/96  12:23    11264
  PMWP.DLL      PMWP.DL_        2    12/04/95  20:56   939461
  PMWPMRI.DLL   PMWPMRI.DL_     5    12/04/95  20:31    45342
  POINTDD.SYS   POINTDD.SY_     2    08/09/95  16:23     1811
  PRINT01.SYS   PRINT01.SY_     6    10/30/95  15:33    11038
  PRINT02.SYS   PRINT02.SY_     6    10/30/95  15:33    10166
  QUECALLS.DLL  QUECALLS.DL_    6    12/04/95  22:36     1024
  RESERVE.SYS   RESERVE.SY_     6    10/30/95  14:41     5702
  RESTORE.EXE   RESTORE.EX_     6    12/05/95  00:03    36080
  REXX.DLL      REXX.DL_        4    09/07/95  10:20   254768
  REXXAPI.DLL   REXXAPI.DL_     6    08/17/95  09:34    33735
  REXXUTIL.DLL  REXXUTIL.DL_    6    06/09/95  16:49    30331
  RSPDSPI.EXE   RSPDSPI.EX_     5    12/05/95  00:46   141752
  RSPINST.EXE   RSPINST.EX_     4    12/04/95  22:00   342752
  RUPINST2.EXE  RUPINST2.EX_    4    12/04/95  21:52   151024
  SBCD2.ADD     SBCD2.AD_       1    10/30/95  15:08    18834
  SEAMLESS.DLL  SEAMLESS.DL_    5    12/22/95  14:39    42112
  SEMAINT.EXE   SEMAINT.EX_     5    12/05/95  00:07    65984
  SESMGR.DLL    SESMGR.DL_      6    12/04/95  19:40     1536
  SETBOOT.EXE   SETBOOT.EX_     6    12/04/95  21:48    19632
  SIPANEL2.DLL  SIPANEL2.DL_    6    12/04/95  21:37    49472
  SOM.DLL       SOM.DL_         4    10/27/95  21:00   130955
  SOM.IR        SOM.IR_         4    10/27/95  21:00   496503
  SOMD.DLL      SOMD.DL_        2    10/27/95  21:00   434110
  SOMD.MSG      SOMD.MS_        5    10/27/95  21:01    15056
  SOMDD.EXE     SOMDD.EX_       6    10/27/95  21:01    37904
  SOMDSVR.EXE   SOMDSVR.EX_     6    10/27/95  21:01    34912
  SOMEM.DLL     SOMEM.DL_       5    10/27/95  21:00    59700
  SOMIR.DLL     SOMIR.DL_       5    10/27/95  21:01   132044
  SOMK.MSG      SOMK.MS_        6    10/27/95  21:01     3718
  SOMS.DLL      SOMS.DL_        6    10/27/95  21:01    31138
  SOMTC.DLL     SOMTC.DL_       5    10/27/95  21:01    42432
  SOMU.DLL      SOMU.DL_        5    10/27/95  21:01   126228
  SONY31A.ADD   SONY31A.AD_     6    10/30/95  15:11    32588
  SS2PCIC1.SYS  SS2PCIC1.SY_    6    11/29/95  22:16    10549
  SS2TCIC1.SYS  SS2TCIC1.SY_    6    11/29/95  22:16    12595
  SSVLSI.SYS    SSVLSI.SY_      6    11/29/95  22:20     6502
  SYSINST1.EXE  SYSINST1.EX_    6    12/04/95  21:45     4224
  SYSINST2.EXE  SYSINST2.EX_    5    12/04/95  21:51   149856
  SYSINSTX.COM  SYSINSTX.CO_    5    12/04/95  19:04    39472
  SYSLEVEL.SDS  SYSLEVEL.SD_    6    12/07/95  21:35      254

  
                   FixPak Corrective Service levels and disk layouts  26


                    January 25 1996 Warp FixPak XR_W017

  SYSLEVEL.SEM  SYSLEVEL.SE_    6    12/07/95  21:35      191
  SYSLEVEL.SIR  SYSLEVEL.SI_    6    12/07/95  21:35      188
  SYSLEVEL.SRK  SYSLEVEL.SR_    6    12/07/95  21:35      185
  SYSLEVEL.SUT  SYSLEVEL.SU_    6    12/07/95  21:35      177
  SYSTEM.TDF    SYSTEM.TD_      6    01/19/96  17:10    82893
  SYSTEM.TFF    SYSTEM.TF_      6    01/19/96  17:10   109330
  TEDIT.EXE     TEDIT.EX_       6    12/05/95  00:07     9390
  TESTCFG.SYS   TESTCFG.SY_     6    10/30/95  15:33     5434
  TRACEFMT.DLL  TRACEFMT.DL_    6    12/05/95  00:33    18061
  TRACEFMT.EXE  TRACEFMT.EX_    5    12/05/95  00:38    53793
  UCDFS.DLL     UCDFS.DL_       6    12/04/95  21:24    13264
  UHPFS.DLL     UHPFS.DL_       4    12/09/95  15:12   187088
  UNPACK2.EXE   UNPACK2.EX_     5    12/05/95  00:11    79792
  VBIOS.SYS     VBIOS.SY_       6    12/05/95  00:07     8688
  VCMOS.SYS     VCMOS.SY_       6    01/06/96  08:40     2272
  VCOM.SYS      VCOM.SY_        6    12/05/95  00:09    12384
  VDPMI.SYS     VDPMI.SY_       6    12/05/95  00:11    22337
  VDPX.SYS      VDPX.SY_        6    12/04/95  23:56    25857
  VKBD.SYS      VKBD.SY_        6    12/05/95  00:11    23575
  VLPT.SYS      VLPT.SY_        6    12/05/95  00:16    10113
  VPIC.SYS      VPIC.SY_        6    12/05/95  00:12     9894
  VTIMER.SYS    VTIMER.SY_      6    12/05/95  00:12     9936
  VWIN.SYS      VWIN.SY_        6    12/05/95  00:18    24592
  VXGA.SYS      VXGA.SY_        6    12/05/95  00:01    24772
  WPCMPNP.DLL   WPCMPNP.DL_     2    12/05/95  00:33   131769
  WPCONFIG.DLL  WPCONFIG.DL_    3    12/04/95  22:28   253747
  WPHELP.HLP    WPHELP.HL_      3    12/05/95  00:16   704236
  WPPRINT.DLL   WPPRINT.DL_     1    12/04/95  22:04   349829
  WPPRTMRI.DLL  WPPRTMRI.DL_    5    12/04/95  22:04    47482
  XDFH.MSG      XDFH.MS_        3    12/04/95  23:25     1045

  *************************************************************
  Product location on CSD:  A:\FIX\OS2.2
  Product name:  "IBM OS/2 Base Operating System"
  Standard Edition  3.00
  Fixpak name:   XR_W017_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3000_
  System Id:  1000
  Component Id:  562260100
  Archive is ON for this product.
  _____________________________________________________________
  Product name:  "IBM OS/2 Base Operating System"
  Standard Edition  3.01
  Fixpak name:   XR_W017_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3002_
  System Id:  1000
  Component Id:  562260100
  Archive is ON for this product.
  _____________________________________________________________
  Product name:  "IBM OS/2 Base Operating System"
  Standard Edition  3.01

  
                   FixPak Corrective Service levels and disk layouts  27


                    January 25 1996 Warp FixPak XR_W017

  Fixpak name:   XR_W017_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3004_
  System Id:  1000
  Component Id:  562260100
  Archive is ON for this product.
  _____________________________________________________________

  Default directories:

          ..\..\
          ..\*

  Files contained in Fixpak for product:

  Filename      Name on CSD   Disk#  Date      Time   Size
  ------------  ------------  -----  --------  -----  -------
  COMMS.SCR     COMMS.SC_       6    12/04/95  18:49     2560
  FIXMGR.DLL    FIXMGR.DL_      6    12/04/95  18:49     2048
  GDIS.SCR      GDIS.SC_        6    12/04/95  18:49     6144
  INSTALL.EXE   INSTALL.EX_     6    05/05/95  19:31   466324
  MCISEQS.SCR   MCISEQS.SC_     6    12/04/95  18:48     2048
  TIMERS.SCR    TIMERS.SC_      6    12/04/95  18:51     2048
  USERS.SCR     USERS.SC_       6    12/04/95  18:49    17408
  WINOS2.COM    WINOS2.CO_      6    12/04/95  18:49    31866
  WINSCLIP.DLL  WINSCLIP.DL_    6    12/04/95  18:50    20480
  WINSDDE.DLL   WINSDDE.DL_     6    12/04/95  18:50    24064
  WINSHELD.EXE  WINSHELD.EX_    6    12/04/95  18:50    23552
  WINSMSG.DLL   WINSMSG.DL_     6    12/04/95  18:50    29184

  *************************************************************
  Product location on CSD:  A:\FIX\OS2.3
  Product name:  "IBM OS/2 Base Operating System"
  Standard Edition  3.00
  Fixpak name:   XR_W017_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3001_
  System Id:  1000
  Component Id:  562274700
  Archive is ON for this product.
  _____________________________________________________________
  Product name:  "IBM OS/2 Base Operating System"
  Standard Edition  3.00
  Fixpak name:   XR_W017_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3003_
  System Id:  1000
  Component Id:  562274700
  Archive is ON for this product.
  _____________________________________________________________
  Product name:  "IBM OS/2 Base Operating System"
  Standard Edition  3.01
  Fixpak name:   XR_W017_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3005_

  
                   FixPak Corrective Service levels and disk layouts  28


                    January 25 1996 Warp FixPak XR_W017

  System Id:  1000
  Component Id:  562274700
  Archive is ON for this product.
  _____________________________________________________________

  Default directories:

          ..\..\
          ..\*

  Files contained in Fixpak for product:

  Filename      Name on CSD   Disk#  Date      Time   Size
  ------------  ------------  -----  --------  -----  -------
  COMM.DRV      COMM.DR_        7    06/12/95  16:58     9520
  COMMDLG.DLL   COMMDLG.DL_     6    01/19/96  11:46    89296
  GDI.EXE       GDI.EX_         7    01/19/96  11:48   226000
  INSTALL.EXE   INSTALL.EX_     7    12/04/95  21:45   476318
  OS2K386.EXE   OS2K386.EX_     6    01/19/96  11:49    80066
  S8514.DRV     S8514.DR_       7    06/12/95  16:53    89744
  USER.EXE      USER.EX_        7    01/19/96  11:52   276736
  WINSCLIP.DLL  WINSCLIP.DL_    7    01/19/96  11:50    14848
  WINSDDE.DLL   WINSDDE.DL_     6    01/19/96  11:50    17920
  WINSHELD.EXE  WINSHELD.EX_    6    01/19/96  11:50    20992
  WINSMSG.DLL   WINSMSG.DL_     6    01/19/96  11:49    24857

  *************************************************************
  Product location on CSD:  A:\FIX\OS2.4
  Product name:  "IBM OS/2 Base Operating System"
  Standard Edition  3.00
  Fixpak name:   XR_W017_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3003_
  System Id:  1000
  Component Id:  562274700
  Archive is ON for this product.
  _____________________________________________________________
  Product name:  "IBM OS/2 Base Operating System"
  Standard Edition  3.01
  Fixpak name:   XR_W017_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3004_
  System Id:  1000
  Component Id:  562260100
  Archive is ON for this product.
  _____________________________________________________________
  Product name:  "IBM OS/2 Base Operating System"
  Standard Edition  3.01
  Fixpak name:   XR_W017_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3005_
  System Id:  1000
  Component Id:  562274700
  Archive is ON for this product.

  
                   FixPak Corrective Service levels and disk layouts  29


                    January 25 1996 Warp FixPak XR_W017

  _____________________________________________________________

  Default directories:

          ..\..\
          ..\*

  Files contained in Fixpak for product:

  Filename      Name on CSD   Disk#  Date      Time   Size
  ------------  ------------  -----  --------  -----  -------
  REXX.DLL      REXX.DL_        7    12/13/95  19:50   248416
  REXXAPI.DLL   REXXAPI.DL_     7    12/13/95  19:50    33415
  REXXUTIL.DLL  REXXUTIL.DL_    7    12/13/95  19:50    30315

  *************************************************************
  Product location on CSD:  A:\FIX\MPM.5
  Product name:  "IBM Multimedia Presentation Manager/2"
  Standard Edition  3.00
  Fixpak name:   XR_W017_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3000_
  System Id:  1000
  Component Id:  562137400
  Archive is ON for this product.
  _____________________________________________________________
  Product name:  "IBM Multimedia Presentation Manager/2"
  Standard Edition  3.00
  Fixpak name:   XR_W017_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3001_
  System Id:  1000
  Component Id:  562274700
  Archive is ON for this product.
  _____________________________________________________________
  Product name:  "IBM Multimedia Presentation Manager/2"
  Standard Edition  3.01
  Fixpak name:   XR_W017_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3002_
  System Id:  1000
  Component Id:  562260100
  Archive is ON for this product.
  _____________________________________________________________
  Product name:  "IBM Multimedia Presentation Manager/2"
  Standard Edition  3.00
  Fixpak name:   XR_W017_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3003_
  System Id:  1000
  Component Id:  562274700
  Archive is ON for this product.
  _____________________________________________________________
  Product name:  "IBM Multimedia Presentation Manager/2"
  Standard Edition  3.01

  
                   FixPak Corrective Service levels and disk layouts  30


                    January 25 1996 Warp FixPak XR_W017

  Fixpak name:   XR_W017_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3004_
  System Id:  1000
  Component Id:  562260100
  Archive is ON for this product.
  _____________________________________________________________
  Product name:  "IBM Multimedia Presentation Manager/2"
  Standard Edition  3.01
  Fixpak name:   XR_W017_   (Country = Generic)
  Pre-requisite CSD Level:  XR_3005_
  System Id:  1000
  Component Id:  562274700
  Archive is ON for this product.
  _____________________________________________________________

  Default directories:

          ..\*

  Files contained in Fixpak for product:

  Filename      Name on CSD   Disk#  Date      Time   Size
  ------------  ------------  -----  --------  -----  -------
  AUDIOSH.DLL   AUDIOSH.DL_     6    11/27/95  19:00      532
  BUSAUDIO.SYS  BUSAUDIO.SY_    7    11/27/95  18:48    27949
  CS4231.SYS    CS4231.SY_      7    06/15/95  15:39    33145
  ES688DD.SYS   ES688DD.SY_     7    11/27/95  18:34    44944
  MEMSH.DLL     MEMSH.DL_       8    11/27/95  18:31    12752
  MMPM.DLL      MMPM.DL_        7    11/27/95  20:36   704504
  MPGIO.DLL     MPGIO.DL_       7    11/27/95  18:53    25219
  MVPRODD.SYS   MVPRODD.SY_     7    11/27/95  19:09    52074
  SB16D2.SYS    SB16D2.SY_      7    11/29/95  10:34    62378
  SBAWED2.SYS   SBAWED2.SY_     7    11/27/95  10:18    88490
  SSM.DLL       SSM.DL_         6    11/27/95  18:13     1044
  SSMDD.SYS     SSMDD.SY_       7    11/27/95  18:15    33272

















  
                   FixPak Corrective Service levels and disk layouts  31


                    January 25 1996 Warp FixPak XR_W017

  SPACE UTILIZATION

  The FixPak installation process needs to write some files to your C:
  drive even if C: is not the drive boot Warp from. These files will be
  deleted when service is complete.

                      Min   Max
                      ---   ---
     PACK.EXE         60k   60k
     IBMCSFLK.EXE     11k   11k
     IBMCSFLK.SYS      4k    4k
     IBMCSFLK.DLL     33k   33k
     IBMCSFLK.MSG      1k    1k
     FIXSTART          2k   15k
     CSF_SEL.000       1k    2k
     --------------------------
     Totals          112k  126k


  Additionally, the following files will be on your boot drive:
































  
                                                   Space Utilization  32


                    January 25 1996 Warp FixPak XR_W017

  In the \OS2\DLL directory:

                      Min   Max
                      ---   ---
     IBMCSFLK.DLL     33k   33k
     --------------------------
     Totals           33k   33k

  In the \OS2\INSTALL directory:

                      Min   Max
                      ---   ---
     SERVICE.LOG      10k   60K
     IBMCSFLK.EXE     11k   11k
     IBMCSFLK.SYS      4k    4k
     IBMCSFLK.DLL     33k   33k
     IBMCSFLK.MSG      1k    1k
     IBMCSFLK.LST      1k   15K
     --------------------------
     Totals           60k  124k

  On all drives being serviced in the directory a supported SYSLEVL
  file was found in:

                      Min   Max
                      ---   ---
     LOGF0000.OS2     10k   100k
     LOGSTART.OS2     10k   100k
     LOCARCH.OS2       5k    15K
     ---------------------------
     Totals           25k   215k


  Files that had service deferred because they were locked (in use by
  the system), are placed in unpacked format in the \IBMCSFLK\FIX
  directory tree on the drive with the most free space.

  The amount of space this requires varies but can be between 1 and
  12MB. These files are then moved to the correct directory on the Warp
  boot drive as part of the Locked File processing which occurs when you
  reboot. The directory and subdirectories are removed as part of this
  processing.










  
                                                   Space Utilization  33
                                            