NETWARE TECH PAPER:

	Western Digital Netware 3.1X and 4.X WD7296 Drivers - V2.10
	============================================================


This disk contains the Western Digital set of Netware 3.1X and 4.X 
drivers for the PCI to SCSI family of host adapters which includes
models WD7193 and WD7197.

This disk provides the following NetWare drivers:

   \NOVELL\V3_1X\WD7296.DSK  -- Netware 3.1X Disk driver for WD7193 and WD7197
   \NOVELL\V3_1X\WDTRAN.DSK  -- Netware 3.1X ASPI Translator for WD7193 and WD7197
   \NOVELL\V4_1X\WD7296.DSK  -- Netware 4.1X Disk driver for WD7193 and WD7197
   \NOVELL\V4_1X\WDTRAN.DSK  -- Netware 4.1X ASPI Translator for WD7193 and WD7197
   \NOVELL\V4_1X\WD7296.DDI  -- Netware 4.1X Installation Info file for WD7296.DSK 
   \NOVELL\V4_1X\WDTRAN.DDI  -- Netware 4.1X Installation Info file for WDTRAN.DSK 

Versions
========
 WD7296.dsk -- V2.10
 WDTRAN.dsk -- V1.07

Installing
==========
To install the Western Digital Netware drivers use the following procedure:

 - Insert the Western Digital Netware diskette into your A: drive.

 - Copy the Netware Western Digital drivers to your Netware directory 
   on the hard disk (usually c:\SERVER.312).
   
	A> COPY A:\NOVELL\V3_1X\WD*.* C:\SERVER.312
   OR
	A> COPY A:\NOVELL\V4_1X\WD*.* C:\NWSERVER

Loading
========
To load the Western Digital Netware disk driver use the following syntax:

	LOAD  [path] WD7296 [options]
	
Example:
	server> LOAD c:\server.312\wd7296

To load the Western Digital ASPI Translator use the following syntax:

	LOAD  [path] WDTRAN [options]
	
Example:
	server> LOAD c:\server.312\wdtran

Requirements
============
- This version requires BIOS 164 or greater
- Supports DOS ASPI build number 135 or greater.
- Do not enable SCAM in the Setup utility, if you are planning to
  use this driver. This release does not support SCAM.



