              OS/2 Video Device Driver for the S3 Trio32/64/64V+
                      Driver Version 2.80.19

  This package contains an OS/2 graphics-accelerator device driver
  supporting the Trio32(732) Trio64(764) and Trio64V+(765) chip sets 
  from S3 Incorporated.

  Important:

  o  "S3 DRV1" must be the label on the installation diskette in this
     package.  This label can be applied using the DOS or OS/2 LABEL
     command.  The installation will fail without this step.

  o  Read this entire document before beginning the device driver
     installation.


  1.0  Supported Features
  _______________________

  This Trio64/64V+ graphics-accelerator device driver provides seamless
  support for accelerated display graphics and advanced color resolutions
  when used with the minimum required video memory.  It conforms to the
  OS/2 32-bit, flat memory model and is designed to function as a
  32-bit Presentation Manager graphics-display device driver under the
  OS/2 32-bit graphics engine.  This device driver supports setting
  the refresh rate using the System - Settings notebook (page 2 of
  the Screen tab) in the OS/2 System Setup folder, and monitor
  detection using Display Data Channel (DDC) protocols.


  1.1  Supported Resolutions

      |========================================|
      | Mode |  Resolution | Memory  |  Trio   |
      |      |             | Required| Family  |
      |      |             |         | 764/765 |
      |      |             |         |   732   |
      |------|-------------|---------|---------|
      |  101 | 640x480x8   |   1 MB  |    Y    |
      |------|-------------|---------|---------|
      |  103 | 800x600x8   |   1 MB  |    Y    |
      |------|-------------|---------|---------|
      |  105 | 1024x768x8  |   1 MB  |    Y    |
      |------|-------------|---------|---------|
      |  107 | 1280x1024x8 |   2 MB  |    Y    |
      |------|-------------|---------|---------|
      |  111 | 640x480x16  |   1 MB  |    Y    |
      |------|-------------|---------|---------|
      |  114 | 800x600x16  |   2 MB  |    Y    |
      |------|-------------|---------|---------|
      |  116 | 1024x768x16 |   2 MB  |    Y    |
      |------|-------------|---------|---------|
      |  212 | 640x480x24  |   1 MB  |   N/S   |
      |------|-------------|---------|---------|
      |  112 | 640x480x32  |   2 MB  |    Y    |
      |========================================|

     NOTES:

     o Y = Supported; N/S = Not Supported.

     o 1 MB only - 640x480x24 is supported for 1 MB memory
       configuration only; for 2 MB and above, 32 bits per pixel (bpp)
       is supported.
    
     o S3 BIOS supports 800x600x16 with 1 MB; S3 OS/2 device driver
       needs 2 MB of memory.

     The 32 bpp device driver might need a large swap space on the
     hard disk, for example, 15 MB.


  2.0  Compatibility
  __________________

  This graphics-accelerator device driver is compatible with OS/2
  2.11, and OS/2 Warp 3.0.

  3.0  DDC Monitor Support
  _______________________________________

  VESA Display Data Channel (DDC) 1 and 2B protocols are supported,
  allowing similarly enabled computers and operating system software
  to identify the monitor and its capabilities.  This device driver
  automatically detects DDC monitor capabilities and sets the display
  to the maximum refresh rate supported by the monitor.  If, after
  installing this device driver, you switch from a non-DDC monitor to
  a DDC monitor or switch to a different DDC monitor, you must run the
  DDC Display Setup program in the System Setup folder.

  Use the following procedures when installing a DDC monitor.

    1. Reset the display to the lowest refresh rate available.  This
       will prevent the system from attempting to display at a refresh
       rate higher than that supported by the new monitor.

    2. Shut down your system and install the new monitor.

    3. Restart your system.

    4. Select the "DDC Display Setup" icon in the OS/2 System Folder.

    5. When you are instructed to do so, shut down your system and
       restart it.


  4.0  Preliminary Steps
  ______________________

  The following steps must be performed before you install the
  Trio64/64V+ graphics-accelerator device driver:

  1.  You must have OS/2 DOS Support installed.
  2.  If you previously installed SVGA support, you must reset the
      resolution to VGA mode, using the procedures in "Setting Your
      Display to VGA Mode" (section 5.0 in this README).
  3.  The device driver diskette must be labeled "S3 DRV1."


  5.0  Setting Your Display to VGA Mode
  _____________________________________

  Use the following procedures to reset to VGA mode.

  NOTE: If your display is out of sync, start OS/2 using the OS/2
        Installation Diskette.  Insert Diskette 1 when prompted, press
        F3 to display a command prompt, and then use the following
        instructions to reset your display mode.

  o   If you are installing this driver on OS/2 Warp, do the
      following:

      1.  Turn on your computer.  If your computer is already on,
          press Ctrl+Alt+Del to restart it.
      2.  When a small white box appears in the upper left-hand corner
          of your screen, press Alt+F1.
      3.  When the Recovery Choices screen appears, press V.

      Your display adapter is restored and can work in VGA mode.  If
      you want to install a new display adapter or video device
      driver, refer to Chapter 16, "Video Procedures," in the User's
      Guide to OS/2 Warp.

  o   If you are installing this driver on OS/2 2.11 or OS/2 for
      Windows, and you installed from diskettes, do the following:

      1.  Before running RSPDSPI, delete the following file:

            [OS2 DRIVE]:\OS2\INSTALL\TRIOV1.DSC

      2.  Be sure RSPDSPI.EXE is in the \OS2\INSTALL directory.  If it
          is, go to step 3.  If it is not, insert Diskette 8 into
          drive A and unpack RSPDSPI.EXE with the following command:

            C:\OS2\UNPACK A:\INSTAID C: /N:RSPDSPI.EXE

          where A: is the drive containing Diskette 8, and C: is the
          drive where OS/2 is installed.

      3.  Type C: and then press Enter.

      4.  Type CD C:\OS2\INSTALL and then press Enter.

      5.  Type the following:

            RSPDSPI /PK:VGA /SK:NONE /S:A:\ /T:C:

          In /T:C:, C: is the target drive where OS/2 is installed.  In /S:A:,
          A: is the source diskette drive for installing the device driver.

          Then press Enter.

    o   If you are installing this driver on OS/2 2.11 or OS/2 for
      Windows, and you installed from CD-ROM or a LAN, do the
      following:

      1.  Before running RSPDSPI, delete the following files:

            [OS2 DRIVE]:\OS2\INSTALL\TRIOV1.DSC

      2.  Be sure RSPDSPI.EXE is in the \OS2\INSTALL directory.  If it
          is, go to step 3.  If it is not, unpack RSPDSPI.EXE with the
          following command:

             C:\OS2\UNPACK E:\DISK_8\INSTAID C: /N:RSPDSPI.EXE

          where C: is the drive where OS/2 is installed, and E: is
          the CD-ROM or LAN drive.

      3.  Type C: and then press Enter.

      4.  Type CD C:\OS2\INSTALL and then press Enter.

      5.  Type the following:

            RSPDSPI /PK:VGA /SK:NONE /S:E:\OS2SE21\ /T:C:

          In /T:C:, C: is the target drive where OS/2 is installed.  In /S:E:,
          E: is the source CD-ROM or LAN drive.

          Then press Enter.

  6.0  Installing from Diskette
  _______________________________

  To install the Trio32/64/64V+ device driver from diskette, do the
  following:

  1.  If system is not in VGA mode, select VGA mode.

  2.  Insert the Trio32/64/64V+ diskette into drive A (or any other
      diskette drive).

      Note: "S3 DRV1" must be the volume label of this diskette.
      To verify the label, use "Label A:".

  3.  Open an OS/2 full-screen or OS/2 window session.

  4.  At the OS/2 command prompt, type the following command to copy
      all necessary files to the OS/2 drive:

        A:SETUP A: C:

      where A: is the diskette drive, and C: is the drive where OS/2
      is installed.

      Then press Enter.

  5.  When prompted to do so, remove the diskette from drive A,
      perform a shutdown, and then restart your computer.

  6.  Open the OS/2 System folder.

  7.  Open the System Setup folder.

  8.  Open the Display Driver Install object or enter "dspinstl" at
      an OS/2 command prompt.  When the Display Driver Install window
      appears, select Primary Display Driver and then select OK.

  9.  When the Display Driver Select window appears, select "S3
      Trio32/64/64V+ [32Bit] Version 2.80.19" to install the video
      driver.

  10. When the Monitor Configuration/Selection Utility window appears,
      the "Install Using Defaults for Monitor Type" choice is
      preselected.  You can accept this choice or select "Install
      Using Display Adapter Utility Program" to choose a different
      refresh rate.  Then select OK.

      If you select the "Install Using Display Adapter Utility
      Program" choice, you must have the DOS monitor utility program
      that came with your display adapter.  Contact the display
      adapter manufacturer's technical support for information on how
      to use the monitor utility program under OS/2.

      NOTE:  DSPINSTL determines the hardware configuration by
             creating the \OS2\SVGADATA.PMI file.  If the
             \OS2\SVGADATA.PMI file has not been created, the adapter
             will not be supported.  This process can take several
             seconds and will black-out the screen.

  11. When the Source Directory pop-up window appears, insert S3
      Trio32/64/64V+ diskette into drive A.  Then select Install.

  12. When the installation is complete, shut down your system, remove
      the diskette, and restart your computer.

  13. When the system has restarted:
      a.  Open the OS/2 System folder.
      b.  Open the System Setup folder.
      c.  Open the System object.
      d.  When the Settings notebook appears, select the Screen tab.
          If your monitor has been detected as Plug and-Play (DDC)
          compatible, go to step 15.

  14. On Screen page 2, select your display from the display list. If
      your display does not appear in the list, select Default.

      It might be necessary to restart your computer to have all
      refresh rate options available.

  15. When the system has restarted:
      a. Open the System object and select Screen page 1, as in step
         13.
      b. Select a screen resolution and a screen refresh rate.
      c. Close the Settings notebook.
      d. Perform a shutdown and restart your computer.

  NOTES:

   o During the installation of this driver, DISPLAY.LOG and
     DSPINSTL.LOG files are created in the OS/2\INSTALL directory.
     These files identify the OS/2 system files that were updated and
     indicate whether the installation was successful.  The contents
     of these files might be useful if you need to report an
     installation problem to IBM.

   o If the video memory size is changed after the device driver is
     installed, the device driver must be reinstalled in order for
     the system to recognize the change.  Not reinstalling the driver
     might result in serious system problems.

  7.0  Installing in a CID Environment
  ______________________________________

  NOTES:

   o The server must contain a directory named S3_DRVS on the same
     drive where the OS/2 diskettes reside.  The S3_DRVS directory
     must contain all of the files from the Trio32/64/64V+ device driver
     diskette.
   o OS/2 must have been successfully installed on the client using
     the CID (Configuration Installation Distribution) method.

  To install the Trio64/64V+ graphics-accelerator device driver
  using CID, use the following information to modify your LCU command
  file.

  NOTE:  The following information is meant as a guide.
         Your LCU command file might be different.

    /*****************************************************/
    /*           LCU PRODUCT DATA SECTION                */
    /*****************************************************/

                          .
                          .
                          .

    x.s3video = 15
    x.15.name='S3 Video'
    x.15.statevar = 'CAS_' || x.15.name
    x.15.instprog = 'x:\img\s3_drvs\SETUP.CMD',
                    ' x:\img\s3_drvs ' || bootdrive || ' CID'
    x.15.rspdir   = ''
    x.15.default  = ''

    x.s3dspinstl = 16
    x.16.name='S3 CID Dspinstl'
    x.16.statevar = 'CAS_' || x.16.name
    x.16.instprog = bootdrive || '\os2\install\DSPINSTL.EXE',
                    ' /pd:' || bootdrive || '\os2\install\TRIOV.dsc',
                    ' /s:x:\img\s3_drvs',
                    ' /t:' || bootdrive,
                    ' /res:640x480x256',
                    ' /u'
    x.16.rspdir   = ''
    x.16.default  = ''

    /*---------------------------------------------------*/
    /*         NUMBER OF PROGRAMS SET UP IN THE          */
    /*               PRODUCT DATA SECTION                */
    /*---------------------------------------------------*/

    NUM_INSTALL_PROGS = 16

    /*****************************************************/
    /*                  INSTALLATION SECTION             */
    /*****************************************************/
                          .
                          .
                          .

        when OVERALL_STATE = 2 then do
          if RunInstall(x.s3video) == BAD_RC then exit
          Call RebootAndGotoState(3)
        end
        when OVERALL_STATE = 3 then do
          if RunInstall(x.s3dspinstl) == BAD_RC then exit
          Call CheckBoot
        end
                          .
                          .
                          .

    /******************************************************/
    /*                ROUTINE SECTION                     */
    /*  The following information should already exist in */
    /*  the LCU command file.                             */
    /******************************************************/
                         .
                         .
                         .
    RebootAndGotoState:
      parse arg new_state, other

      rc2 = SetState(new_state, 'RebootAndGotoState', 1)    /* Set the state */
                                                            /*  to go to in  */
                                                            /* OVERALL_STATE */

      Call SaveStates                           /* Save the environment vars */

      Call Reboot                               /* Reboot the machine */

      return

                          .
                          .
                          .


    /*****************************************************/
                END OF LCU INFORMATION TO BE ADDED
    /*****************************************************/

  Following is an explanation of the line that is
  executed in the LCU command file:

    C:\OS2\INSTALL\DSPINSTL /pd:c:\os2\install\TRIOV1.dsc
    /S:X:\img\s3_drvs /T:C: /res:640x480x256 /u

       /pd:c:\os2\install\TRIOV1.dsc
        is the dsc laid down during setup phase.

       /S:X:\img\s3_drvs
        where X:\img\s3_drvs is the redirected source path.

       /T:C:
        where C: is the drive where OS/2 is installed.

       /res:640x480x256
        is a resolution/color depth from the list of "Supported
        Resolutions" that appears earlier in this README.

       /u
        means Unattended installation.

  NOTES:

   o  Be sure you have the stated video memory required, as listed
      in "Supported Resolutions" earlier in this README.  A safe
      choice is 640x480x256.  Any of the listed resolutions can be
      selected, but your display might be damaged if you select a
      resolution that your display does not support.

   o  After the Trio32/64/64V+ device driver has been successfully
      installed on the client machine using the CID method and the
      client machine is restarted, the resolution will be as specified
      by command line argument.

   o  After the CID installation, refer the end user to section 6.0
      "Installation from Diskette," step 12.

  8.0  Selecting Small or Large Fonts for Windows
  _______________________________________

  The default font sizes for Windows sessions are listed below.

    Resolution      Default Font Size
    ----------      ---------------------------
    640x480             Small
    800x600             Small
    1024x768            Large
    1280x1024           Large
    1600x1200           Large

    NOTE: Large fonts are not available for 640x480 resolution.

  Use the following procedures to select small or large fonts
  for Windows sessions.

    1. Select the "S3 Windows Font Size" object in the OS/2 System
       Setup Folder.

    2. Click on the radio button next to the font size you wish to
       select.

    3. Click on the OK button.

    4. A message will display saying that the new settings will take
       effect the next time you restart your Windows session.
       Currently open sessions will not be affected by the new
       settings.

    5. Click on the OK button.

    6. Start any WIN-OS/2 window or full-screen session.

  The setting you select will remain in effect until you explicitly
  change it, you change your display resolution, or you install a new
  display driver.

  9.0  Features and Fixes Included in this Driver
  _____________________________________________

  - "System - Settings" notebook support for setting refresh rate
  - DDC monitor detection support
  - Windows "Large font" and "Small font" support in high resolutions
  - WIN-OS/2 based on latest S3 Windows 3.1 drivers
  - One-diskette package

  10.0 Limitations
  _______________________

  1. CID install pauses due to SVGA.EXE loading in the background.
     Workaround: In the CID install script, do not initiate any other
     processes until DISPINSTL completes execution.  Ensure that no
     other processes are running during CID install.  This can be
     accomplished by adding the following line to the CONFIGSYS_LINE
     keyword of the CID response file:

     SET RESTART_OBJECTS=STARTUP_FOLDERS_ONLY

  2. During CID install of IBM AntiVirus when using NetView DM/2,
     the OS/2 full screen is displayed as a black screen.
     Workaround: Perform CID install under VGA.

  3. DSPINSTL does not allow CID selection of monitor and refresh
     rate.  The workaround is as follows:

        Requirements:
        * A system with the same graphics card and monitor configured with the
          S3 driver version 2.80.19, the correct display type,
          the desired resolution, and the desired refresh rate.

        Step 1: Copy Configured Video/Display Data Files
        * copy the video and display data files containing information about
          the display type, resolution and refresh rate to the CID server
          (\img\svgadata).

          > copy \os2\svgadata.pmi x:\img\svgadata
          > copy \os2\video.cfg x:\img\svgadata

        Step 2: Create CID Command File
        * create a command file to copy svgadata.pmi and video.cfg to the
          client system's \os2 directory via CID.
        * reboot the client system.
        * the client system will be configured with the correct driver,
          display type, resolution and refresh rate.

  4. Some programs, such as WINBENCH95, WINBENCH96, and After
     Dark 3.0, were written specifically for the Windows environment.
     In the Windows environment, these programs prevent any keystrokes
     from interfering with their proper execution.  However, in the
     OS/2 environment, it is possible to switch context away from the
     Windows session without notifying these programs.  General
     Protection Faults (GPFs) may result.  Therefore, context
     switching during the execution of WINBENCH95 and WINBENCH96 tests
     is not recommended.  Also, context switching during the execution
     of the After Dark 3.0 demo is not recommended.

  5. Problem with IBM AntiVirus 2.2 have been reported. This problem
     can result in a system hang condition and is still under 
     investigation. The driver has been tested with thelatest version 
     (version 2.4) and no problems have been found. If you experience 
     problems with earlier versions, update to version 2.4.

6.  When attempting to start a Win-OS/2 session from a DOS Full screen
    command line, by typing 'WIN' as the executable - you must first be
    sure that the settings of your DOS Full session are changed in the
    following manner:   Right Click on the DOS Full Screen icon and
    choose "Settings", then select the tab - "Sessions".  Select the
    button titles DOS settings, and ensure that "All DOS Settings" is
    selected from the list, then select OK.  From the list of settings
    which appear ensure that "VIDEO_8514A_XGA_IOTRAP" is switched OFF,
    AND "VIDEO_SWITCH_NOTIFICATION" is switched to ON.
                                (End of Document)



