
This document lists some of the popular modem's startup strings and
dip-switch settings. In order, the modems covered here are:

    - US Robotics Courier HST "Dual Standard"
    - Hayes V-Series (older V42 modems)
    - Multitech 224E(h)
    - Hayes 2400
    - Multitech 9600 baud V.32 modem
    - Intel 14.4
    - Practical Peripherals PM14400FXSA
    - Zoom v.32bis
    - Supra 9600
    - Boca 144
    - Hayes Optima 144
    - Telebit QBlazer
    - US Robotics Sportster
    - Zoom v.32bis

Be sure to read the closing notes at the end of this document!!
It explains how to set up most any modem.

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

===========================================
=                                         =
= US Robotics Courier HST "Dual Standard" =
=                                         =
===========================================

    LARGE switch labeled CTS:  UP

The 10 dipswitches next to that large switch are as follows:

    Switch#      Setting

      1            UP
      2           DOWN
      3           DOWN
      4           DOWN
      5            UP
      6            UP
      7            UP
      8           DOWN
      9           DOWN
     10            UP

The following is the configuration parms for the STARTUP.x file:

YMODEMG:      N ; Allow Ymodem-G for non error-correcting modems? (Y/N)
VERBOSE_CONNECT: CONNECT
BAUDRATE:    57600 ; 110,150,300,600,1200,2400,4800,9600,19200,38400,57600,1152
PARITY:       n ; N,E,O,M, or S (None,Even,Odd,Mark,Space)
DATABITS:     8 ; 5, 6, 7, or 8
STOPBITS:     1 ; 1, 1.5, or 2
WAITCARRIER:  40 ; 1 to 255 seconds
MODEMRESET:   AT Z ; Usually AT Z
STARTUP1:     AT &F1 M0 &K3 S2=255 S7=40 &W ; Modem Startup Command
STARTUP2:     ; Modem Startup Command
STARTUP3:     ; Modem Startup Command
REINIT:       AT Z ; Modem Reinitialization string
DELAY1:       1000 ; Modem Delay 1
DELAY2:       100 ; Modem Delay 2
DELAY3:       100 ; Modem Delay 3
DTELOCKED:    y ; y=Lock DTE at BAUDRATE, n=do not lock
ANSWERTYPE:   r ; r=ring detect, a=autoanswer, d=DCD
OPENMODE:     n ; s=shared mode, n=nonshared mode
ANSWERCMD:    ATA ; Modem answer command
ONHOOK:       ATH0 ; Modem command to go onhook (hangup)
OFFHOOK:      ATM0H1 ; Modem command to go offhook
ESC_CMDMODE:  +++ ; Escape Command (enter cmd mode)
ESC_GRDTIME:  700 ; Escape Command Guard Time (ms)
GO_ONLINE:    AT O ; Go back online (leave ESC_CMD)
END_OFFHOOK:  Y ; Place phone offhook at MBBS termination (y=yes,n=no)
ERRORCHECK:   n ; y=error correcting (EC) modem (ie: MNP/ARQ), n=none

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

==================
=                =
= Hayes V-Series =
=                =
==================

VERBOSE_CONNECT: CARRIER
BAUDRATE:     38400 ; 110,150,300,600,1200,2400,4800,9600, or 19200
PARITY:       n ; N,E,O,M, or S (None,Even,Odd,Mark,Space)
DATABITS:     8 ; 5, 6, 7, or 8
STOPBITS:     1 ; 1, 1.5, or 2
WAITCARRIER:  30 ; 1 to 255 seconds
MODEMRESET:   AT Z0 ; Usually AT Z
STARTUP1:     AT &F ; Modem Startup Command
STARTUP2:     AT E1M1L1Q0V1X4B1N1W1Y1S7=30S0=0S2=255S36=3S37=9 ; Modem Startup Command
STARTUP3:     AT S10=3S38=2&C1&D2&G0&K3&P0&Q5&R1&S1&Y0&W0 ; Modem Startup Command
REINIT:       AT Z0 ; Modem Reinitialization string
DELAY1:       1000 ; Modem Delay 1
DELAY2:       2000 ; Modem Delay 2
DELAY3:       2000 ; Modem Delay 3
DTELOCKED:    y ; y=Lock DTE at BAUDRATE, n=do not lock
ANSWERTYPE:   r ; r=ring detect, a=autoanswer
OPENMODE:     n ; s=shared mode, n=nonshared mode
ANSWERCMD:    ATA ; Modem answer command
ONHOOK:       ATH0 ; Modem command to go onhook (hangup)
OFFHOOK:      ATH1 ; Modem command to go offhook
ESC_CMDMODE:  +++ ; Escape Command (enter cmd mode)
ESC_GRDTIME:  700 ; Escape Command Guard Time (ms)
GO_ONLINE:    AT O ; Go back online (leave ESC_CMD)
END_OFFHOOK:  N ; Place phone offhook at MBBS termination (y=yes,n=no)

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

=====================
=                   =
= MultiTech 224E(h) =
=                   =
=====================

The dip-switch settings for this modem are as follows:

The 8-switch block on the bottom of the modem:

    Switch#      Setting

      1            UP
      2           DOWN
      3           DOWN
      4           DOWN
      5           DOWN
      6            UP
      7            UP
      8           DOWN

The 4-switch block on the inside of the modem:

    Switch#      Setting

      1           DOWN
      2            UP
      3           DOWN
      4           DOWN

All jumpers on the inside of the modem (there's 3 of them) should be jumpered
towards the front two pins. The front is the side where the modem lights are.

The following is the configuration parameters for your STARTUP.x file:

YMODEMG:      N ; Allow Ymodem-G for non error-correcting modems? (Y/N)
BAUDRATE:     9600 ; 110,150,300,600,1200,2400,4800,9600,19200,38400,57600
PARITY:       n ; N,E,O,M, or S (None,Even,Odd,Mark,Space)
DATABITS:     8 ; 5, 6, 7, or 8
STOPBITS:     1 ; 1, 1.5, or 2
WAITCARRIER:  30 ; 1 to 255 seconds
MODEMRESET:   AT Z ; Usually AT Z
STARTUP1:     AT &F ; Modem Startup Command
STARTUP2:     AT E0&E1&E4&E15&Q0V0M0S7=30X1S2=255 ; Modem Startup Command
STARTUP3:     AT S0=0&BS0&B1$SB9600$BA0&W0 ; Modem Startup Command
REINIT:       AT Z ; Modem Reinitialization string
DELAY1:       500 ; Modem Delay 1
DELAY2:       2500 ; Modem Delay 2
DELAY3:       1500 ; Modem Delay 3
DTELOCKED:    y ; y=Lock DTE at BAUDRATE, n=do not lock
ANSWERTYPE:   r ; r=ring detect, a=autoanswer, d=DCD
OPENMODE:     n ; s=shared mode, n=nonshared mode
ANSWERCMD:    ATA ; Modem answer command
ONHOOK:       ATH0 ; Modem command to go onhook (hangup)
OFFHOOK:      ATH1 ; Modem command to go offhook
ESC_CMDMODE:  +++ ; Escape Command (enter cmd mode)
ESC_GRDTIME:  700 ; Escape Command Guard Time (ms)
GO_ONLINE:    AT O ; Go back online (leave ESC_CMD)
END_OFFHOOK:  N ; Place phone offhook at MBBS termination (y=yes,n=no)
RC_110:        ; Result Code for 110 baud
RC_150:        ; Result Code for 150 baud
RC_300:       1 ; Result Code for 300 baud
RC_600:        ; Result Code for 600 baud
RC_1200:      5 ; Result Code for 1200 baud
RC_2400:      9 ; Result Code for 2400 baud
RC_4800:       ; Result Code for 4800 baud
RC_9600:       ; Result Code for 9600 buad
RC_12000:      ; Result Code for 12000 baud
RC_14400:      ; Result Code for 14400 baud
RC_16800:      ; Result Code for 16800 baud
RC_19200:      ; Result Code for 19200 baud
ERRORCHECK:   y ; y=error correcting (EC) modem (ie: MNP/ARQ), n=none
ERC_110:       ; EC Result Code for 110 baud
ERC_150:       ; EC Result Code for 150 baud
ERC_300:       ; EC Result Code for 300 baud
ERC_600:       ; EC Result Code for 600 baud
ERC_1200:     5R ; EC Result Code for 1200 baud
ERC_2400:     9R ; EC Result Code for 2400 baud
ERC_4800:      ; EC Result Code for 4800 baud
ERC_9600:      ; EC Result Code for 9600 baud
ERC_12000:     ; EC Result Code for 12000 baud
ERC_14400:     ; EC Result Code for 14400 baud
ERC_16800:     ; EC Result Code for 16800 baud
ERC_19200:     ; EC Result Code for 19200 baud

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

==============
=            =
= Hayes 2400 =
=            =
==============

   VERBOSE_CONNECT: CONNECT
   BAUDRATE:    2400
   PARITY:      n
   DATABITS:    8
   STOPBITS:    1
   WAITCARRIER: 30
   MODEMRESET:
   STARTUP1:    AT &F&W
   STARTUP2:    AT S10=7E0V1M0Q0&C1&D2S0=1&W
   STARTUP3:
   REINIT:
   DELAY1:      1500
   DELAY2:      1500
   DELAY3:      2500
   DTELOCKED:   n
   ANSWERTYPE:  a
   OPENMODE:    n
   ANSWERCMD:   ATA
   ONHOOK:      ATH0
   OFFHOOK:     ATH1
   ESC_CMDMODE: +++
   ESC_GRDTIM:  700
   GO_ONLINE:   AT O
   END_OFFHOOK: N
   ERRORCHECK:  n

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

==================================
=                                =
= Multitech 9600 baud V.32 modem =
=                                =
==================================


The dip-switch settings for this modem are as follows:

The 4-switch block:

    Switch#      Setting

      1           DOWN
      2            UP
      3           DOWN
      4           DOWN

The 8-switch block:

    Switch#      Setting

      1            UP
      2           DOWN
      3           DOWN
      4           DOWN
      5            UP
      6            UP
      7            UP
      8           DOWN

Startup Sequences:

   BAUDRATE:    19200
   PARITY:      n
   DATABITS:    8
   STOPBITS:    1
   WAITCARRIER: 30
   MODEMRESET:  AT Z
   STARTUP1:    AT &F
   STARTUP2:    AT E0 &E1 &E4 &E15 $SB19200 $BA0 &R1
   STARTUP3:    AT V0 M1 Q0 X1 S0=1 S2=255 S7=30 &W0
   REINIT:      AT Z
   DELAY1:      1000
   DELAY2:      1500
   DELAY3:      1500
   DTELOCKED:   y
   ANSWERTYPE:  a
   OPENMODE:    n
   ANSWERCMD:   ATA
   ONHOOK:      ATH0
   OFFHOOK:     ATH1
   ESC_CMDMODE: +++
   ESC_GRDTIME: 1200
   GO_ONLINE:   AT O
   END_OFFHOOK: N
   RC_110:
   RC_150:
   RC_300:      1
   RC_600:
   RC_1200:     5
   RC_2400:     9
   RC_4800:     11
   RC_9600:     12
   RC_19200:
   ERRORCHECK:  y
   ERC_110:
   ERC_150:
   ERC_300:     1R
   ERC_600:
   ERC_1200:    5R
   ERC_2400:    9R
   ERC_4800:    11R
   ERC_9600:    12R
   ERC_19200:

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

====================
=                  =
= Intel 14.4 modem =
=                  =
====================
;
;
; Magnum BBS Config Parms for Intel 14,400 baud Modem
;
;
YMODEMG:      Y ; Allow Ymodem-G for non error-correcting modems? (Y/N)
;
VERBOSE_CONNECT: CONNECT ; Usually CONNECT or CARRIER
;
BAUDRATE:     38400 ; 110,150,300,600,1200,2400,4800,9600,19200,38400
PARITY:       n ; N,E,O,M, or S (None,Even,Odd,Mark,Space)
DATABITS:     8 ; 5, 6, 7, or 8
STOPBITS:     1 ; 1, 1.5, or 2
WAITCARRIER:  30 ; 1 to 255 seconds
MODEMRESET:   AT Z ; Usually AT Z
STARTUP1:     AT Z ; Modem Startup Command
STARTUP2:     AT E0&Q0V1M1Q0S7=30X1L0 ; Modem Startup Command
STARTUP3:     AT S0=1S2=255&R1&C1&W0 ; Modem Startup Command
REINIT:       AT Z ; Modem Reinitialization string
DELAY1:       1200 ; Modem Delay 1
DELAY2:       1200 ; Modem Delay 2
DELAY3:       1200 ; Modem Delay 3
DTELOCKED:    y ; y=Lock DTE at BAUDRATE, n=do not lock
ANSWERTYPE:   a ; r=ring detect, a=autoanswer
OPENMODE:     n ; s=shared mode, n=nonshared mode
ANSWERCMD:    ATA ; Modem answer command
ONHOOK:       ATH0 ; Modem command to go onhook (hangup)
OFFHOOK:      ATM0H1 ; Modem command to go offhook
ESC_CMDMODE:  +++ ; Escape Command (enter cmd mode)
ESC_GRDTIME:  700 ; Escape Command Guard Time (ms)
GO_ONLINE:    AT O ; Go back online (leave ESC_CMD)
END_OFFHOOK:  Y ; Place phone offhook at MBBS termination (y=yes,n=no)
ERRORCHECK:   n ; y=error correcting (EC) modem (ie: MNP/ARQ), n=none

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

============================================
=                                          =
= Practical Peripherals PM 14400FXSA Modem =
=                                          =
============================================

;
;
; Magnum BBS Config Parms for Practical Peripherals PM14400FXSA External Modem
;
;
YMODEMG:      Y ; Allow Ymodem-G for non error-correcting modems? (Y/N)
;
VERBOSE_CONNECT: CONNECT ; Usually CONNECT or CARRIER
;
BAUDRATE:     38400 ; 110,150,300,600,1200,2400,4800,9600,19200,38400
PARITY:       n ; N,E,O,M, or S (None,Even,Odd,Mark,Space)
DATABITS:     8 ; 5, 6, 7, or 8
STOPBITS:     1 ; 1, 1.5, or 2
WAITCARRIER:  30 ; 1 to 255 seconds
MODEMRESET:   AT Z1 ; Usually AT Z
STARTUP1:     AT &F1M1L0 ; Modem Startup Command
STARTUP2:     AT Q0V1S7=30X1S0=0S2=255W2S37=11N1S38=0 ; Modem Startup Command
STARTUP3:     AT &C1&D3&K3&Q5&Y1&W1 ; Modem Startup Command
REINIT:       AT Z1 ; Modem Reinitialization string
DELAY1:       1200 ; Modem Delay 1
DELAY2:       1200 ; Modem Delay 2
DELAY3:       1200 ; Modem Delay 3
DTELOCKED:    y ; y=Lock DTE at BAUDRATE, n=do not lock
ANSWERTYPE:   r ; r=ring detect, a=autoanswer
OPENMODE:     n ; s=shared mode, n=nonshared mode
ANSWERCMD:    ATA ; Modem answer command
ONHOOK:       ATH0 ; Modem command to go onhook (hangup)
OFFHOOK:      ATM0H1&D2 ; Modem command to go offhook
ESC_CMDMODE:  +++ ; Escape Command (enter cmd mode)
ESC_GRDTIME:  700 ; Escape Command Guard Time (ms)
GO_ONLINE:    AT O ; Go back online (leave ESC_CMD)
END_OFFHOOK:  Y ; Place phone offhook at MBBS termination (y=yes,n=no)
ERRORCHECK:   n ; y=error correcting (EC) modem (ie: MNP/ARQ), n=none

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

======================
=                    =
= Zoom v.32bis modem =
=                    =
======================
;
;
; Magnum BBS Config Parms for Zoom v.32bis Modem
;
;
YMODEMG:      Y ; Allow Ymodem-G for non error-correcting modems? (Y/N)
;
VERBOSE_CONNECT: CONNECT ; Usually CONNECT or CARRIER
;
BAUDRATE:     38400 ; 110,150,300,600,1200,2400,4800,9600,19200,38400
PARITY:       n ; N,E,O,M, or S (None,Even,Odd,Mark,Space)
DATABITS:     8 ; 5, 6, 7, or 8
STOPBITS:     1 ; 1, 1.5, or 2
WAITCARRIER:  30 ; 1 to 255 seconds
MODEMRESET:   AT Z0 ; Usually AT Z
STARTUP1:     AT B1N1V1W1X4
STARTUP2:     AT &C1&D2&K3&Q5&R0&S0&X2
STARTUP3:     AT S7=30S36=7S46=136S48=7&Y0&W0
REINIT:       AT Z0 ; Modem Reinitialization string
DELAY1:       1200 ; Modem Delay 1
DELAY2:       1200 ; Modem Delay 2
DELAY3:       1200 ; Modem Delay 3
DTELOCKED:    y ; y=Lock DTE at BAUDRATE, n=do not lock
ANSWERTYPE:   r ; r=ring detect, a=autoanswer
OPENMODE:     n ; s=shared mode, n=nonshared mode
ANSWERCMD:    ATA ; Modem answer command
ONHOOK:       ATH0 ; Modem command to go onhook (hangup)
OFFHOOK:      ATM0H1&D2 ; Modem command to go offhook
ESC_CMDMODE:  +++ ; Escape Command (enter cmd mode)
ESC_GRDTIME:  700 ; Escape Command Guard Time (ms)
GO_ONLINE:    AT O ; Go back online (leave ESC_CMD)
END_OFFHOOK:  Y ; Place phone offhook at MBBS termination (y=yes,n=no)
ERRORCHECK:   n ; y=error correcting (EC) modem (ie: MNP/ARQ), n=none

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

==============
=            =
= Supra 9600 =
=            =
==============

YMODEMG:      N ; Allow Ymodem-G for non error-correcting modems? (Y/N)
VERBOSE_CONNECT: CARRIER ; Usually CONNECT or CARRIER
BAUDRATE:     19200 ; 110,150,300,600,1200,2400,4800,9600,19200,38400,57600
PARITY:       n ; N,E,O,M, or S (None,Even,Odd,Mark,Space)
DATABITS:     8 ; 5, 6, 7, or 8
STOPBITS:     1 ; 1, 1.5, or 2
WAITCARRIER:  30 ; 1 to 255 seconds
MODEMRESET:      ; Usually AT Z
STARTUP1:     AT &F2 %C0 &D2 ; Modem Startup Command
STARTUP2:     AT &C1 V1 M0 Q W1 ; Modem Startup Command
STARTUP3:     AT S0=1 ; Modem Startup Command
REINIT:               ; Modem Reinitialization string
DELAY1:       1500 ; Modem Delay 1
DELAY2:       1500 ; Modem Delay 2
DELAY3:       1500 ; Modem Delay 3
DTELOCKED:    y ; y=Lock DTE at BAUDRATE, n=do not lock
ANSWERTYPE:   a ; r=ring detect, a=autoanswer, d=DCD
OPENMODE:     n ; s=shared mode, n=nonshared mode
ANSWERCMD:    ATA ; Modem answer command
ONHOOK:       ATH0 ; Modem command to go onhook (hangup)
OFFHOOK:      ATH1 ; Modem command to go offhook
ESC_CMDMODE:  +++ ; Escape Command (enter cmd mode)
ESC_GRDTIME:  1000 ; Escape Command Guard Time (ms)
GO_ONLINE:    AT O ; Go back online (leave ESC_CMD)
END_OFFHOOK:  Y ; Place phone offhook at MBBS termination (y=yes,n=no)
ERRORCHECK:   n ; y=error correcting (EC) modem (ie: MNP/ARQ), n=none

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

===========
=         =
= BOCA144 =
=         =
===========

YMODEMG:      N ; Allow Ymodem-G for non error-correcting modems? (Y/N)
VERBOSE_CONNECT: CONNECT ; Usually CONNECT or CARRIER
BAUDRATE:     38400 ; 110,150,300,600,1200,2400,4800,9600,19200,38400,57600
PARITY:       n ; N,E,O,M, or S (None,Even,Odd,Mark,Space)
DATABITS:     8 ; 5, 6, 7, or 8
STOPBITS:     1 ; 1, 1.5, or 2
WAITCARRIER:  60 ; 1 to 255 seconds
MODEMRESET:   AT Z ; Usually AT Z
STARTUP1:     AT &F ; Modem Startup Command
STARTUP2:     AT E1 S7=60 S11=60 V1 X1 Q0 S0=0 &W ; Modem Startup Command
STARTUP3:     ; Modem Startup Command
REINIT:       AT Z ; Modem Reinitialization string
DELAY1:       1000 ; Modem Delay 1
DELAY2:       1000 ; Modem Delay 2
DELAY3:       100 ; Modem Delay 3
DTELOCKED:    y ; y=Lock DTE at BAUDRATE, n=do not lock
ANSWERTYPE:   r ; r=ring detect, a=autoanswer, d=DCD
OPENMODE:     n ; s=shared mode, n=nonshared mode
ANSWERCMD:    ATA ; Modem answer command
ONHOOK:       ATH0 ; Modem command to go onhook (hangup)
OFFHOOK:      ATH1 ; Modem command to go offhook
ESC_CMDMODE:  +++ ; Escape Command (enter cmd mode)
ESC_GRDTIME:  1000 ; Escape Command Guard Time (ms)
GO_ONLINE:    AT O ; Go back online (leave ESC_CMD)
END_OFFHOOK:  Y ; Place phone offhook at MBBS termination (y=yes,n=no)
ERRORCHECK:   n ; y=error correcting (EC) modem (ie: MNP/ARQ), n=none

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

====================
=                  =
= HAYES OPTIMA 144 =
=                  =
====================

YMODEMG:      N ; Allow Ymodem-G for non error-correcting modems? (Y/N)
VERBOSE_CONNECT: CONNECT ; Usually CONNECT or CARRIER
BAUDRATE:     38400 ; 110,150,300,600,1200,2400,4800,9600,19200,38400,57600
PARITY:       n ; N,E,O,M, or S (None,Even,Odd,Mark,Space)
DATABITS:     8 ; 5, 6, 7, or 8
STOPBITS:     1 ; 1, 1.5, or 2
WAITCARRIER:  40 ; 1 to 255 seconds
MODEMRESET:   AT Z0 ; Usually AT Z
STARTUP1:     AT &F ; Modem Startup Command
STARTUP2:     AT V1L1&C1&D2W2S7=40S95=2S2=255S38=1&Y0&W0 ; Startup Command
STARTUP3:     ; Modem Startup Command
REINIT:       AT Z0 ; Modem Reinitialization string
DELAY1:       1000 ; Modem Delay 1
DELAY2:       2500 ; Modem Delay 2
DELAY3:       100 ; Modem Delay 3
DTELOCKED:    y ; y=Lock DTE at BAUDRATE, n=do not lock
ANSWERTYPE:   r ; r=ring detect, a=autoanswer, d=DCD
OPENMODE:     n ; s=shared mode, n=nonshared mode
ANSWERCMD:    ATA ; Modem answer command
ONHOOK:       ATH0 ; Modem command to go onhook (hangup)
OFFHOOK:      ATH1 ; Modem command to go offhook
ESC_CMDMODE:  +++ ; Escape Command (enter cmd mode)
ESC_GRDTIME:  1000 ; Escape Command Guard Time (ms)
GO_ONLINE:    AT O ; Go back online (leave ESC_CMD)
END_OFFHOOK:  Y ; Place phone offhook at MBBS termination (y=yes,n=no)
ERRORCHECK:   n ; y=error correcting (EC) modem (ie: MNP/ARQ), n=none

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

===================
=                 =
= TELEBIT QBLAZER =
=                 =
===================

The STARTUP strings on file for this modem are:

WAITCARRIER: 40
MODEMRESET:  AT Z0
STARTUP1:    AT &F
STARTUP2:    AT E1V1Q0X2S0=2S51=4
STARTUP3:    AT &C1&D2S58=2S59=15&W0
REINIT:      AT Z0
DELAY1:      1000
DELAY2:      1000
DELAY3:      1000
DTELOCKED:   y
ANSWERTYPE:  a

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

=========================
=                       =
= US Robotics Sportster =
=                       =
=========================


The 8 dipswitch settings are:

    Switch#      Setting

      1            UP
      2            UP
      3           DOWN
      4            UP
      5           DOWN
      6            UP
      7            UP
      8           DOWN


YMODEMG:      N ; Allow Ymodem-G for non error-correcting modems? (Y/N)
VERBOSE_CONNECT: CONNECT
BAUDRATE:    57600 ; 110,150,300,600,1200,2400,4800,9600,19200,38400,57600,1152
PARITY:       n ; N,E,O,M, or S (None,Even,Odd,Mark,Space)
DATABITS:     8 ; 5, 6, 7, or 8
STOPBITS:     1 ; 1, 1.5, or 2
WAITCARRIER:  45 ; 1 to 255 seconds
MODEMRESET:   AT Z ; Usually AT Z
STARTUP1:     AT &F ; Modem Startup Command
STARTUP2:     AT Q0V1X4B0S7=45S0=0S2=255S15=8S10=14; Modem Startup Command
STARTUP3:     AT &A3&B1&H1&I0&K3&M4&N0&R2&S0&Y1&W ; Modem Startup Command
REINIT:       AT Z ; Modem Reinitialization string
DELAY1:       2500 ; Modem Delay 1
DELAY2:       2500 ; Modem Delay 2
DELAY3:       2500 ; Modem Delay 3
DTELOCKED:    y ; y=Lock DTE at BAUDRATE, n=do not lock
ANSWERTYPE:   r ; r=ring detect, a=autoanswer, d=DCD

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

================
=              =
= ZOOM v.32bis =
=              =
================

YMODEMG:      N ; Allow Ymodem-G for non error-correcting modems? (Y/N)
VERBOSE_CONNECT: CONNECT ; Usually CONNECT or CARRIER
BAUDRATE:     38400 ; 110,150,300,600,1200,2400,4800,9600,19200,38400,57600
PARITY:       n ; N,E,O,M, or S (None,Even,Odd,Mark,Space)
DATABITS:     8 ; 5, 6, 7, or 8
STOPBITS:     1 ; 1, 1.5, or 2
WAITCARRIER:  40 ; 1 to 255 seconds
MODEMRESET:   AT Z ; Usually AT Z
STARTUP1:     AT &F ; Modem Startup Command
STARTUP2:     AT V1B1N1W1X4&C1&D2&K3&Q5&R0&S0&X2 ; Startup Command
STARTUP3:     AT S0=0 S7=40 S36=7 S46=136 S48=7 &Y0 &W0 ; Modem Startup Command
REINIT:       AT Z ; Modem Reinitialization string
DELAY1:       1000 ; Modem Delay 1
DELAY2:       2500 ; Modem Delay 2
DELAY3:       2000 ; Modem Delay 3
DTELOCKED:    y ; y=Lock DTE at BAUDRATE, n=do not lock
ANSWERTYPE:   r ; r=ring detect, a=autoanswer, d=DCD
OPENMODE:     n ; s=shared mode, n=nonshared mode
ANSWERCMD:    ATA ; Modem answer command
ONHOOK:       ATH0 ; Modem command to go onhook (hangup)
OFFHOOK:      ATH1 ; Modem command to go offhook
ESC_CMDMODE:  +++ ; Escape Command (enter cmd mode)
ESC_GRDTIME:  1000 ; Escape Command Guard Time (ms)
GO_ONLINE:    AT O ; Go back online (leave ESC_CMD)
END_OFFHOOK:  Y ; Place phone offhook at MBBS termination (y=yes,n=no)
ERRORCHECK:   n ; y=error correcting (EC) modem (ie: MNP/ARQ), n=none

===========================================================================

                               IMPORTANT!
                             CLOSING NOTES.

Modem models change very fast!

For the fastest possible setup for any modem, once you've filled in your
STARTUPx strings, use Verbose (word) result codes (a V1 anywhere in
your STARTUP strings should turn on verbose result codes). Then:

   VERBOSE_CONNECT: CONNECT
                  (Some Hayes models may need  VERBOSE_CONNECT: CARRIER)
   YMODEMG: N

and delete all text lines starting with RC_, ERC_, ERCA_, ERCB_ if any of
these appear in your STARTUP.n file(s).

Additionally, create a SPECIAL.x (x=node#) file in your PGM_DIR for that
node.  The contents should be:

     ARQ {
         ec
         }

     MNP {
         ec
         }

     LAP {
         ec
         }

     CONNECT {
             log
             }

===========================================================================
