POWER CONTROL FOR REMOTE PCs -- 24 HOURS A DAY

Upgraded Version Of 'Remote Power On/Off' Features New Reboot And
Line-Sharing Capabilities

SUNNYVALE, CA--Server Technology, Inc. introduces Remote Power On/Off+Aux,
an upgraded version of the company's telephone-activated power switch for
remote PCs. New features include a variety of reboot enhancements,
including an off-hook two-hour reboot-power limit that prevents a stuck
modem from locking up the line indefinitely, and the ability to share
either a modem and answering machine or a modem and fax machine on one
phone line.

Remote Power On/Off + Aux automatically turns on a remote PC when a phone
call is detected, permitting 24-hour access without the need to leave the
PC running continuously, and reboots locked-up PCs for remote users. It
consists of two hardware components -- a small control box and a power
module that plugs into the phone outlet -- that detect the RING and ONHOOK
telephone signals.

Three Operating Modes

There are three operating modes. The first, designed primarily for the
single remote user who needs access to the office PC when it is turned
off, powers on a remote PC when a ring is detected and turns it off when
the call has ended. It supports both data modems and fax modems.

The second is a new AUX Port Mode that allows homes or offices with single
phone lines to share a PC's modem with an answering or fax machine. This
eliminates the need for a dedicated modem line.

The third, aimed at the PC that runs 24 hours a day and supports multiple
remote users, reboots a locked-up workstation, gateway or server with one
phone call. Enhancements include:

* An off-hook two-hour reboot-power limit that prevents a stuck
  modem from locking up the line indefinitely.
* An immediate 1-second reboot useful for high-traffic BBS or
  e-mail systems
* A reboot-power safeguard that prevents continuous linked reboots
  in high-traffic systems.

Other Features, Pricing

Users can program the device to power on a remote PC after either 1, 6 or
12 rings and to turn it off in either 2, 15 or 60 minutes after hang-up.
Installation requires three cables, which are provided.

Remote Power On/Off + Aux lists for $169.95. It is also available bundled
with pcANYWHERE for $199.95. It is fully compatible with standard internal
or external modems, comm software and remote control applications such as
pcANYWHERE, Carbon Copy, CoSession, Close-Up, ProCOMM, LapLink and others.
It also runs with NetWare.

It is sold through PC Connection, MicroWarehouse and Elek-Tek or by calling
Server Technology at 800/835-1515 or 408/745-0300. Remote Power On/Off is
distributed through Ingram Micro and Merisel. Internet address is
http://www.powerboot.com.
---------------------------------------------------------------------
Server Technology, founded in 1984, develops and manufactures remote power
control products. They are a forerunner in the remote power control
industry, providing solutions for traveling laptop users and LAN and WAN
Network Administrators, and now with the VersaTimer, the home consumer as
well. Server Technology Products include the VersaTimer, Remote Power
On/Off and Sentry Network Power Managers.

Server Technology
1288 Hammerwood Ave
Sunnyvale, CA 94089
408-745-0300,  800-835-1515,  fax 408-745-0392

 ============================================================
 From the  'New Product News'  Electronic News Service on....
 AOL (Keyword = New Products) & Delphi (GO COMPUTING PRODUCT)
 ============================================================
 This information was processed from data provided by the 
 company or author mentioned. For additional details, please 
 contact them directly at the address/phone number indicated.
 All trademarks are the property of their respective owners.
 ============================================================
 All submissions for this service should be addressed to:
 BAKER ENTERPRISES,  20 Ferro Dr,  Sewell, NJ  08080  U.S.A.
 Email: RBakerPC (AOL/Delphi), rbakerpc@delphi.com (Internet)
 ============================================================
