Intel Introduces Fastest Pentium Processor Designed For Mobile Computers

Sets Stage for Broad Product Offerings Based on Pentium Processors

SANTA CLARA, CALIF. October 23, 1995 -- Intel Corporation today introduced
a 120-MHz Pentium processor, continuing to set the pace for desktop-
equivalent performance in mobile computers. The fastest Pentium processor
for notebooks will continue to accelerate the trend toward integrating
advanced desktop features into mobile systems. Many systems based on the
120-MHz Pentium processor will include multimedia capabilities such as
sound and full-motion video, larger and higher resolution screens and
exchangeable peripherals such as CD-ROMs.

The Pentium processor at iCOMP index 1000/120 is also the first
microprocessor for mobile systems built on Intel's advanced .35 micron
manufacturing technology, resulting in a chip the size of a small child's
fingernail, but containing 3.3 million transistors. The small chip size
makes it possible for systems to deliver the highest level of performance
with very low power consumption for long battery life. The 120-MHz Pentium
processor is the third member of the Pentium processor family to be
introduced in a year.

"The 120-MHz Pentium processor in notebooks will offer a no-compromise
solution to professionals who need high performance and multimedia
capabilities commonly found in desktop systems today," said Stephen P.
Nachtsheim, vice president, Mobile and Handheld Products Group. "For
mobile users, its introduction broadens the selection of price and
performance choices based on the Pentium processor family."

IDC estimates that the worldwide mobile computing market will exceed 9.5
million units this year. This will be a 29 percent increase over 1994,
compared with 20 percent for the desktop market segment, making the
portable market segment one of the fastest growing in the industry. Key
elements driving the market are the expected rapid upgrade by users to
color displays and to Pentium processors, and the emergence of a
high-volume value market, according to IDC.

Like the 90- and 75-MHz processors for mobile systems introduced in the
past year, the 120-MHz Pentium processor is offered in an innovative
postage-stamp sized package. The processor has a dual voltage capability
that allows high-performance processors to operate in a thermally
efficient manner.

The 120-MHz Pentium processor in the thin, light-weight Tape Carrier
Package (TCP) offers a highly efficient means for managing thermal
elements in mobile systems. Voltage Reduction Technology enables the
120-MHz Pentium processor to interface at 3.3 volts with other
off-the-shelf components, while its inner core operates at a lower power,
2.9 volts. Voltage Reduction Technology allows the processor to deliver up
to 30 percent more performance than the 90-MHz Pentium processor but at
the same power consumption.

The 120-MHz Pentium processor for mobile systems is available in both Tape
Carrier Packaging (TCP) and conventional ceramic packaging with built-in
Voltage Reduction Technology. In 1,000-unit quantities it is priced at
$681. The price of the 90-MHz Pentium processor is $341, while the 75-MHz
Pentium processor is $204 in 1,000-unit quantities. For pricing and
availability outside the United States, contact a regional Intel sales
office. Phone numbers are listed in the Worldwide Customer Information and
Support Network.

The 120-MHz Pentium processor delivers 172 SPECint92 and 108 SPECfp92 of
performance, and SPECint95 performance of 3.72 and SPECfp95 performance of
2.81. It has a typical power dissipation of 2.5 to 3.5 watts and idle
power consumption of less than 1 watt.

Intel, the world's largest chip maker, is also a leading manufacturer of
personal computer, networking, and communications products.
 
 =========================================================
 From the 'New Product News' Electronic News Service on...
 AOL (Keyword = New Products) and Delphi (GO COMP PROD)
 =========================================================
 This information was processed from data provided by the
 company/author mentioned. For additional details, please
 contact them directly at the address/phone# indicated.
 Trademarks are the property of their respective owners.
 =========================================================
 All submissions for this service should be addressed to:
 BAKER ENTERPRISES,  20 Ferro Dr,  Sewell, NJ  08080  USA
 Email: rbakerpc@delphi.com  -or- RBakerPC (on AOL/Delphi)
 =========================================================
