Z80 Opcode Listing
Z-80 CPU Instruction Set
---- --- ----------- ---

ADC   HL,ss       Add with carry register pair ss to HL.
ADC   A,s         Add with carry operand s to accumulator.
ADD   A,n         Add value n to accumulator.
ADD   A,r         Add register r to accumulator.
ADD   A,(HL)      Add location (HL) to acccumulator.
ADD   A,(IX+d)    Add location (IX+d) to accumulator.
ADD   A,(IY+d)    Add location (IY+d) to accumulator.
ADD   HL,ss       Add register pair ss to HL.
ADD   IX,pp       Add register pair pp to IX.
ADD   IY,rr       Add register pair rr to IY.
AND   s           Logical AND of operand s to accumulator.
BIT   b,(HL)      Test bit b of location (HL).
BIT   b,(IX+d)    Test bit b of location (IX+d).
BIT   b,(IY+d)    Test bit b of location (IY+d).
BIT   b,r         Test bit b of register r.
CALL  cc,nn       Call subroutine at location nn if condition CC is true.
CCF               Complement carry flag.
CP    s           Compare operand s with accumulator.
CPD               Comapre location (HL) and acc., decrement HL and BC,
CPDR              Perform a CPD and repeat until BC=0.
CPI               Compare location (HL) and acc., incr HL, decr BC.
CPIR              Perform a CPI and repeat until BC=0.
CPL               Complement accumulator (1's complement).
DAA               Decimal adjust accumulator.
DEC   m           Decrement operand m.
DEC   IX          Decrement IX.
DEC   IY          Decrement IY.
DEC   ss          Decrement register pair ss.
DI                Disable interrupts.
DJNZ  e           Decrement B and jump relative if B=0.
EI                Enable interrupts.
EX    (SP),HL     Exchange the location (SP) and HL.
EX    (SP),IX     Exchange the location (SP) and IX.
EX    (SP),IY     Exchange the location (SP) and IY.
EX    AF,AF'      Exchange the contents of AF and AF'.
EX    DE,HL       Exchange the contents of DE and HL.
EXX               Exchange the contents of BC,DE,HL with BC',DE',HL'.
HALT              Halt computer and wait for interrupt.
IM    0           Set interrupt mode 0.
IM    1           Set interrupt mode 1.
IM    2           Set interrupt mode 2.
IN    A,(n)       Load the accumulator with input from device n.
IN    r,(c)       Load the register r with input from device (C).
INC   (HL)        Increment location (HL).
INC   IX          Increment IX.
INC   (IX+d)      Increment location (IX+d).
INC   IY          Increment IY.
INC   (IY+d)      Increment location (IY+d).
INC   r           Increment register r.
INC   ss          Increment register pair ss.
IND               (HL)=Input from port (C). Decrement HL and B.
INDR              Perform an IND and repeat until B=0.
INI               (HL)=Input from port (C). HL=HL+1. B=B-1.
INIR              Perform an INI and repeat until B=0.
JP    (HL)        Unconditional jump to location (HL).
JP    (IX)        Unconditional jump to location (IX).
JP    (IY)        Unconditional jump to location (IY).
JP    cc,nn       Jump to location nn if condition cc is true.
JR    C,e         Jump relative to PC+e if carry=1.
JR    e           Unconditional jump relative to PC+e.
JR    NC,e        Jump relative to PC+e if carry=0.
JR    NZ,e        Jump relative to PC+e if non zero (Z=0).
JR    Z,e         Jump relative to PC+e if zero (Z=1).
LD    A,(BC)      Load accumulator with location (BC).
LD    A,(DE)      Load accumulator with location (DE).
LD    A,I         Load accumulator with I.
LD    A,(nn)      Load accumulator with location nn.
LD    A,R         Load accumulator with R.
LD    (BC),A      Load location (BC) with accumulator.
LD    (DE),A      Load location (DE) with accumulator.
LD    (HL),A      Load location (HL) with accumulator.
LD    dd,nn       Load register pair dd with nn.
LD    dd,(nn)     Load register pair dd with location (nn).
LD    HL,(nn)     Load HL with location (nn).
LD    (HL),r      Load location (HL) with register r.
LD    I,A         Load I with accumulator.
LD    IX,nn       Load IX with value nn.
LD    IX,(nn)     Load IX with location (nn).
LD    (IX+d),n    Load location (IX+d) with n.
LD    (IX+d),r    Load location (IX+d) with register r.
LD    IY,nn       Load IY with value nn.
LD    IY,(nn)     Load IY with location (nn).
LD    (IY+d),n    Load location (IY+d) with value n.
LD    (IY+d),r    Load location (IY+d) with register r.
LD    (nn),A      Load location (nn) with accumulator.
LD    (nn),dd     Load location (nn) with register pair dd.
LD    (nn),HL     Load location (nn) with HL.
LD    (nn),IX     Load location (nn) with IX.
LD    (nn),IY     Load location (nn) with IY.
LD    R,A         Load R with accumulator.
LD    r,(HL)      Load register r with location (HL).
LD    r,(IX+d)    Load register r with location (IX+d).
LD    r,(IY+d)    Load register r with location (IY+d).
LD    r,n         Load register r with value n.
LD    r,r'        Load register r with register r'.
LD    SP,HL       Load SP with HL.
LD    SP,IX       Load SP with IX.
LD    SP,IY       Load SP with IY.
LDD               Load location (DE) with location (HL), decrement DE,HL,BC.
LDDR              Perform an LDD and repeat until BC=0.
LDI               Load location (DE) with location (HL), incr DE,HL; decr BC.
LDIR              Perform an LDI and repeat until BC=0.
NEG               Negate accumulator (2's complement).
NOP               No operation.
OR    s           Logical OR of operand s and accumulator.
OTDR              Perform an OUTD and repeat until B=0.
OTIR              Perform an OTI and repeat until B=0.
OUT   (C),r       Load output port (C) with register r.
OUT   (n),A       Load output port (n) with accumulator.
OUTD              Load output port (C) with (HL), decrement HL and B.
OUTI              Load output port (C) with (HL), incr HL, decr B.
POP   IX          Load IX with top of stack.
POP   IY          Load IY with top of stack.
POP   qq          Load register pair qq with top of stack.
PUSH  IX          Load IX onto stack.
PUSH  IY          Load IY onto stack.
PUSH  qq          Load register pair qq onto stack.
RES   b,m         Reset bit b of operand m.
RET               Return from subroutine.
RET   cc          Return from subroutine if condition cc is true.
RETI              Return from interrupt.
RETN              Return from non-maskable interrupt.
RL    m           Rotate left through operand m.
RLA               Rotate left accumulator through carry.
RLC   (HL)        Rotate location (HL) left circular.
RLC   (IX+d)      Rotate location (IX+d) left circular.
RLC   (IY+d)      Rotate location (IY+d) left circular.
RLC   r           Rotate register r left circular.
RLCA              Rotate left circular accumulator.
RLD               Rotate digit left and right between accumulator and (HL).
RR    m           Rotate right through carry operand m.
RRA               Rotate right accumulator through carry.
RRC   m           Rotate operand m right circular.
RRCA              Rotate right circular accumulator.
RRD               Rotate digit right and left between accumulator and (HL).
RST   p           Restart to location p.
SBC   A,s         Subtract operand s from accumulator with carry.
SBC   HL,ss       Subtract register pair ss from HL with carry.
SCF               Set carry flag (C=1).
SET   b,(HL)      Set bit b of location (HL).
SET   b,(IX+d)    Set bit b of location (IX+d).
SET   b,(IY+d)    Set bit b of location (IY+d).
SET   b,R         Set bit b of register r.
SLA   m           Shift operand m left arithmetic.
SRA   m           Shift operand m right arithmetic.
SRL   m           Shift operand m right logical.
SUB   s           Subtract operand s from accumulator.
XOR   s           Exclusive OR operand s and accumulator.
