Go to the first, previous, next, last section, table of contents.

# M680x0 Dependent Features

- M68K-Opts: M680x0 Options
- M68K-Syntax: Syntax
- M68K-Moto-Syntax: Motorola Syntax
- M68K-Float: Floating Point
- M68K-Directives: 680x0 Machine Directives
- M68K-opcodes: Opcodes

## M680x0 Options

The Motorola 680x0 version of `as` has a few machine dependent options.

You can use the ``-l'` option to shorten the size of references to undefined symbols. If you do not use the ``-l'` option, references to undefined symbols are wide enough for a full `long` (32 bits). (Since `as` cannot know where these symbols end up, `as` can only allocate space for the linker to fill in later. Since `as` does not know how far away these symbols are, it allocates as much space as it can.) If you use this option, the references are only one word wide (16 bits). This may be useful if you want the object file to be as small as possible, and you know that the relevant symbols are always less than 17 bits away.

For some configurations, especially those where the compiler normally does not prepend an underscore to the names of user variables, the assembler requires a ``%'` before any use of a register name. This is intended to let the assembler distinguish between C variables and functions named ``a0'` through ``a7'`, and so on. The ``%'` is always accepted, but is not required for certain configurations, notably ``sun3'`. The ``--register-prefix-optional'` option may be used to permit omitting the ``%'` even for configurations for which it is normally required. If this is done, it will generally be impossible to refer to C variables and functions with the same names as register names.

Normally the character ``|'` is treated as a comment character, which means that it can not be used in expressions. The ``--bitwise-or'` option turns ``|'` into a normal character. In this mode, you must either use C style comments, or start comments with a ``#'` character at the beginning of a line.

`as` can assemble code for several different members of the Motorola 680x0 family. The default depends upon how `as` was configured when it was built; normally, the default is to assemble code for the 68020 microprocessor. The following options may be used to change the default. These options control which instructions and addressing modes are permitted. The members of the 680x0 family are very similar. For detailed information about the differences, see the Motorola manuals.

``-m68000'`
``-m68008'`
``-m68302'`
  Assemble for the 68000. ``-m68008'` and ``-m68302'` are synonyms for ``-m68000'`, since the chips are the same from the point of view of the assembler.
``-m68010'`
  Assemble for the 68010.
``-m68020'`
  Assemble for the 68020. This is normally the default.
``-m68030'`
  Assemble for the 68030.
``-m68040'`
  Assemble for the 68040.
``-m68060'`
  Assemble for the 68060.
``-mcpu32'`
``-m68331'`
``-m68332'`
``-m68333'`
``-m68340'`
``-m68360'`
  Assemble for the CPU32 family of chips.
``-m68881'`
``-m68882'`
  Assemble 68881 floating point instructions. This is the default for the 68020, 68030, and the CPU32. The 68040 and 68060 always support floating point instructions.
``-mno-68881'`
  Do not assemble 68881 floating point instructions. This is the default for 68000 and the 68010. The 68040 and 68060 always support floating point instructions, even if this option is used.
``-m68851'`
  Assemble 68851 MMU instructions. This is the default for the 68020, 68030, and 68060. The 68040 accepts a somewhat different set of MMU instructions; ``-m68851'` and ``-m68040'` should not be used together.
``-mno-68851'`
  Do not assemble 68851 MMU instructions. This is the default for the 68000, 68010, and the CPU32. The 68040 accepts a somewhat different set of MMU instructions.

## Syntax

This syntax for the Motorola 680x0 was developed at MIT.

The 680x0 version of `as` uses instructions names and syntax compatible with the Sun assembler. Intervening periods are ignored; for example, ``movl'` is equivalent to ``mov.l'`.

In the following table apc stands for any of the address registers (``%a0'` through ``%a7'`), the program counter (``%pc'`), the zero-address relative to the program counter (``%zpc'`), a suppressed address register (``%za0'` through ``%za7'`), or it may be omitted entirely. The use of size means one of ``w'` or ``l'`, and it may be omitted, along with the leading colon, unless a scale is also specified. The use of scale means one of ``1'`, ``2'`, ``4'`, or ``8'`, and it may always be omitted along with the leading colon.

The following addressing modes are understood:

Immediate
  ``#number'`
Data Register
  ``%d0'` through ``%d7'`
Address Register
  ``%a0'` through ``%a7'`
  ``%a7'` is also known as ``%sp'`, i.e. the Stack Pointer. `%a6` is also known as ``%fp'`, the Frame Pointer.
Address Register Indirect
  ``%a0@'` through ``%a7@'`
Address Register Postincrement
  ``%a0@+'` through ``%a7@+'`
Address Register Predecrement
  ``%a0@-'` through ``%a7@-'`
Indirect Plus Offset
  ``apc@(number)'`
Index
  ``apc@(number,register:size:scale)'` The number may be omitted.
Postindex
  ``apc@(number)@(onumber,register:size:scale)'` The onumber or the register, but not both, may be omitted.
Preindex
  ``apc@(number,register:size:scale)@(onumber)'` The number may be omitted. Omitting the register produces the Postindex addressing mode.
Absolute
  ``symbol'`, or ``digits'`, optionally followed by ``:b'`, ``:w'`, or ``:l'`.

## Motorola Syntax

The standard Motorola syntax for this chip differs from the syntax already discussed (see section Syntax). `as` can accept Motorola syntax for operands, even if MIT syntax is used for other operands in the same instruction. The two kinds of syntax are fully compatible.

In the following table apc stands for any of the address registers (``%a0'` through ``%a7'`), the program counter (``%pc'`), the zero-address relative to the program counter (``%zpc'`), or a suppressed address register (``%za0'` through ``%za7'`). The use of size means one of ``w'` or ``l'`, and it may always be omitted along with the leading dot. The use of scale means one of ``1'`, ``2'`, ``4'`, or ``8'`, and it may always be omitted along with the leading asterisk.

The following additional addressing modes are understood:

Address Register Indirect
  ``(%a0)'` through ``(%a7)'`
  ``%a7'` is also known as ``%sp'`, i.e. the Stack Pointer. `%a6` is also known as ``%fp'`, the Frame Pointer.
Address Register Postincrement
  ``(%a0)+'` through ``(%a7)+'`
Address Register Predecrement
  ``-(%a0)'` through ``-(%a7)'`
Indirect Plus Offset
  ``number(%a0)'` through ``number(%a7)'`, or ``number(%pc)'`. The number may also appear within the parentheses, as in ``(number,%a0)'`. When used with the pc, the number may be omitted (with an address register, omitting the number produces Address Register Indirect mode).
Index
  ``number(apc,register.size*scale)'` The number may be omitted, or it may appear within the parentheses. The apc may be omitted. The register and the apc may appear in either order. If both apc and register are address registers, and the size and scale are omitted, then the first register is taken as the base register, and the second as the index register.
Postindex
  ``([number,apc],register.size*scale,onumber)'` The onumber, or the register, or both, may be omitted. Either the number or the apc may be omitted, but not both.
Preindex
  ``([number,apc,register.size*scale],onumber)'` The number, or the apc, or the register, or any two of them, may be omitted. The onumber may be omitted. The register and the apc may appear in either order. If both apc and register are address registers, and the size and scale are omitted, then the first register is taken as the base register, and the second as the index register.

## Floating Point

Packed decimal (P) format floating literals are not supported. Feel free to add the code!

The floating point formats generated by directives are these.

`.float`
  `Single` precision floating point constants.
`.double`
  `Double` precision floating point constants.
`.extend`
`.ldouble`
  `Extended` precision (`long double`) floating point constants.

## 680x0 Machine Directives

In order to be compatible with the Sun assembler the 680x0 assembler understands the following directives.

`.data1`
  This directive is identical to a `.data 1` directive.
`.data2`
  This directive is identical to a `.data 2` directive.
`.even`
  This directive is a special case of the `.align` directive; it aligns the output to an even byte boundary.
`.skip`
  This directive is identical to a `.space` directive.

## Opcodes

- M68K-Branch: Branch Improvement
- M68K-Chars: Special Characters

### Branch Improvement

Certain pseudo opcodes are permitted for branch instructions. They expand to the shortest branch instruction that reach the target. Generally these mnemonics are made by substituting ``j'` for ``b'` at the start of a Motorola mnemonic.

The following table summarizes the pseudo-operations. A `*` flags cases that are more fully described after the table:

              Displacement
              +-------------------------------------------------
              |                68020   68000/10
    Pseudo-Op |BYTE    WORD    LONG    LONG      non-PC relative
              +-------------------------------------------------
         jbsr |bsrs    bsr     bsrl    jsr       jsr
          jra |bras    bra     bral    jmp       jmp
    *     jXX |bXXs    bXX     bXXl    bNXs;jmpl bNXs;jmp
    *    dbXX |dbXX    dbXX        dbXX; bra; jmpl
    *    fjXX |fbXXw   fbXXw   fbXXl             fbNXw;jmp

    XX: condition
    NX: negative of condition XX

`*`---see full description below

`jbsr`
`jra`
  These are the simplest jump pseudo-operations; they always map to one particular machine instruction, depending on the displacement to the branch target.
`jXX`
  Here, ``jXX'` stands for an entire family of pseudo-operations, where XX is a conditional branch or condition-code test. The full list of pseudo-ops in this family is:

       jhi   jls   jcc   jcs   jne   jeq   jvc
       jvs   jpl   jmi   jge   jlt   jgt   jle

  For the cases of non-PC relative displacements and long displacements on the 68000 or 68010, `as` issues a longer code fragment in terms of NX, the opposite condition to XX. For example, for the non-PC relative case:

          jXX foo

  gives

           bNXs oof
           jmp foo
       oof:

`dbXX`
  The full family of pseudo-operations covered here is

       dbhi   dbls   dbcc   dbcs   dbne   dbeq   dbvc
       dbvs   dbpl   dbmi   dbge   dblt   dbgt   dble
       dbf    dbra   dbt

  Other than for word and byte displacements, when the source reads ``dbXX foo'`, `as` emits

           dbXX oo1
           bra oo2
       oo1:jmpl foo
       oo2:

`fjXX`
  This family includes

       fjne   fjeq   fjge   fjlt   fjgt   fjle   fjf
       fjt    fjgl   fjgle  fjnge  fjngl  fjngle fjngt
       fjnle  fjnlt  fjoge  fjogl  fjogt  fjole  fjolt
       fjor   fjseq  fjsf   fjsne  fjst   fjueq  fjuge
       fjugt  fjule  fjult  fjun

  For branch targets that are not PC relative, `as` emits

           fbNX oof
           jmp foo
       oof:

  when it encounters ``fjXX foo'`.

### Special Characters

The immediate character is ``#'` for Sun compatibility. The line-comment character is ``|'` (unless the ``--bitwise-or'` option is used). If a ``#'` appears at the beginning of a line, it is treated as a comment unless it looks like ``# line file'`, in which case it is treated normally.

Go to the first, previous, next, last section, table of contents.