                        --------------------------------------
                                       READ.ME

                              DSP Development Corporation
                                  One Kendall Square
                                 Cambridge, MA 02139
                                         USA

                                Phone:  1-617-577-1133
                                Fax:    1-617-577-8211


                                   July 1, 1993
                        --------------------------------------

                               DADiSP/32 TRiAL KIT    

        1. INTRODUCTION
        ______________________________________________________________________

        Welcome to the DADiSP/32 TRiAL KIT for the IBM 386 and 486
        PCs and compatible computers running DOS 3.0 and higher.  In
        addition to the documentation supplied with the TRiAL KIT, the
        kit includes one High Density floppy disk.  Because DADiSP/32
        runs the system processor in protected mode, the DADiSP program
        can directly address up to 64 MB of extended memory.  To
        operate correctly, DADiSP requires 2 MB of extended memory,
        plus 512 KB of conventional memory, for a total of 2.5 MB of
        system memory.

        2. INSTALLING THE TRiAL
        ______________________________________________________________________

        To install the TRiAL on your hard disk:

                a) Place the floppy disk into the floppy drive.
                b) Go to the floppy drive by typing A: or B:.
                c) Type: INSTALL. 


        3. RUNNING THE TRiAL
        ______________________________________________________________________

        The DADiSP/32 Worksheet TRiAL contains two modes: 1) a self-running 
        demonstration and 2) an interactive session. 

        To run the DADiSP TRiAL in either mode, you must first install the
        TRiAL as described above.

        To run the demonstration, type

                        DEMO

        in the directory where the TRiAL is installed (e.g. C:\DSPTRIAL).

        To start the TRiAL interactive mode, type:

                        DSPTRIAL

        To access the DADiSP Worksheet functions through a pop-up menu, press 
        the / key when you are in a Worksheet.  The TRiAL does not contain 
        all the functions included in the full product nor does it allow data 
        import or export.

        The TRiAL requires VGA graphics.


        4. TROUBLE STARTING THE TRiAL
        ______________________________________________________________________

        If you experience difficulty getting the DADiSP TRiAL to
        run the first time, please contact our technical support
        department or your DADiSP Dealer.  They are always ready
        to assist you.

        If you have problems or questions, please call or fax DSP
        at the above numbers or contact your DADiSP Dealer.

        ______________________________________________________________________

                                  END OF READ.ME 
        ______________________________________________________________________
