
            Using X24WIN31.ZIP for the PowerGraph X-24 Adapter

You must use PKUNZIP version 1.1 or later to decompress this archive. Be
sure and use the "-d" switch to build subdirectories so that there will be
a FILES, WIN30DRV, and WIN31DRV subdirectories when you finish
decompressing this file.

Once you've decompressed the files, we recommend that you create a disk by
formatting a blank 1.2 mb floppy, then use "XCOPY /S *.* A:\" which will
copy all the files from this archive including "/s" subdirectories.  Once
you've done that, you should have a disk in drive A: (or B:) with this
read.me file in the root directory, a FILES subdirectory which contains all
of the .FON, .DRV, and etc. files, a WIN30DRV directory for the Windows 3.0
OEMSETUP and a WIN31DRV for the Windows 3.1 OEMSETUP.  Label the disk
"PowerGraph X-24 Windows 3.0/3.1 Drivers Release 1.2".

Refer to your PowerGraph X-24 adapter card manual for further instructions
on how to use Windows SETUP to install these drivers. You can also use the
Winstall program with this drivers disk (just enter "A:" or "B:" when it
asks you for the Windows 3.1 Drivers Disk and put the newly created disk in
the appropriate drive).  For more information about Winstall, consult your
PowerGraph X-24 manual.

If you have any trouble installing or using these drivers, please contact
STB Tech Support 214-234-8750 or leave us a message on the STB Tech BBS at
214-437-9615, 2400-16.8k baud, v.32/v.32bis and HST compatible, no parity,
8 bits, 1 stop-bit; 24 hours, 3 nodes.

