How to set up the SERVER.CON file for Multi-port Cards



     1)  Any NON-INTELLIGENT Multiple Port Board with contiguous port

         addressing will be compatible with Modem Assist Plus 2.0 or higher.

         If the board includes driver software, the driver should not be

         loaded if you intend to use Modem Assist to control the ports.



     2)  In SERVER.CON file, the only changes that need to be made include:



        a)  Asynchronous Line definition section should have an individual

            port assignment for each port on the board.



        b)  The line definition for each line should have the exact port

            and interrupt reference for that board.  So the interrupt will

            remain the same for each line but the port address in each case

            will increment up by the hex amount specified in the setup of

            the board.



                      ***************************************************

EXAMPLE:              LINE NAME=LINE1        PORT 1

           ------->        PORT=100H         PORT ADDRESS

                           INTERRUPT=5       IRQ LEVEL

                           TRANSMIT=T9600    TRANSMIT SPEED BPS

                           MODEM=Y           MODEM PRESENT

                      ;

