NOTE    THIS IS a DATABASE FOR VERSION 1.40 OF 22DISK BY SYDEX.
note
note  Last update: 3.9.1994
note  ----------------------
note  skip = initial tracks in Single Density
note  order sides even-odd = ???;  order eagle !
note  see = ?? (cross reference)


note BEGIN HD1  Hd-TestFormat 3.5"
note DENSITY MFM,HIGH CYLINDERS 80 SIDES 2 SECTORS 18,512
note SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18
note SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18
note ORDER SIDES
note BSH 5 BLM 31 EXM 3 DSM 176 DRM 127 AL0 080H AL1 0 OFS 0
note END



note untested:
BEGIN MAG2 MAGIC DOS from longshot (Serge Querne) 2x410Ko DSDD side 2
note As I haven't a side swith on my 3,5", I can't be sure that side 2 works
note OFS should be changed perhaps to 83 ?
DENSITY MFM,LOW CYLINDERS 82 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 193,194,195,196,197,198,199,200,201,202
SIDE2 0 1,2,3,4,5,6,7,8,9,10
ORDER CYLINDERS
BSH 004h BLM 00fh EXM 001h DSM 0cch DRM 03fh AL0 080h AL1 000h OFS 000h
END

note untested:
BEGIN MAG1 MAGIC DOS from longshot (Serge Querne) 2x410Ko DSDD side 1
DENSITY MFM,LOW CYLINDERS 82 SIDES 1 SECTORS 10,512 SKEW 2
SIDE1 0 193,194,195,196,197,198,199,200,201,202
ORDER CYLINDERS
BSH 004h BLM 00fh EXM 001h DSM 0cch DRM 03fh AL0 080h AL1 000h OFS 000h
END


BEGIN KCS1  KC Compact 169K System Format
DENSITY MFM,LOW CYLINDERS 80 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 041h, 042h, 043h, 044h, 045h, 046h, 047h, 048h, 049h
BSH 3 BLM 7 EXM 0 DSM 170 DRM 63 AL0 0C0H AL1 0 OFS 0
END

BEGIN KCD1  KC Compact 178K Data Format
DENSITY MFM,LOW CYLINDERS 80 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 0c1h, 0c2h, 0c3h, 0c4h, 0c5h, 0c6h, 0c7h, 0c8h, 0c9h
BSH 3 BLM 7 EXM 0 DSM 179 DRM 63 AL0 0C0H AL1 0 OFS 0
END

BEGIN P2  Amstrad PCW8256 - DSDD 48 tpi - 9x512x40x2
DENSITY MFM,LOW CYLINDERS 40 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES LABEL AMS1
BSH 4  BLM 15  EXM 0  DSM 356  DRM 255  AL0 0F0H  AL1 0  OFS 1
END

BEGIN P1  Amstrad PCW8256 - DSDD 96tpi - 9x512x80x2
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES LABEL AMS1
BSH 4  BLM 15  EXM 0  DSM 356  DRM 255  AL0 0F0H  AL1 0  OFS 1
END

BEGIN AP2  Amstrad CPC DiskPara 3-Format DSDD 96tpi 10x512x80x2
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 399  DRM 127  AL0 0C0H  AL1 0  OFS 0
END

BEGIN AP1  Amstrad CPC 830K-DiskPara-Format - DDSS 10x512x83x2
DENSITY MFM,LOW CYLINDERS 83 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 0 11,12,13,14,15,16,17,18,19,20
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 414  DRM 191  AL0 224  AL1 0  OFS 0
END

BEGIN V1  Vortex - DSDD 96 tpi 5.25 - 9x512x80x2
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512
SIDE1 0 001h, 002h, 003h, 004h, 005h, 006h, 007h, 008h, 009h
SIDE2 1 001h, 002h, 003h, 004h, 005h, 006h, 007h, 008h, 009h
ORDER SIDES
BSH 5 BLM 31 EXM 3 DSM 176 DRM 127 AL0 080H AL1 0 OFS 2
END


BEGIN AMSD2  Amstrad CPC System DSDD 96tpi 5.25" - DOBBERTIN -
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SKEW 2
SIDE1 0 65,66,67,68,69,70,71,72,73
SIDE2 1 65,66,67,68,69,70,71,72,73
ORDER SIDES
BSH 5 BLM 31 EXM 3 DSM 176 DRM 127 AL0 080H AL1 0 OFS 2
END

BEGIN AMSD1  Amstrad DOBBERTIN DATA DSDD 96 tpi 5.25" Skew 5
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SKEW 2
SIDE1 0 193,194,195,196,197,198,199,200,201
SIDE2 1 193,194,195,196,197,198,199,200,201
BSH 5 BLM 31 EXM 3 DSM 179 DRM 127 AL0 080H AL1 0 OFS 0
END


BEGIN AII2  Amstrad CPC 154K IBM CP/M-86 SSDD Side 2 (3.5")
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 8,512
SIDE1 0 001h, 002h, 003h, 004h, 005h, 006h, 007h, 008h
SIDE2 0 001h, 002h, 003h, 004h, 005h, 006h, 007h, 008h
ORDER EAGLE
BSH 3 BLM 7 EXM 0 DSM 155 DRM 63 AL0 0C0H AL1 0 OFS 81
END

BEGIN AII1  Amstrad CPC 154K IBM CP/M-86 SSDD Side 1 (3.5")
DENSITY MFM,LOW CYLINDERS 80 SIDES 1 SECTORS 8,512
SIDE1 0 001h, 002h, 003h, 004h, 005h, 006h, 007h, 008h
BSH 3 BLM 7 EXM 0 DSM 155 DRM 63 AL0 0C0H AL1 0 OFS 1
END

BEGIN AI2  Amstrad CPC 154K IBM CP/M-86 SSDD Side 2 (5.25")
DENSITY MFM,LOW CYLINDERS 40 SIDES 2 SECTORS 8,512
SIDE1 0 001h, 002h, 003h, 004h, 005h, 006h, 007h, 008h
SIDE2 0 001h, 002h, 003h, 004h, 005h, 006h, 007h, 008h
ORDER EAGLE
BSH 3 BLM 7 EXM 0 DSM 155 DRM 63 AL0 0C0H AL1 0 OFS 41
END

BEGIN AI1  Amstrad CPC 154K IBM CP/M-86 SSDD Side 1 (5.25")
DENSITY MFM,LOW CYLINDERS 40 SIDES 1 SECTORS 8,512
SIDE1 0 001h, 002h, 003h, 004h, 005h, 006h, 007h, 008h
BSH 3 BLM 7 EXM 0 DSM 155 DRM 63 AL0 0C0H AL1 0 OFS 1
END

BEGIN ASS2  Amstrad CPC 169K System Side 2 (3.5")
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 041h, 042h, 043h, 044h, 045h, 046h, 047h, 048h, 049h
SIDE2 0 041h, 042h, 043h, 044h, 045h, 046h, 047h, 048h, 049h
ORDER EAGLE
BSH 3 BLM 7 EXM 0 DSM 170 DRM 63 AL0 0C0H AL1 0 OFS 82
END

BEGIN ASS1  Amstrad CPC 169K System Side 1 (3.5")
DENSITY MFM,LOW CYLINDERS 80 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 041h, 042h, 043h, 044h, 045h, 046h, 047h, 048h, 049h
BSH 3 BLM 7 EXM 0 DSM 170 DRM 63 AL0 0C0H AL1 0 OFS 2
END

BEGIN AS2  Amstrad CPC 169K System Side 2 (5.25")
DENSITY MFM,LOW CYLINDERS 40 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 041h, 042h, 043h, 044h, 045h, 046h, 047h, 048h, 049h
SIDE2 0 041h, 042h, 043h, 044h, 045h, 046h, 047h, 048h, 049h
ORDER EAGLE
BSH 3 BLM 7 EXM 0 DSM 170 DRM 63 AL0 0C0H AL1 0 OFS 42
END

BEGIN AS1  Amstrad CPC 169K System Side 1 (5.25")
DENSITY MFM,LOW CYLINDERS 40 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 041h, 042h, 043h, 044h, 045h, 046h, 047h, 048h, 049h
BSH 3 BLM 7 EXM 0 DSM 170 DRM 63 AL0 0C0H AL1 0 OFS 2
END

BEGIN ADD2  Amstrad CPC 178K Data Side 2 (3.5")
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 0c1h, 0c2h, 0c3h, 0c4h, 0c5h, 0c6h, 0c7h, 0c8h, 0c9h
SIDE2 0 0c1h, 0c2h, 0c3h, 0c4h, 0c5h, 0c6h, 0c7h, 0c8h, 0c9h
ORDER EAGLE
BSH 3 BLM 7 EXM 0 DSM 179 DRM 63 AL0 0C0H AL1 0 OFS 80
END

BEGIN ADD1  Amstrad CPC 178K Data Side 1 (3.5")
DENSITY MFM,LOW CYLINDERS 80 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 0c1h, 0c2h, 0c3h, 0c4h, 0c5h, 0c6h, 0c7h, 0c8h, 0c9h
BSH 3 BLM 7 EXM 0 DSM 179 DRM 63 AL0 0c0H AL1 0 OFS 0
END

BEGIN AD2  Amstrad CPC 178K Data Side 2 (5.25")
DENSITY MFM,LOW CYLINDERS 40 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 0c1h, 0c2h, 0c3h, 0c4h, 0c5h, 0c6h, 0c7h, 0c8h, 0c9h
SIDE2 0 0c1h, 0c2h, 0c3h, 0c4h, 0c5h, 0c6h, 0c7h, 0c8h, 0c9h
ORDER EAGLE
BSH 3 BLM 7 EXM 0 DSM 179 DRM 63 AL0 0C0H AL1 0 OFS 40
END

BEGIN AD1  Amstrad CPC 178K Data Side 1 (5.25")
DENSITY MFM,LOW CYLINDERS 40 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 0c1h, 0c2h, 0c3h, 0c4h, 0c5h, 0c6h, 0c7h, 0c8h, 0c9h
BSH 3 BLM 7 EXM 0 DSM 179 DRM 63 AL0 0c0H AL1 0 OFS 0
END

NOTE End of cpmdisks.def
