Define Device (
	Manufacturer "Oberheim"
	Device "Matrix-6R"
	Channel 1
	CharSet (
		az2AZ
		Disable (
			#! ## #% #& #( #) #: #; #? #@ #[ #] #^ #` #{-#~
		)
		Remap (
			#< to #(
			#> to #)
		)
	)
	Checksum NybbleLM Sum
	Updates Final
)

Define Font "Numbers" (
	Name "Helvetica.font"
	Size 9
)

Define Font "Topaz2" (
	Name "Topaz2.font"
	Size 8
)

Define Font "Topaz2p" (
	Name "Topaz2p.font"
	Size 8
)


Define Window "Page Select" (
	Position 0 14
	Size 640 24
)

Define Window "DCOs" (
	Position 0 41
	Size 640 359
)
Define Window "VCF-VCA" (
	Position 0 41
	Size 640 359
)
Define Window "Ramps-Port-Track-FM" (
	Position 0 41
	Size 640 359
)
Define Window "Envelopes" (
	Position 0 41
	Size 640 359
)
Define Window "LFOs" (
	Position 0 41
	Size 640 359
)
Define Window "MatrixModulations" (
	Position 0 41
	Size 640 359
)

Define Link "Pages" (
	Type Windows (
		Data (
			"DCOs"
			"VCF-VCA"
			"Ramps-Port-Track-FM"
			"Envelopes"
			"LFOs"
			"MatrixModulations"
		)
	)
)


'Define Midi "Quick Edit"  (
'	Data (
'		F0H
'		10H 'Oberheim ID
'		06H 'Matrix 6 / 6R
'		05H 'Opcode: Select Quick Patch Edit Mode
'		F7H
'	)
'       Send
')

Define Midi "Parameter" (
	Data (
		F0H
		10H 'Oberheim ID
		06H 'Matrix 6 / 6R
		06H 'Opcode: Change Parameter
		Byte 'Parameter #
		Byte 'Value
		F7H
	)
)

Define Midi "Patch" (
	Loadable
	DataFile "Temporary:MSE/definitions/Oberheim/Matrix-6R_Patch.midi"
	Midi (
		Data (
			273 CHECKSUM 5 271
		)
	)
)


Window "Page Select" (
	Border (
		Position 0 0
		Size 640 24
		Fill 3
	)

	Text "OBERHEIM - Matrix 6R" (
		Position 473 14
		Color 2
		Shadow
	)

	Gadget "Page" (
		Position 8 5
		Type Cycle (
			Data (
				"DCO 1 / 2"
				"VCF / VCA"
				"Ramps / Portamento / Tracking / FM"
				"Envelope 1 / 2 / 3"
				"LFO 1 / 2"
				"Matrix Modulations"
			)
			Link "Pages"
		)
	)

	Gadget "PatchName" (
		Position 355 5
		Font "Topaz2"
		Type String (
			MaxChars 8
		)
		Midi "Patch" (
			Data (
				5 VALUE NybbleLM
			)
			Send
		)
	)
)


Window "DCOs" (
	Border (
		Position 0 0
		Size 640 147
		Frame 3D-Recess
	)
	Border (
		Position 0 145
		Size 640 17
		Fill 3
		Frame 3D-Recess
	)
	Text "DCO 1" (
		Position 301 156
	)


	Text "Frequency" (
		Position 49 17
	)
	Gadget "DCO1_Frequency" (
		Position 33 33
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 0 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				23 VALUE NybbleLM
			)
		)
	)

	Text "Frequency" (
		Position 49 58
	)
	Text "Modulation by LFO1" (
		Position 17 68
	)
	Gadget "DCO1_FreqModLFO1" (
		Position 33 84
		Font "Numbers"
		Type Slider (
			Range -63 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Patch" (
			Data (
				177 VALUE Signed NybbleLM
			)
			Send
		)
	)

	Text "Pulse Width" (
		Position 211 17
	)
	Gadget "DCO1_PulseWidth" (
		Position 199 33
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 3 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				27 VALUE NybbleLM
			)
		)
	)

	Text "Pulse Width" (
		Position 211 58
	)
	Text "Modulation by LFO2" (
		Position 181 68
	)
	Gadget "DCO1_PulseModLFO2" (
		Position 199 84
		Font "Numbers"
		Type Slider (
			Range -63 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Patch" (
			Data (
				179 VALUE Signed NybbleLM
			)
			Send
		)
	)

	Text "Sync DCO2" (
		Position 148 116
	)
	Gadget "DCO1_SyncDCO2" (
		Position 143 120
		Type Cycle (
			Data (
				"OFF"
				"Soft"
				"Medium"
				"Hard"
			)
		)
		Midi "Parameter" (
			Data (
				4 2 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				55 VALUE NybbleLM
			)
		)
	)

	Text "Wave Shape" (
		Position 363 17
	)
	Gadget "DCO1_WaveShape" (
		Position 352 33
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 5 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				25 VALUE NybbleLM
			)
		)
	)

	Text "Wave Select" (
		Position 360 68
	)
	Gadget "DCO1_WaveSelect" (
		Position 337 72
		Type Cycle (
			Data (
				"OFF"
				"Pulse"
				"Wave"
				"Pulse + Wave"
			)
		)
		Midi "Parameter" (
			Data (
				4 6 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				31 VALUE NybbleLM
			)
		)
	)

	Text "Levers" (
		Position 397 116
	)
	Gadget "DCO1_Levers" (
		Position 339 120
		Type Cycle (
			Data (
				"OFF"
				"Bender"
				"Vibrato"
				"Bender + Vibrato"
			)
		)
		Midi "Parameter" (
			Data (
				4 7 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				29 VALUE NybbleLM
			)
		)
	)

	Text "Tracking" (
		Position 517 17
	)
	Gadget "DCO1_Tracking" (
		Position 489 21
		Type Cycle (
			Data (
				"Keyboard"
				"Portamento"
			)
		)
		Midi "Parameter" (
			Data (
				4 8 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				47 VALUE NybbleLM
			)
		)
	)

	Text "Click" (
		Position 538 68
	)
	Gadget "DCO1_Click" (
		Position 524 72
		Type Cycle (
			Data (
				"OFF"
				"ON"
			)
		)
		Midi "Parameter" (
			Data (
				4 9 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				49 VALUE NybbleLM
			)
		)
	)

	Border (
		Position 0 169
		Size 640 147
		Frame 3D-Recess
	)
	Border (
		Position 0 314
		Size 640 17
		Fill 3
		Frame 3D-Recess
	)
	Text "DCO 2" (
		Position 301 325
	)


	Text "Frequency" (
		Position 49 186
	)
	Gadget "DCO2_Frequency" (
		Position 33 202
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 10 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				33 VALUE NybbleLM
			)
		)
	)

	Text "Frequency" (
		Position 49 227
	)
	Text "Modulation by LFO1" (
		Position 17 237
	)
	Gadget "DCO2_FreqModLFO1" (
		Position 33 253
		Font "Numbers"
		Type Slider (
			Range -63 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Patch" (
			Data (
				181 VALUE Signed NybbleLM
			)
			Send
		)
	)

	Text "Pulse Width" (
		Position 211 186
	)
	Gadget "DCO2_PulseWidth" (
		Position 199 202
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 13 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				37 VALUE NybbleLM
			)
		)
	)

	Text "Pulse Width" (
		Position 211 227
	)
	Text "Modulation by LFO2" (
		Position 181 237
	)
	Gadget "DCO2_PulseModLFO2" (
		Position 199 253
		Font "Numbers"
		Type Slider (
			Range -63 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Patch" (
			Data (
				183 VALUE Signed NybbleLM
			)
			Send
		)
	)

	Text "Detune DCO1" (
		Position 207 285
	)
	Gadget "DCO2_DetuneDCO1" (
		Position 199 301
		Font "Numbers"
		Type Slider (
			Range -31 31
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Patch" (
			Data (
				43 VALUE Signed NybbleLM
			)
			Send
		)
	)

	Text "Wave Shape" (
		Position 363 186
	)
	Gadget "DCO2_WaveShape" (
		Position 352 202
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 15 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				35 VALUE NybbleLM
			)
		)
	)

	Text "Wave Select" (
		Position 360 237
	)
	Gadget "DCO2_WaveSelect" (
		Position 337 241
		Type Cycle (
			Data (
				"OFF"
				"Pulse"
				"Wave"
				"Pulse + Wave"
				"Noise"
			)
		)
		Midi "Parameter" (
			Data (
				4 16 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				41 VALUE NybbleLM
			)
		)
	)

	Text "Levers" (
		Position 397 285
	)
	Gadget "DCO2_Levers" (
		Position 339 289
		Type Cycle (
			Data (
				"OFF"
				"Bender"
				"Vibrato"
				"Bender + Vibrato"
			)
		)
		Midi "Parameter" (
			Data (
				4 17 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				39 VALUE NybbleLM
			)
		)
	)

	Text "Tracking" (
		Position 517 186
	)
	Gadget "DCO2_Tracking" (
		Position 489 190
		Type Cycle (
			Data (
				"OFF"
				"Keyboard"
				"Portamento"
			)
			DataValues (
				%00 %10 %01
			)
		)
		Midi "Parameter" (
			Data (
				4 18 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				51 VALUE NybbleLM
			)
		)
	)

	Text "Click" (
		Position 538 237
	)
	Gadget "DCO2_Click" (
		Position 524 241
		Type Cycle (
			Data (
				"OFF"
				"ON"
			)
		)
		Midi "Parameter" (
			Data (
				4 19 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				53 VALUE NybbleLM
			)
		)
	)
)

Window "VCF-VCA" (
	Border (
		Position 51 0
		Size 524 147
		Frame 3D-Recess
	)
	Border (
		Position 51 145
		Size 524 17
		Fill 3
		Frame 3D-Recess
	)
	Text "VCF" (
		Position 309 156
	)


	Text "Frequency" (
		Position 100 17
	)
	Gadget "VCF_Frequency" (
		Position 84 33
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 21 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				57 VALUE NybbleLM
			)
		)
	)

	Text "Frequency" (
		Position 100 58
	)
	Text "Modulation by ENV1" (
		Position 67 68
	)
	Gadget "VCF_FreqModENV1" (
		Position 84 84
		Font "Numbers"
		Type Slider (
			Range -63 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Patch" (
			Data (
				185 VALUE Signed NybbleLM
			)
			Send
		)
	)

	Text "Resonance" (
		Position 274 17
	)
	Gadget "VCF_Resonance" (
		Position 258 33
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 24 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				59 VALUE NybbleLM
			)
		)
	)

	Text "Frequency" (
		Position 274 58
	)
	Text "Modulation by Pressure" (
		Position 224 68
	)
	Gadget "VCF_FreqModPress" (
		Position 258 84
		Font "Numbers"
		Type Slider (
			Range -63 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Patch" (
			Data (
				187 VALUE Signed NybbleLM
			)
			Send
		)
	)

	Text "DCO Mix" (
		Position 187 116
	)
	Text "DCO1" (
		Position 126 128
	)
	Text "DCO2" (
		Position 268 128
	)
	Gadget "VCF_DCOMix" (
		Position 162 132
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 20 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				45 VALUE NybbleLM
			)
		)
	)

	Text "Levers" (
		Position 463 89
	)
	Gadget "VCF_Levers" (
		Position 405 93
		Type Cycle (
			Data (
				"OFF"
				"Bender"
				"Vibrato"
				"Bender + Vibrato"
			)
		)
		Midi "Parameter" (
			Data (
				4 25 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				61 VALUE NybbleLM
			)
		)
	)

	Text "Tracking" (
		Position 458 42
	)
	Gadget "VCF_Tracking" (
		Position 430 47
		Type Cycle (
			Data (
				"OFF"
				"Keyboard"
				"Portamento"
			)
			DataValues (
				%00 %10 %01
			)
		)
		Midi "Parameter" (
			Data (
				4 26 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				63 VALUE NybbleLM
			)
		)
	)

	Border (
		Position 119 172
		Size 381 104
		Frame 3D-Recess
	)
	Border (
		Position 119 274
		Size 381 17
		Fill 3
		Frame 3D-Recess
	)
	Text "VCA" (
		Position 309 285
	)


	Text "VCA1 Volume" (
		Position 180 190
	)
	Gadget "VCA1_Volume" (
		Position 170 206
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 27 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				67 VALUE NybbleLM
			)
		)
	)

	Text "VCA1" (
		Position 205 230
	)
	Text "Modulation by Velocity" (
		Position 141 240
	)
	Gadget "VCA_VCA1ModVel" (
		Position 170 256
		Font "Numbers"
		Type Slider (
			Range -63 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Patch" (
			Data (
				189 VALUE Signed NybbleLM
			)
			Send
		)
	)

	Text "VCA2" (
		Position 392 230
	)
	Text "Modulation by ENV2" (
		Position 338 240
	)
	Gadget "VCA_VCA2ModENV2" (
		Position 356 256
		Font "Numbers"
		Type Slider (
			Range -63 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Patch" (
			Data (
				191 VALUE Signed NybbleLM
			)
			Send
		)
	)
)

Window "Ramps-Port-Track-FM" (
	Border (
		Position 0 0
		Size 219 88
		Frame 3D-Recess
	)
	Border (
		Position 0 86
		Size 219 17
		Fill 3
		Frame 3D-Recess
	)
	Text "Ramp 1 Generator" (
		Position 54 97
	)

	Text "Rate" (
		Position 94 17
	)
	Gadget "Ramp1_Rate" (
		Position 58 33
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 40 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				169 VALUE NybbleLM
			)
		)
	)

	Text "Trigger" (
		Position 84 56
	)
	Gadget "Ramp1_Trigger" (
		Position 9 60
		Type Cycle (
			Data (
				"Single"
				"Multiple"
				"External Single"
				"External Single Gated"
			)
		)
		Midi "Parameter" (
			Data (
				4 41 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				171 VALUE NybbleLM
			)
		)
	)

	Border (
		Position 0 112
		Size 219 88
		Frame 3D-Recess
	)
	Border (
		Position 0 198
		Size 219 17
		Fill 3
		Frame 3D-Recess
	)
	Text "Ramp 2 Generator" (
		Position 54 209
	)

	Text "Rate" (
		Position 94 130
	)
	Gadget "Ramp2_Rate" (
		Position 58 146
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 42 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				173 VALUE NybbleLM
			)
		)
	)

	Text "Trigger" (
		Position 84 168
	)
	Gadget "Ramp2_Trigger" (
		Position 9 172
		Type Cycle (
			Data (
				"Single"
				"Multiple"
				"External Single"
				"External Single Gated"
			)
		)
		Midi "Parameter" (
			Data (
				4 43 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				175 VALUE NybbleLM
			)
		)
	)

	Border (
		Position 228 0
		Size 205 211
		Frame 3D-Recess
	)
	Border (
		Position 228 209
		Size 205 17
		Fill 3
		Frame 3D-Recess
	)
	Text "Portamento" (
		Position 292 220
	)

	Text "Portamento Rate" (
		Position 272 17
	)
	Gadget "PortamentoRate" (
		Position 280 33
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 44 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				69 VALUE NybbleLM
			)
		)
	)

	Text "Portamento" (
		Position 292 59
	)
	Text "Modulation by Velocity" (
		Position 250 69
	)
	Gadget "Port_ModVelocity" (
		Position 280 85
		Font "Numbers"
		Type Slider (
			Range -63 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Patch" (
			Data (
				203 VALUE Signed NybbleLM
			)
			Send
		)
	)

	Text "Portamento Mode" (
		Position 273 109
	)
	Gadget "Port_Mode" (
		Position 262 113
		Type Cycle (
			Data (
				"Constant Rate"
				"Constant Time"
				"Exponential"
			)
		)
		Midi "Parameter" (
			Data (
				4 46 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				71 VALUE NybbleLM
			)
		)
	)

	Text "Keyboard Mode" (
		Position 281 146
	)
	Gadget "Port_KeyboardMode" (
		Position 266 150
		Type Cycle (
			Data (
				"Reassign"
				"Rotate"
				"Unison"
				"Reassign Rob"
			)
		)
		Midi "Parameter" (
			Data (
				4 48 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				21 VALUE NybbleLM
			)
		)
	)

	Text "Legato Portamento" (
		Position 265 182
	)
	Gadget "Port_Legato" (
		Position 301 186
		Type Cycle (
			Data (
				"OFF"
				"ON"
			)
		)
		Midi "Parameter" (
			Data (
				4 47 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				73 VALUE NybbleLM
			)
		)
	)

	Border (
		Position 444 0
		Size 196 146
		Frame 3D-Recess
	)
	Border (
		Position 444 144
		Size 196 17
		Fill 3
		Frame 3D-Recess
	)
	Text "Tracking Generator" (
		Position 473 155
	)

	Text "Track Input" (
		Position 501 17
	)
	Gadget "TrackInput" (
		Position 453 21
		Type Cycle (
			Data (
				"Envelope 1"
				"Envelope 2"
				"Envelope 3"
				"LFO 1"
				"LFO 2"
				"Vibrato"
				"Ramp 1"
				"Ramp 2"
				"Keyboard"
				"Portamento"
				"Tracking Generator"
				"Keyboard Gate"
				"Velocity"
				"Release Velocity"
				"Pressure"
				"Pedal 1"
				"Pedal 2"
				"Lever 1"
				"Lever 2"
				"Lever 3"
			)
		)
		Midi "Parameter" (
			Data (
				4 33 Byte
				5 VALUE Offset 1 Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				157 VALUE Offset 1 NybbleLM
			)
		)
	)

	Text "Track Points" (
		Position 498 50
	)
	Text "1" (
		Position 480 63
	)
	Gadget "Track_Point1" (
		Position 493 54
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace RIGHT
		)
		Midi "Parameter" (
			Data (
				4 34 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				159 VALUE NybbleLM
			)
		)
	)
	Text "2" (
		Position 479 80
	)
	Gadget "Track_Point2" (
		Position 493 71
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace RIGHT
		)
		Midi "Parameter" (
			Data (
				4 35 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				161 VALUE NybbleLM
			)
		)
	)
	Text "3" (
		Position 479 97
	)
	Gadget "Track_Point3" (
		Position 493 88
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace RIGHT
		)
		Midi "Parameter" (
			Data (
				4 36 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				163 VALUE NybbleLM
			)
		)
	)
	Text "4" (
		Position 479 114
	)
	Gadget "Track_Point4" (
		Position 493 105
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace RIGHT
		)
		Midi "Parameter" (
			Data (
				4 37 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				165 VALUE NybbleLM
			)
		)
	)
	Text "5" (
		Position 479 131
	)
	Gadget "Track_Point5" (
		Position 493 122
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace RIGHT
		)
		Midi "Parameter" (
			Data (
				4 38 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				167 VALUE NybbleLM
			)
		)
	)

	Border (
		Position 444 171
		Size 196 154
		Frame 3D-Recess
	)
	Border (
		Position 444 323
		Size 196 17
		Fill 3
		Frame 3D-Recess
	)
	Text "FM" (
		Position 532 334
	)

	Text "VCF FM Amount" (
		Position 490 187
	)
	Gadget "FM_VCFAmount" (
		Position 490 203
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 30 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				65 VALUE NybbleLM
			)
		)
	)

	Text "FM" (
		Position 532 230
	)
	Text "Modulation by ENV3" (
		Position 472 240
	)
	Gadget "FM_ModENV3" (
		Position 490 256
		Font "Numbers"
		Type Slider (
			Range -63 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Patch" (
			Data (
				205 VALUE Signed NybbleLM
			)
			Send
		)
	)

	Text "FM" (
		Position 532 280
	)
	Text "Modulation by Pressure" (
		Position 458 290
	)
	Gadget "FM_ModPressure" (
		Position 490 306
		Font "Numbers"
		Type Slider (
			Range -63 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Patch" (
			Data (
				207 VALUE Signed NybbleLM
			)
			Send
		)
	)
)

Window "Envelopes" (
	Border (
		Position 0 0
		Size 640 117
		Frame 3D-Recess
	)
	Border (
		Position 384 100
		Size 256 17
		Fill 3
		Frame 3D-Recess
	)
	Text "Envelope 1" (
		Position 479 111
	)

	Text "Delay" (
		Position 45 13
	)
	Gadget "ENV1_Delay" (
		Position 13 29
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 50 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				105 VALUE NybbleLM
			)
		)
	)

	Text "Attack" (
		Position 160 13
	)
	Gadget "ENV1_Attack" (
		Position 131 29
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 52 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				109 VALUE NybbleLM
			)
		)
	)

	Text "Decay" (
		Position 282 13
	)
	Gadget "ENV1_Decay" (
		Position 251 29
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 54 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				113 VALUE NybbleLM
			)
		)
	)

	Text "Sustain" (
		Position 38 49
	)
	Gadget "ENV1_Sustain" (
		Position 13 65
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 51 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				107 VALUE NybbleLM
			)
		)
	)

	Text "Release" (
		Position 156 49
	)
	Gadget "ENV1_Release" (
		Position 131 65
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 53 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				111 VALUE NybbleLM
			)
		)
	)


	Text "Amplitude" (
		Position 94 85
	)
	Gadget "ENV1_Amplitude" (
		Position 74 101
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 55 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				115 VALUE NybbleLM
			)
		)
	)

	Text "Amplitude" (
		Position 272 75
	)
	Text "Modulation by Velocity" (
		Position 223 85
	)
	Gadget "ENV1_AmpModVel" (
		Position 252 101
		Font "Numbers"
		Type Slider (
			Range -63 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Patch" (
			Data (
				193 VALUE Signed NybbleLM
			)
			Send
		)
	)

	Text "Envelope Mode" (
		Position 464 15
	)
	Gadget "ENV1_Mode" (
		Position 390 19
		Type Cycle (
			Data (
				"Normal"
				"Delay-Attack-Decay-Release"
				"Freerun"
				"DADR + Freerun"
			)
		)
		Midi "Parameter" (
			Data (
				4 58 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				119 VALUE NybbleLM
			)
		)
	)

	Text "Trigger Mode" (
		Position 472 45
	)
	Gadget "ENV1_TriggerMode" (
		Position 406 49
		Type Cycle (
			Data (
				"Single"
				"Multiple"
				"Single Reset"
				"Multiple Reset"
				"External Single"
				"External Multiple"
				"External Single Reset"
				"External Multiple Reset"
			)
			DataValues (
				%000 %010 %001 %011 %100 %110 %101 %111
			)
		)
		Midi "Parameter" (
			Data (
				4 57 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				103 VALUE NybbleLM
			)
		)
	)

	Text "LFO 1 Trigger" (
		Position 472 73
	)
	Gadget "ENV1_LFO1Trig" (
		Position 431 77
		Type Cycle (
			Data (
				"Normal"
				"LFO 1"
				"Gate LFO 1 Trigger"
			)
			DataValues (
				0 2 3
			)
		)
		Midi "Parameter" (
			Data (
				4 59 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				117 VALUE NybbleLM
			)
		)
	)

	Border (
		Position 0 121
		Size 640 117
		Frame 3D-Recess
	)
	Border (
		Position 384 221
		Size 256 17
		Fill 3
		Frame 3D-Recess
	)
	Text "Envelope 2" (
		Position 479 232
	)

	Text "Delay" (
		Position 45 134
	)
	Gadget "ENV2_Delay" (
		Position 13 150
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 60 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				123 VALUE NybbleLM
			)
		)
	)

	Text "Attack" (
		Position 160 134
	)
	Gadget "ENV2_Attack" (
		Position 131 150
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 62 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				127 VALUE NybbleLM
			)
		)
	)

	Text "Decay" (
		Position 282 134
	)
	Gadget "ENV2_Decay" (
		Position 251 150
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 64 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				131 VALUE NybbleLM
			)
		)
	)

	Text "Sustain" (
		Position 38 170
	)
	Gadget "ENV2_Sustain" (
		Position 13 186
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 61 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				125 VALUE NybbleLM
			)
		)
	)

	Text "Release" (
		Position 156 170
	)
	Gadget "ENV2_Release" (
		Position 131 186
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 63 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				129 VALUE NybbleLM
			)
		)
	)


	Text "Amplitude" (
		Position 94 206
	)
	Gadget "ENV2_Amplitude" (
		Position 74 222
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 65 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				133 VALUE NybbleLM
			)
		)
	)

	Text "Amplitude" (
		Position 272 196
	)
	Text "Modulation by Velocity" (
		Position 223 206
	)
	Gadget "ENV2_AmpModVel" (
		Position 252 222
		Font "Numbers"
		Type Slider (
			Range -63 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Patch" (
			Data (
				195 VALUE Signed NybbleLM
			)
			Send
		)
	)

	Text "Envelope Mode" (
		Position 464 136
	)
	Gadget "ENV2_Mode" (
		Position 390 140
		Type Cycle (
			Data (
				"Normal"
				"Delay-Attack-Decay-Release"
				"Freerun"
				"DADR + Freerun"
			)
		)
		Midi "Parameter" (
			Data (
				4 68 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				137 VALUE NybbleLM
			)
		)
	)

	Text "Trigger Mode" (
		Position 472 165
	)
	Gadget "ENV2_TriggerMode" (
		Position 406 169
		Type Cycle (
			Data (
				"Single"
				"Multiple"
				"Single Reset"
				"Multiple Reset"
				"External Single"
				"External Multiple"
				"External Single Reset"
				"External Multiple Reset"
			)
			DataValues (
				%000 %010 %001 %011 %100 %110 %101 %111
			)
		)
		Midi "Parameter" (
			Data (
				4 67 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				121 VALUE NybbleLM
			)
		)
	)

	Text "LFO 1 Trigger" (
		Position 472 194
	)
	Gadget "ENV2_LFO1Trig" (
		Position 431 198
		Type Cycle (
			Data (
				"Normal"
				"LFO 1"
				"Gate LFO 1 Trigger"
			)
			DataValues (
				0 2 3
			)
		)
		Midi "Parameter" (
			Data (
				4 69 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				135 VALUE NybbleLM
			)
		)
	)


	Border (
		Position 0 242
		Size 640 117
		Frame 3D-Recess
	)
	Border (
		Position 384 342
		Size 256 17
		Fill 3
		Frame 3D-Recess
	)
	Text "Envelope 3" (
		Position 479 353
	)

	Text "Delay" (
		Position 45 255
	)
	Gadget "ENV3_Delay" (
		Position 13 271
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 70 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				141 VALUE NybbleLM
			)
		)
	)

	Text "Attack" (
		Position 160 255
	)
	Gadget "ENV3_Attack" (
		Position 131 271
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 72 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				145 VALUE NybbleLM
			)
		)
	)

	Text "Decay" (
		Position 282 256
	)
	Gadget "ENV3_Decay" (
		Position 251 272
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 74 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				149 VALUE NybbleLM
			)
		)
	)

	Text "Sustain" (
		Position 38 291
	)
	Gadget "ENV3_Sustain" (
		Position 13 307
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 71 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				143 VALUE NybbleLM
			)
		)
	)

	Text "Release" (
		Position 156 291
	)
	Gadget "ENV3_Release" (
		Position 131 307
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 73 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				147 VALUE NybbleLM
			)
		)
	)


	Text "Amplitude" (
		Position 94 327
	)
	Gadget "ENV3_Amplitude" (
		Position 74 343
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 75 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				151 VALUE NybbleLM
			)
		)
	)

	Text "Amplitude" (
		Position 272 317
	)
	Text "Modulation by Velocity" (
		Position 223 327
	)
	Gadget "ENV3_AmpModVel" (
		Position 252 343
		Font "Numbers"
		Type Slider (
			Range -63 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Patch" (
			Data (
				197 VALUE Signed NybbleLM
			)
			Send
		)
	)

	Text "Envelope Mode" (
		Position 464 257
	)
	Gadget "ENV3_Mode" (
		Position 390 261
		Type Cycle (
			Data (
				"Normal"
				"Delay-Attack-Decay-Release"
				"Freerun"
				"DADR + Freerun"
			)
		)
		Midi "Parameter" (
			Data (
				4 78 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				155 VALUE NybbleLM
			)
		)
	)

	Text "Trigger Mode" (
		Position 472 285
	)
	Gadget "ENV3_TriggerMode" (
		Position 406 289
		Type Cycle (
			Data (
				"Single"
				"Multiple"
				"Single Reset"
				"Multiple Reset"
				"External Single"
				"External Multiple"
				"External Single Reset"
				"External Multiple Reset"
			)
			DataValues (
				%000 %010 %001 %011 %100 %110 %101 %111
			)
		)
		Midi "Parameter" (
			Data (
				4 77 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				139 VALUE NybbleLM
			)
		)
	)

	Text "LFO 1 Trigger" (
		Position 472 315
	)
	Gadget "ENV3_LFO1Trig" (
		Position 431 319
		Type Cycle (
			Data (
				"Normal"
				"LFO 1"
				"Gate LFO 1 Trigger"
			)
			DataValues (
				0 2 3
			)
		)
		Midi "Parameter" (
			Data (
				4 79 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				153 VALUE NybbleLM
			)
		)
	)
)

Window "LFOs" (
	Border (
		Position 0 0
		Size 640 146
		Frame 3D-Recess
	)
	Border (
		Position 0 144
		Size 640 17
		Fill 3
		Frame 3D-Recess
	)
	Text "LFO 1" (
		Position 290 155
	)

	Text "Speed" (
		Position 78 15
	)
	Gadget "LFO1_Speed" (
		Position 47 31
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 80 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				75 VALUE NybbleLM
			)
		)
	)

	Text "Amplitude" (
		Position 251 15
	)
	Gadget "LFO1_Amplitude" (
		Position 230 31
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 84 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				87 VALUE NybbleLM
			)
		)
	)

	Text "Speed" (
		Position 78 56
	)
	Text "Modulation by Pressure" (
		Position 14 66
	)
	Gadget "LFO1_SpeedModPress" (
		Position 47 82
		Font "Numbers"
		Type Slider (
			Range -63 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Patch" (
			Data (
				209 VALUE Signed NybbleLM
			)
			Send
		)
	)

	Text "Amplitude" (
		Position 251 56
	)
	Text "Modulation by Ramp1" (
		Position 209 66
	)
	Gadget "LFO1_AmpModRamp1" (
		Position 230 82
		Font "Numbers"
		Type Slider (
			Range -63 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Patch" (
			Data (
				199 VALUE Signed NybbleLM
			)
			Send
		)
	)

	Text "Waveform" (
		Position 68 112
	)
	Gadget "LFO1_Waveform" (
		Position 12 116
		Type Cycle (
			Data (
				"Triangle"
				"Positive Sawtooth"
				"Negative Sawtooth"
				"Square"
				"Random"
				"Noise"
				"Sampled"
			)
		)
		Midi "Parameter" (
			Data (
				4 82 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				81 VALUE NybbleLM
			)
		)
	)

	Text "Lag" (
		Position 412 67
	)
	Gadget "LFO1_Lag" (
		Position 393 71
		Type Cycle (
			Data (
				"OFF"
				"ON"
			)
		)
		Midi "Parameter" (
			Data (
				4 87 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				79 VALUE NybbleLM
			)
		)
	)

	Text "Trigger Mode" (
		Position 488 15
	)
	Gadget "LFO1_TriggerMode" (
		Position 458 19
		Type Cycle (
			Data (
				"OFF"
				"Single"
				"Multiple"
				"External Single"
			)
		)
		Midi "Parameter" (
			Data (
				4 86 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				77 VALUE NybbleLM
			)
		)
	)

	Text "Retrigger Point" (
		Position 485 47
	)
	Gadget "LFO1_RetriggerPoint" (
		Position 490 63
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 83 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				83 VALUE NybbleLM
			)
		)
	)

	Text "Sample" (
		Position 513 111
	)
	Gadget "LFO1_Sample" (
		Position 449 115
		Type Cycle (
			Data (
				"Envelope 1"
				"Envelope 2"
				"Envelope 3"
				"LFO 1"
				"LFO 2"
				"Vibrato"
				"Ramp 1"
				"Ramp 2"
				"Keyboard"
				"Portamento"
				"Tracking Generator"
				"Keyboard Gate"
				"Velocity"
				"Release Velocity"
				"Pressure"
				"Pedal 1"
				"Pedal 2"
				"Lever 1"
				"Lever 2"
				"Lever 3"
			)
		)
		Midi "Parameter" (
			Data (
				4 88 Byte
				5 VALUE Offset 1 Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				85 VALUE Offset 1 NybbleLM
			)
		)
	)

	Border (
		Position 0 173
		Size 640 146
		Frame 3D-Recess
	)
	Border (
		Position 0 317
		Size 640 17
		Fill 3
		Frame 3D-Recess
	)
	Text "LFO 2" (
		Position 290 328
	)

	Text "Speed" (
		Position 78 188
	)
	Gadget "LFO2_Speed" (
		Position 47 204
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 90 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				89 VALUE NybbleLM
			)
		)
	)

	Text "Amplitude" (
		Position 251 188
	)
	Gadget "LFO2_Amplitude" (
		Position 230 204
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 94 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				101 VALUE NybbleLM
			)
		)
	)

	Text "Speed" (
		Position 78 229
	)
	Text "Modulation by Keyboard" (
		Position 13 239
	)
	Gadget "LFO2_SpeedModKey" (
		Position 47 255
		Font "Numbers"
		Type Slider (
			Range -63 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Patch" (
			Data (
				211 VALUE Signed NybbleLM
			)
			Send
		)
	)

	Text "Amplitude" (
		Position 251 229
	)
	Text "Modulation by Ramp2" (
		Position 209 239
	)
	Gadget "LFO2_AmpModRamp1" (
		Position 230 255
		Font "Numbers"
		Type Slider (
			Range -63 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Patch" (
			Data (
				201 VALUE Signed NybbleLM
			)
			Send
		)
	)

	Text "Waveform" (
		Position 68 285
	)
	Gadget "LFO2_Waveform" (
		Position 12 289
		Type Cycle (
			Data (
				"Triangle"
				"Positive Sawtooth"
				"Negative Sawtooth"
				"Square"
				"Random"
				"Noise"
				"Sampled"
			)
		)
		Midi "Parameter" (
			Data (
				4 92 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				95 VALUE NybbleLM
			)
		)
	)

	Text "Lag" (
		Position 412 239
	)
	Gadget "LFO2_Lag" (
		Position 393 243
		Type Cycle (
			Data (
				"OFF"
				"ON"
			)
		)
		Midi "Parameter" (
			Data (
				4 97 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				93 VALUE NybbleLM
			)
		)
	)

	Text "Trigger Mode" (
		Position 488 188
	)
	Gadget "LFO2_TriggerMode" (
		Position 458 192
		Type Cycle (
			Data (
				"OFF"
				"Single"
				"Multiple"
				"External Single"
			)
		)
		Midi "Parameter" (
			Data (
				4 96 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				91 VALUE NybbleLM
			)
		)
	)

	Text "Retrigger Point" (
		Position 485 219
	)
	Gadget "LFO2_RetriggerPoint" (
		Position 490 235
		Font "Numbers"
		Type Slider (
			Range 0 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace ABOVE
		)
		Midi "Parameter" (
			Data (
				4 93 Byte
				5 VALUE Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				97 VALUE NybbleLM
			)
		)
	)

	Text "Sample" (
		Position 513 284
	)
	Gadget "LFO2_Sample" (
		Position 449 288
		Type Cycle (
			Data (
				"Envelope 1"
				"Envelope 2"
				"Envelope 3"
				"LFO 1"
				"LFO 2"
				"Vibrato"
				"Ramp 1"
				"Ramp 2"
				"Keyboard"
				"Portamento"
				"Tracking Generator"
				"Keyboard Gate"
				"Velocity"
				"Release Velocity"
				"Pressure"
				"Pedal 1"
				"Pedal 2"
				"Lever 1"
				"Lever 2"
				"Lever 3"
			)
		)
		Midi "Parameter" (
			Data (
				4 98 Byte
				5 VALUE Offset 1 Byte
			)
			Send
		)
		Midi "Patch" (
			Data (
				99 VALUE Offset 1 NybbleLM
			)
		)
	)
)

Window "MatrixModulations" (
	Border (
		Position 0 0
		Size 210 96
		Frame 3D-Recess
	)
	Border (
		Position 0 79
		Size 24 17
		Fill 3
		Frame 3D-Recess
	)
	Text "0" (
		Position 9 90
	)

	Text "Modulation Source" (
		Position 45 14
	)
	Gadget "Matrix0_Source" (
		Position 18 18
		Type Cycle (
			Data (
				"NONE"
				"Envelope 1"
				"Envelope 2"
				"Envelope 3"
				"LFO 1"
				"LFO 2"
				"Vibrato"
				"Ramp 1"
				"Ramp 2"
				"Keyboard"
				"Portamento"
				"Tracking Generator"
				"Keyboard Gate"
				"Velocity"
				"Release Velocity"
				"Pressure"
				"Pedal 1"
				"Pedal 2"
				"Lever 1"
				"Lever 2"
				"Lever 3"
			)
		)
		Midi "Patch" (
			Data (
				213 VALUE NybbleLM
			)
			Send
		)
	)
	Text "Modulation Destination" (
		Position 28 43
	)
	Gadget "Matrix0_Destination" (
		Position 9 47
		Type Cycle (
			Data (
				"NONE"
				"DCO 1 Frequency"
				"DCO 1 Pulse Width"
				"DCO 1 Waveshape"
				"DCO 2 Frequency"
				"DCO 2 Pulse Width"
				"DCO 2 Waveshape"
				"Mix Level"
				"VCF FM Amount"
				"VCF Frequency"
				"VCF Resonance"
				"VCA 1 Level"
				"VCA 2 Level"
				"Envelope 1 Delay"
				"Envelope 1 Attack"
				"Envelope 1 Decay"
				"Envelope 1 Release"
				"Envelope 1 Amplitude"
				"Envelope 2 Delay"
				"Envelope 2 Attack"
				"Envelope 2 Decay"
				"Envelope 2 Release"
				"Envelope 2 Amplitude"
				"Envelope 3 Delay"
				"Envelope 3 Attack"
				"Envelope 3 Decay"
				"Envelope 3 Release"
				"Envelope 3 Amplitude"
				"LFO 1 Speed"
				"LFO 1 Amplitude"
				"LFO 2 Speed"
				"LFO 2 Amplitude"
				"Portamento Time"
			)
		)
		Midi "Patch" (
			Data (
				217 VALUE NybbleLM
			)
			Send
		)
	)
	Text "Amount" (
		Position 86 73
	)
	Gadget "Matrix0_Amount" (
		Position 55 77
		Font "Numbers"
		Type Slider (
			Range -63 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace RIGHT
		)
		Midi "Patch" (
			Data (
				215 VALUE Signed NybbleLM
			)
			Send
		)
	)

	Border (
		Position 215 0
		Size 210 96
		Frame 3D-Recess
	)
	Border (
		Position 215 79
		Size 24 17
		Fill 3
		Frame 3D-Recess
	)
	Text "1" (
		Position 224 90
	)

	Text "Modulation Source" (
		Position 260 14
	)
	Gadget "Matrix1_Source" (
		Position 233 18
		Type Cycle (
			Data (
				"NONE"
				"Envelope 1"
				"Envelope 2"
				"Envelope 3"
				"LFO 1"
				"LFO 2"
				"Vibrato"
				"Ramp 1"
				"Ramp 2"
				"Keyboard"
				"Portamento"
				"Tracking Generator"
				"Keyboard Gate"
				"Velocity"
				"Release Velocity"
				"Pressure"
				"Pedal 1"
				"Pedal 2"
				"Lever 1"
				"Lever 2"
				"Lever 3"
			)
		)
		Midi "Patch" (
			Data (
				219 VALUE NybbleLM
			)
			Send
		)
	)
	Text "Modulation Destination" (
		Position 243 43
	)
	Gadget "Matrix1_Destination" (
		Position 224 47
		Type Cycle (
			Data (
				"NONE"
				"DCO 1 Frequency"
				"DCO 1 Pulse Width"
				"DCO 1 Waveshape"
				"DCO 2 Frequency"
				"DCO 2 Pulse Width"
				"DCO 2 Waveshape"
				"Mix Level"
				"VCF FM Amount"
				"VCF Frequency"
				"VCF Resonance"
				"VCA 1 Level"
				"VCA 2 Level"
				"Envelope 1 Delay"
				"Envelope 1 Attack"
				"Envelope 1 Decay"
				"Envelope 1 Release"
				"Envelope 1 Amplitude"
				"Envelope 2 Delay"
				"Envelope 2 Attack"
				"Envelope 2 Decay"
				"Envelope 2 Release"
				"Envelope 2 Amplitude"
				"Envelope 3 Delay"
				"Envelope 3 Attack"
				"Envelope 3 Decay"
				"Envelope 3 Release"
				"Envelope 3 Amplitude"
				"LFO 1 Speed"
				"LFO 1 Amplitude"
				"LFO 2 Speed"
				"LFO 2 Amplitude"
				"Portamento Time"
			)
		)
		Midi "Patch" (
			Data (
				223 VALUE NybbleLM
			)
			Send
		)
	)
	Text "Amount" (
		Position 301 73
	)
	Gadget "Matrix1_Amount" (
		Position 270 77
		Font "Numbers"
		Type Slider (
			Range -63 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace RIGHT
		)
		Midi "Patch" (
			Data (
				221 VALUE Signed NybbleLM
			)
			Send
		)
	)

	Border (
		Position 430 0
		Size 210 96
		Frame 3D-Recess
	)
	Border (
		Position 430 79
		Size 24 17
		Fill 3
		Frame 3D-Recess
	)
	Text "2" (
		Position 439 90
	)

	Text "Modulation Source" (
		Position 475 14
	)
	Gadget "Matrix2_Source" (
		Position 448 18
		Type Cycle (
			Data (
				"NONE"
				"Envelope 1"
				"Envelope 2"
				"Envelope 3"
				"LFO 1"
				"LFO 2"
				"Vibrato"
				"Ramp 1"
				"Ramp 2"
				"Keyboard"
				"Portamento"
				"Tracking Generator"
				"Keyboard Gate"
				"Velocity"
				"Release Velocity"
				"Pressure"
				"Pedal 1"
				"Pedal 2"
				"Lever 1"
				"Lever 2"
				"Lever 3"
			)
		)
		Midi "Patch" (
			Data (
				225 VALUE NybbleLM
			)
			Send
		)
	)
	Text "Modulation Destination" (
		Position 458 43
	)
	Gadget "Matrix2_Destination" (
		Position 439 47
		Type Cycle (
			Data (
				"NONE"
				"DCO 1 Frequency"
				"DCO 1 Pulse Width"
				"DCO 1 Waveshape"
				"DCO 2 Frequency"
				"DCO 2 Pulse Width"
				"DCO 2 Waveshape"
				"Mix Level"
				"VCF FM Amount"
				"VCF Frequency"
				"VCF Resonance"
				"VCA 1 Level"
				"VCA 2 Level"
				"Envelope 1 Delay"
				"Envelope 1 Attack"
				"Envelope 1 Decay"
				"Envelope 1 Release"
				"Envelope 1 Amplitude"
				"Envelope 2 Delay"
				"Envelope 2 Attack"
				"Envelope 2 Decay"
				"Envelope 2 Release"
				"Envelope 2 Amplitude"
				"Envelope 3 Delay"
				"Envelope 3 Attack"
				"Envelope 3 Decay"
				"Envelope 3 Release"
				"Envelope 3 Amplitude"
				"LFO 1 Speed"
				"LFO 1 Amplitude"
				"LFO 2 Speed"
				"LFO 2 Amplitude"
				"Portamento Time"
			)
		)
		Midi "Patch" (
			Data (
				229 VALUE NybbleLM
			)
			Send
		)
	)
	Text "Amount" (
		Position 516 73
	)
	Gadget "Matrix2_Amount" (
		Position 485 77
		Font "Numbers"
		Type Slider (
			Range -63 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace RIGHT
		)
		Midi "Patch" (
			Data (
				227 VALUE Signed NybbleLM
			)
			Send
		)
	)

	Border (
		Position 0 101
		Size 210 96
		Frame 3D-Recess
	)
	Border (
		Position 0 180
		Size 24 17
		Fill 3
		Frame 3D-Recess
	)
	Text "3" (
		Position 9 191
	)

	Text "Modulation Source" (
		Position 45 115
	)
	Gadget "Matrix3_Source" (
		Position 18 119
		Type Cycle (
			Data (
				"NONE"
				"Envelope 1"
				"Envelope 2"
				"Envelope 3"
				"LFO 1"
				"LFO 2"
				"Vibrato"
				"Ramp 1"
				"Ramp 2"
				"Keyboard"
				"Portamento"
				"Tracking Generator"
				"Keyboard Gate"
				"Velocity"
				"Release Velocity"
				"Pressure"
				"Pedal 1"
				"Pedal 2"
				"Lever 1"
				"Lever 2"
				"Lever 3"
			)
		)
		Midi "Patch" (
			Data (
				231 VALUE NybbleLM
			)
			Send
		)
	)
	Text "Modulation Destination" (
		Position 28 144
	)
	Gadget "Matrix3_Destination" (
		Position 9 148
		Type Cycle (
			Data (
				"NONE"
				"DCO 1 Frequency"
				"DCO 1 Pulse Width"
				"DCO 1 Waveshape"
				"DCO 2 Frequency"
				"DCO 2 Pulse Width"
				"DCO 2 Waveshape"
				"Mix Level"
				"VCF FM Amount"
				"VCF Frequency"
				"VCF Resonance"
				"VCA 1 Level"
				"VCA 2 Level"
				"Envelope 1 Delay"
				"Envelope 1 Attack"
				"Envelope 1 Decay"
				"Envelope 1 Release"
				"Envelope 1 Amplitude"
				"Envelope 2 Delay"
				"Envelope 2 Attack"
				"Envelope 2 Decay"
				"Envelope 2 Release"
				"Envelope 2 Amplitude"
				"Envelope 3 Delay"
				"Envelope 3 Attack"
				"Envelope 3 Decay"
				"Envelope 3 Release"
				"Envelope 3 Amplitude"
				"LFO 1 Speed"
				"LFO 1 Amplitude"
				"LFO 2 Speed"
				"LFO 2 Amplitude"
				"Portamento Time"
			)
		)
		Midi "Patch" (
			Data (
				235 VALUE NybbleLM
			)
			Send
		)
	)
	Text "Amount" (
		Position 86 174
	)
	Gadget "Matrix3_Amount" (
		Position 55 178
		Font "Numbers"
		Type Slider (
			Range -63 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace RIGHT
		)
		Midi "Patch" (
			Data (
				233 VALUE Signed NybbleLM
			)
			Send
		)
	)

	Border (
		Position 215 101
		Size 210 96
		Frame 3D-Recess
	)
	Border (
		Position 215 180
		Size 24 17
		Fill 3
		Frame 3D-Recess
	)
	Text "4" (
		Position 224 191
	)

	Text "Modulation Source" (
		Position 260 115
	)
	Gadget "Matrix4_Source" (
		Position 233 119
		Type Cycle (
			Data (
				"NONE"
				"Envelope 1"
				"Envelope 2"
				"Envelope 3"
				"LFO 1"
				"LFO 2"
				"Vibrato"
				"Ramp 1"
				"Ramp 2"
				"Keyboard"
				"Portamento"
				"Tracking Generator"
				"Keyboard Gate"
				"Velocity"
				"Release Velocity"
				"Pressure"
				"Pedal 1"
				"Pedal 2"
				"Lever 1"
				"Lever 2"
				"Lever 3"
			)
		)
		Midi "Patch" (
			Data (
				237 VALUE NybbleLM
			)
			Send
		)
	)
	Text "Modulation Destination" (
		Position 243 144
	)
	Gadget "Matrix4_Destination" (
		Position 224 148
		Type Cycle (
			Data (
				"NONE"
				"DCO 1 Frequency"
				"DCO 1 Pulse Width"
				"DCO 1 Waveshape"
				"DCO 2 Frequency"
				"DCO 2 Pulse Width"
				"DCO 2 Waveshape"
				"Mix Level"
				"VCF FM Amount"
				"VCF Frequency"
				"VCF Resonance"
				"VCA 1 Level"
				"VCA 2 Level"
				"Envelope 1 Delay"
				"Envelope 1 Attack"
				"Envelope 1 Decay"
				"Envelope 1 Release"
				"Envelope 1 Amplitude"
				"Envelope 2 Delay"
				"Envelope 2 Attack"
				"Envelope 2 Decay"
				"Envelope 2 Release"
				"Envelope 2 Amplitude"
				"Envelope 3 Delay"
				"Envelope 3 Attack"
				"Envelope 3 Decay"
				"Envelope 3 Release"
				"Envelope 3 Amplitude"
				"LFO 1 Speed"
				"LFO 1 Amplitude"
				"LFO 2 Speed"
				"LFO 2 Amplitude"
				"Portamento Time"
			)
		)
		Midi "Patch" (
			Data (
				241 VALUE NybbleLM
			)
			Send
		)
	)
	Text "Amount" (
		Position 301 174
	)
	Gadget "Matrix4_Amount" (
		Position 270 178
		Font "Numbers"
		Type Slider (
			Range -63 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace RIGHT
		)
		Midi "Patch" (
			Data (
				239 VALUE Signed NybbleLM
			)
			Send
		)
	)


	Border (
		Position 430 101
		Size 210 96
		Frame 3D-Recess
	)
	Border (
		Position 430 180
		Size 24 17
		Fill 3
		Frame 3D-Recess
	)
	Text "5" (
		Position 439 191
	)

	Text "Modulation Source" (
		Position 475 115
	)
	Gadget "Matrix5_Source" (
		Position 448 119
		Type Cycle (
			Data (
				"NONE"
				"Envelope 1"
				"Envelope 2"
				"Envelope 3"
				"LFO 1"
				"LFO 2"
				"Vibrato"
				"Ramp 1"
				"Ramp 2"
				"Keyboard"
				"Portamento"
				"Tracking Generator"
				"Keyboard Gate"
				"Velocity"
				"Release Velocity"
				"Pressure"
				"Pedal 1"
				"Pedal 2"
				"Lever 1"
				"Lever 2"
				"Lever 3"
			)
		)
		Midi "Patch" (
			Data (
				243 VALUE NybbleLM
			)
			Send
		)
	)
	Text "Modulation Destination" (
		Position 458 144
	)
	Gadget "Matrix5_Destination" (
		Position 439 148
		Type Cycle (
			Data (
				"NONE"
				"DCO 1 Frequency"
				"DCO 1 Pulse Width"
				"DCO 1 Waveshape"
				"DCO 2 Frequency"
				"DCO 2 Pulse Width"
				"DCO 2 Waveshape"
				"Mix Level"
				"VCF FM Amount"
				"VCF Frequency"
				"VCF Resonance"
				"VCA 1 Level"
				"VCA 2 Level"
				"Envelope 1 Delay"
				"Envelope 1 Attack"
				"Envelope 1 Decay"
				"Envelope 1 Release"
				"Envelope 1 Amplitude"
				"Envelope 2 Delay"
				"Envelope 2 Attack"
				"Envelope 2 Decay"
				"Envelope 2 Release"
				"Envelope 2 Amplitude"
				"Envelope 3 Delay"
				"Envelope 3 Attack"
				"Envelope 3 Decay"
				"Envelope 3 Release"
				"Envelope 3 Amplitude"
				"LFO 1 Speed"
				"LFO 1 Amplitude"
				"LFO 2 Speed"
				"LFO 2 Amplitude"
				"Portamento Time"
			)
		)
		Midi "Patch" (
			Data (
				247 VALUE NybbleLM
			)
			Send
		)
	)
	Text "Amount" (
		Position 516 174
	)
	Gadget "Matrix5_Amount" (
		Position 485 178
		Font "Numbers"
		Type Slider (
			Range -63 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace RIGHT
		)
		Midi "Patch" (
			Data (
				245 VALUE Signed NybbleLM
			)
			Send
		)
	)

	Border (
		Position 0 202
		Size 210 96
		Frame 3D-Recess
	)
	Border (
		Position 0 281
		Size 24 17
		Fill 3
		Frame 3D-Recess
	)
	Text "6" (
		Position 9 292
	)

	Text "Modulation Source" (
		Position 45 216
	)
	Gadget "Matrix6_Source" (
		Position 18 220
		Type Cycle (
			Data (
				"NONE"
				"Envelope 1"
				"Envelope 2"
				"Envelope 3"
				"LFO 1"
				"LFO 2"
				"Vibrato"
				"Ramp 1"
				"Ramp 2"
				"Keyboard"
				"Portamento"
				"Tracking Generator"
				"Keyboard Gate"
				"Velocity"
				"Release Velocity"
				"Pressure"
				"Pedal 1"
				"Pedal 2"
				"Lever 1"
				"Lever 2"
				"Lever 3"
			)
		)
		Midi "Patch" (
			Data (
				249 VALUE NybbleLM
			)
			Send
		)
	)
	Text "Modulation Destination" (
		Position 28 245
	)
	Gadget "Matrix6_Destination" (
		Position 9 249
		Type Cycle (
			Data (
				"NONE"
				"DCO 1 Frequency"
				"DCO 1 Pulse Width"
				"DCO 1 Waveshape"
				"DCO 2 Frequency"
				"DCO 2 Pulse Width"
				"DCO 2 Waveshape"
				"Mix Level"
				"VCF FM Amount"
				"VCF Frequency"
				"VCF Resonance"
				"VCA 1 Level"
				"VCA 2 Level"
				"Envelope 1 Delay"
				"Envelope 1 Attack"
				"Envelope 1 Decay"
				"Envelope 1 Release"
				"Envelope 1 Amplitude"
				"Envelope 2 Delay"
				"Envelope 2 Attack"
				"Envelope 2 Decay"
				"Envelope 2 Release"
				"Envelope 2 Amplitude"
				"Envelope 3 Delay"
				"Envelope 3 Attack"
				"Envelope 3 Decay"
				"Envelope 3 Release"
				"Envelope 3 Amplitude"
				"LFO 1 Speed"
				"LFO 1 Amplitude"
				"LFO 2 Speed"
				"LFO 2 Amplitude"
				"Portamento Time"
			)
		)
		Midi "Patch" (
			Data (
				253 VALUE NybbleLM
			)
			Send
		)
	)
	Text "Amount" (
		Position 86 275
	)
	Gadget "Matrix6_Amount" (
		Position 55 279
		Font "Numbers"
		Type Slider (
			Range -63 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace RIGHT
		)
		Midi "Patch" (
			Data (
				251 VALUE Signed NybbleLM
			)
			Send
		)
	)

	Border (
		Position 215 202
		Size 210 96
		Frame 3D-Recess
	)
	Border (
		Position 215 281
		Size 24 17
		Fill 3
		Frame 3D-Recess
	)
	Text "7" (
		Position 224 292
	)

	Text "Modulation Source" (
		Position 260 216
	)
	Gadget "Matrix7_Source" (
		Position 233 220
		Type Cycle (
			Data (
				"NONE"
				"Envelope 1"
				"Envelope 2"
				"Envelope 3"
				"LFO 1"
				"LFO 2"
				"Vibrato"
				"Ramp 1"
				"Ramp 2"
				"Keyboard"
				"Portamento"
				"Tracking Generator"
				"Keyboard Gate"
				"Velocity"
				"Release Velocity"
				"Pressure"
				"Pedal 1"
				"Pedal 2"
				"Lever 1"
				"Lever 2"
				"Lever 3"
			)
		)
		Midi "Patch" (
			Data (
				255 VALUE NybbleLM
			)
			Send
		)
	)
	Text "Modulation Destination" (
		Position 243 245
	)
	Gadget "Matrix7_Destination" (
		Position 224 249
		Type Cycle (
			Data (
				"NONE"
				"DCO 1 Frequency"
				"DCO 1 Pulse Width"
				"DCO 1 Waveshape"
				"DCO 2 Frequency"
				"DCO 2 Pulse Width"
				"DCO 2 Waveshape"
				"Mix Level"
				"VCF FM Amount"
				"VCF Frequency"
				"VCF Resonance"
				"VCA 1 Level"
				"VCA 2 Level"
				"Envelope 1 Delay"
				"Envelope 1 Attack"
				"Envelope 1 Decay"
				"Envelope 1 Release"
				"Envelope 1 Amplitude"
				"Envelope 2 Delay"
				"Envelope 2 Attack"
				"Envelope 2 Decay"
				"Envelope 2 Release"
				"Envelope 2 Amplitude"
				"Envelope 3 Delay"
				"Envelope 3 Attack"
				"Envelope 3 Decay"
				"Envelope 3 Release"
				"Envelope 3 Amplitude"
				"LFO 1 Speed"
				"LFO 1 Amplitude"
				"LFO 2 Speed"
				"LFO 2 Amplitude"
				"Portamento Time"
			)
		)
		Midi "Patch" (
			Data (
				259 VALUE NybbleLM
			)
			Send
		)
	)
	Text "Amount" (
		Position 301 275
	)
	Gadget "Matrix7_Amount" (
		Position 270 279
		Font "Numbers"
		Type Slider (
			Range -63 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace RIGHT
		)
		Midi "Patch" (
			Data (
				257 VALUE Signed NybbleLM
			)
			Send
		)
	)

	Border (
		Position 430 202
		Size 210 96
		Frame 3D-Recess
	)
	Border (
		Position 430 281
		Size 24 17
		Fill 3
		Frame 3D-Recess
	)
	Text "8" (
		Position 439 292
	)

	Text "Modulation Source" (
		Position 475 216
	)
	Gadget "Matrix8_Source" (
		Position 448 220
		Type Cycle (
			Data (
				"NONE"
				"Envelope 1"
				"Envelope 2"
				"Envelope 3"
				"LFO 1"
				"LFO 2"
				"Vibrato"
				"Ramp 1"
				"Ramp 2"
				"Keyboard"
				"Portamento"
				"Tracking Generator"
				"Keyboard Gate"
				"Velocity"
				"Release Velocity"
				"Pressure"
				"Pedal 1"
				"Pedal 2"
				"Lever 1"
				"Lever 2"
				"Lever 3"
			)
		)
		Midi "Patch" (
			Data (
				261 VALUE NybbleLM
			)
			Send
		)
	)
	Text "Modulation Destination" (
		Position 458 245
	)
	Gadget "Matrix8_Destination" (
		Position 439 249
		Type Cycle (
			Data (
				"NONE"
				"DCO 1 Frequency"
				"DCO 1 Pulse Width"
				"DCO 1 Waveshape"
				"DCO 2 Frequency"
				"DCO 2 Pulse Width"
				"DCO 2 Waveshape"
				"Mix Level"
				"VCF FM Amount"
				"VCF Frequency"
				"VCF Resonance"
				"VCA 1 Level"
				"VCA 2 Level"
				"Envelope 1 Delay"
				"Envelope 1 Attack"
				"Envelope 1 Decay"
				"Envelope 1 Release"
				"Envelope 1 Amplitude"
				"Envelope 2 Delay"
				"Envelope 2 Attack"
				"Envelope 2 Decay"
				"Envelope 2 Release"
				"Envelope 2 Amplitude"
				"Envelope 3 Delay"
				"Envelope 3 Attack"
				"Envelope 3 Decay"
				"Envelope 3 Release"
				"Envelope 3 Amplitude"
				"LFO 1 Speed"
				"LFO 1 Amplitude"
				"LFO 2 Speed"
				"LFO 2 Amplitude"
				"Portamento Time"
			)
		)
		Midi "Patch" (
			Data (
				265 VALUE NybbleLM
			)
			Send
		)
	)
	Text "Amount" (
		Position 516 275
	)
	Gadget "Matrix8_Amount" (
		Position 485 279
		Font "Numbers"
		Type Slider (
			Range -63 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace RIGHT
		)
		Midi "Patch" (
			Data (
				263 VALUE Signed NybbleLM
			)
			Send
		)
	)

	Border (
		Position 0 303
		Size 640 39
		Frame 3D-Recess
	)
	Border (
		Position 0 325
		Size 24 17
		Fill 3
		Frame 3D-Recess
	)
	Text "9" (
		Position 9 336
	)

	Text "Modulation Source" (
		Position 70 317
	)
	Gadget "Matrix9_Source" (
		Position 43 321
		Type Cycle (
			Data (
				"NONE"
				"Envelope 1"
				"Envelope 2"
				"Envelope 3"
				"LFO 1"
				"LFO 2"
				"Vibrato"
				"Ramp 1"
				"Ramp 2"
				"Keyboard"
				"Portamento"
				"Tracking Generator"
				"Keyboard Gate"
				"Velocity"
				"Release Velocity"
				"Pressure"
				"Pedal 1"
				"Pedal 2"
				"Lever 1"
				"Lever 2"
				"Lever 3"
			)
		)
		Midi "Patch" (
			Data (
				267 VALUE NybbleLM
			)
			Send
		)
	)
	Text "Modulation Destination" (
		Position 274 317
	)
	Gadget "Matrix9_Destination" (
		Position 255 321
		Type Cycle (
			Data (
				"NONE"
				"DCO 1 Frequency"
				"DCO 1 Pulse Width"
				"DCO 1 Waveshape"
				"DCO 2 Frequency"
				"DCO 2 Pulse Width"
				"DCO 2 Waveshape"
				"Mix Level"
				"VCF FM Amount"
				"VCF Frequency"
				"VCF Resonance"
				"VCA 1 Level"
				"VCA 2 Level"
				"Envelope 1 Delay"
				"Envelope 1 Attack"
				"Envelope 1 Decay"
				"Envelope 1 Release"
				"Envelope 1 Amplitude"
				"Envelope 2 Delay"
				"Envelope 2 Attack"
				"Envelope 2 Decay"
				"Envelope 2 Release"
				"Envelope 2 Amplitude"
				"Envelope 3 Delay"
				"Envelope 3 Attack"
				"Envelope 3 Decay"
				"Envelope 3 Release"
				"Envelope 3 Amplitude"
				"LFO 1 Speed"
				"LFO 1 Amplitude"
				"LFO 2 Speed"
				"LFO 2 Amplitude"
				"Portamento Time"
			)
		)
		Midi "Patch" (
			Data (
				271 VALUE NybbleLM
			)
			Send
		)
	)
	Text "Amount" (
		Position 516 318
	)
	Gadget "Matrix9_Amount" (
		Position 485 322
		Font "Numbers"
		Type Slider (
			Range -63 63
			Size 100 12
			Direction HORIZONTAL
			LevelPlace RIGHT
		)
		Midi "Patch" (
			Data (
				269 VALUE Signed NybbleLM
			)
			Send
		)
	)
)
