/* X file system entry
 *
 * This mount file enables reading of disks via fd.device and
 * XFSD handler, which should be in DEVS: and L: respectively
 * before the first MOUNT command is issued, e.g.
 * mount FD0: from DEVS:mountlist.fd   (or FD1:, FD2:, FD3:)
 */

FD0:
FileSystem     = L:xfsd
Device         = fd.device
Unit           = 0
Flags          = 0
Surfaces       = 2
BlocksPerTrack = 11
Reserved       = 0
Interleave     = 0
LowCyl         = 0
HighCyl        = 79
Buffers        = 15
BufMemType     = 1
StackSize      = 10000
Priority       = 8
GlobVec        = -1
DosType        = 0x444F5300 /* 'DOS\x00' */

FD1:
FileSystem     = L:xfsd
Device         = fd.device
Unit           = 1
Flags          = 0
Surfaces       = 2
BlocksPerTrack = 11
Reserved       = 0
Interleave     = 0
LowCyl         = 0
HighCyl        = 79
Buffers        = 15
BufMemType     = 1
StackSize      = 10000
Priority       = 8
GlobVec        = -1
DosType        = 0x444F5300 /* 'DOS\x00' */

FD2:
FileSystem     = L:xfsd
Device         = fd.device
Unit           = 2
Flags          = 0
Surfaces       = 2
BlocksPerTrack = 11
Reserved       = 0
Interleave     = 0
LowCyl         = 0
HighCyl        = 79
Buffers        = 15
BufMemType     = 1
StackSize      = 10000
Priority       = 8
GlobVec        = -1
DosType        = 0x444F5300 /* 'DOS\x00' */

FD3:
FileSystem     = L:xfsd
Device         = fd.device
Unit           = 3
Flags          = 0
Surfaces       = 2
BlocksPerTrack = 11
Reserved       = 0
Interleave     = 0
LowCyl         = 0
HighCyl        = 79
Buffers        = 15
BufMemType     = 1
StackSize      = 10000
Priority       = 8
GlobVec        = -1
DosType        = 0x444F5300 /* 'DOS\x00' */

