                  Printer definition file for WSSINDEX

All lines of this file are comments until a line beginning ----.  After that,
alternate lines are comments and parameters.  Printer control sequences and
other items (except for the printer name and label id string) are decimal
numbers, separated by commas or spaces.  The codes in this file are for a DEC
LA50 or LA100 dot matrix printer.

Codes used in this file:

  10 = line feed
  12 = form feed
  13 - carriage return
  27 91 52 119    = \e [ \4 w    = 16.5 character per inch
  27 91 50 122    = \e [ \2 z    = 8 lines per inch
  27 91 56 56 116 = \e [ \8 \8 t = 88 lines per page
  27 91 48 34 122 = \e [ \0 " z  = normal print density

Based on contributions from David P. Maroun and Uwe Christmann.
------------------------------------------------------------
Printer name
DEC LA printers
Optional string printed on all labels

Printer initialization command for 1,2,... column printing
13 27 91 52 119 27 91 50 122 27 91 56 56 116 27 91 48 34 122
Printer initialization command for labels, 20 max (pitch, line spacing, etc.)
13 27 91 52 119 27 91 50 122 27 91 56 56 116 27 91 48 34 122
Printer initialization command for disk covers, 20 max
13 27 91 52 119 27 91 50 122 27 91 56 56 116 27 91 48 34 122
Printer deinitialization command, 10 max (form feed for laser printer, etc.)
12
Number of spaces in left margin for labels
3
Number of columns for labels
2
Width of labels (characters)
29
Number of characters between labels (if multiple columns)
42
Length of label in lines (including unusable lines)
7
Number of usable lines for label
7
Number of spaces in left margin for disk covers
0
Width of paper for disk covers (characters)
89
Length of page in lines for disk covers
36
Printer command to position for the next disk cover
13 10 10 10 10
Character to use for sides of disk cover box (32 = blank prints faster)
32
Character to use for top and bottom lines
32
Character to use for top left corner
32
Character to use for top right corner
32
Character to use for bottom left corner
32
Character to use for bottom right corner
32
End of printer configuration file
