       Printer definition file for WSSINDEX custom print utility

All lines of this file are comments until a line beginning ----.  After that,
alternate lines are comments and parameters.  See the CUSTPRNT documentation
for a description of the format allowed here.  To make it easier for people
to read the printer sequences, I have used blanks to separate characters,
and commas to separate multi-character printer commands.  Most of these
delimiters are not required by the routine which reads this file.

Generated from a donated copy of a printer manual, but not tested.

Commands used in this file:

  \e : = 12 characters per inch
  \e \0 = 8 lines per inch
  0xf = 17.1 characters per inch
  \e S 0 = superscript mode
  \e \3 18 = 18/216 inch line feed (12 lines per inch)
  0x18 = 10 characters per inch
------------------------------------------------------------
Printer name
Okidata Microline 192 with IBM ROM chip (untested)
Optional string printed on all labels
Property of <your name here>
Printer initialization command for 1,2,... column printing, 50 max
\e :, \e \0
Printer initialization command for labels, 50 max (pitch, line spacing, etc.)
0xf, \e S 0, \e \3 18
Printer initialization command for disk covers, 50 max
\e 0, 0xf
Printer deinitialization command, 10 max (form feed for laser printer, etc.)
0x18
Number of spaces in left margin for labels
5
Number of columns for labels
1
Width of labels (characters)
50
Number of characters between labels (if multiple columns)
5
Length of label in lines (including unusable lines)
12
Number of usable lines for label
9
Number of spaces in left margin for disk covers
0
Width of paper for disk covers (characters)
90
Length of page in lines for disk covers
40
Printer command to position for the next disk cover
10 10 10 10
Character to use for sides of disk cover box (32 = blank prints faster)
245
Character to use for top and bottom lines
241
Character to use for top left corner
240
Character to use for top right corner
242
Character to use for bottom left corner
246
Character to use for bottom right corner
247
End of printer configuration file
