                  Printer definition file for WSSINDEX

All lines of this file are comments until a line beginning ----.  After that,
alternate lines are comments and parameters.  See the WSSINDEX documentation
for a description of the format allowed here.  The codes in this file are for
a Tandy DMP-105 dot matrix printer.

Codes used in this file:

  10 = line feed
  13 = carriage return
  27 21   = \e 21  = suppresses the automatic line feed when a carriage
                     return is received
  27 20   = \e 20  = selects condensed type
  27 91 8 = \e [ 8 = selects a line feed of 8/72 inches

Contributed by David P. Maroun
------------------------------------------------------------
Printer name
Tandy DMP-105
Optional string printed on all labels

Printer initialization command for 1,2,... column printing
13 27 21 27 20 27 91 8
Printer initialization command for labels, 20 max (pitch, line spacing, etc.)
13 27 21 27 20 27 91 8
Printer initialization command for disk covers, 20 max
13 27 21 27 20 27 91 8
Printer deinitialization command, 10 max (form feed for laser printer, etc.)
13 10
Number of spaces in left margin for labels
3
Number of columns for labels
2
Width of labels (characters)
29
Number of characters between labels (if multiple columns)
42
Length of label in lines (including unusable lines)
8
Number of usable lines for label
8
Number of spaces in left margin for disk covers
0
Width of paper for disk covers (characters)
89
Length of page in lines for disk covers
39
Printer command to position for the next disk cover
13 10 10 10 10
Character to use for sides of disk cover box (32 = blank prints faster)
245
Character to use for top and bottom lines
241
Character to use for top left corner
240
Character to use for top right corner
242
Character to use for bottom left corner
246
Character to use for bottom right corner
247
End of printer configuration file
