       Printer definition file for WSSINDEX custom print utility

All lines of this file are comments until a line beginning ----.  After that,
alternate lines are comments and parameters.  See the CUSTPRNT documentation
for a description of the format allowed here.

Contributed by Alan G. Haddon, typed in by RWB.  No manual pages were included
with the contributed file, so I have made reasonable guesses as to the
meanings of the commands used here.

Commands used in this file:

  27 65 6 = \e A 6 = 6/72 inch line feed (12 lines per inch)
  27 94 = \e ^ = superscript mode (????)
  15 = compressed print
  27 65 9 = \e A 9 = 9/72 inch line feed (8 lines per inch)
  27 64 = \e @ = reset
------------------------------------------------------------
Printer name
TI 855
Optional string printed on all labels
Property of <your name here>
Printer initialization command for 1,2,... column printing, 50 max

Printer initialization command for labels, 50 max (pitch, line spacing, etc.)
27 65 6 27 94 15
Printer initialization command for disk covers, 50 max
27 65 9 15
Printer deinitialization command, 10 max (form feed for laser printer, etc.)
27,64
Number of spaces in left margin for labels
5
Number of columns for labels
1
Width of labels (characters)
50
Number of characters between labels (if multiple columns)
5
Length of label in lines (including unusable lines)
12
Number of usable lines for label
9
Number of spaces in left margin for disk covers
0
Width of paper for disk covers (characters)
90
Length of page in lines for disk covers
40
Printer command to position for the next disk cover
10 10 10 10
Character to use for sides of disk cover box (32 = blank prints faster)
181
Character to use for top and bottom lines
163
Character to use for top left corner
183
Character to use for top right corner
181
Character to use for bottom left corner
163
Character to use for bottom right corner
161
End of printer configuration file
